OBJECTID|FieldID|LocationConfidenceMeters|ObservedMapUnit|MapUnit|Symbol|Label|PlotAtScale|Notes|LocationMethod|created_user|created_date|last_edited_user|last_edited_date|DataSourceID|WellsPoints_ID|LatitudeDecimalDegrees|LongitudeDecimalDegrees|CountyName|StateName|WellName|QuadrangleName|DateDrilled|Type|CoreDiameterInches|CoreCondition|BoxType|Reference1URL|Reference2URL|Reference3URL|URLNWIS|Feature1|Feature1DepthBelowGroundSurfaceFeet|Feature2|Feature2DepthBelowGroundSurfaceFeet|Feature3|Feature3DepthBelowGroundSurfaceFeet|Feature4|Feature4DepthBelowGroundSurfaceFeet|Feature5|Feature5DepthBelowGroundSurfaceFeet|Feature6|Feature6DepthBelowGroundSurfaceFeet|Feature7|Feature7DepthBelowGroundSurfaceFeet|Feature8|Feature8DepthBelowGroundSurfaceFeet|Feature9|Feature9DepthBelowGroundSurfaceFeet|Feature10|Feature10DepthBelowGroundSurfaceFeet|Feature11|Feature11DepthBelowGroundSurfaceFeet|Feature12|Feature12DepthBelowGroundSurfaceFeet|Feature13|Feature13DepthBelowGroundSurfaceFeet|Feature14|Feature14DepthBelowGroundSurfaceFeet|Feature15|Feature15DepthBelowGroundSurfaceFeet|Feature16|Feature16DepthBelowGroundSurfaceFeet|Feature17|Feature17DepthBelowGroundSurfaceFeet|BoreholeDepthLoggedFeet|LandSurfaceElevationFeetAboveSeaLevel
|903|AA Ac 23|25.0|||RSY12|AA Ac 23|0.0| 36 envelopes in 2 box(es); spanning depths of 0 to 335 feet; continuous coverage; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0001|39.20066318|-76.67635758|Anne Arundel|Maryland|AA Ac 23|Relay||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=391202076403601&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
904|AA Ad 33|25.0|||RSY12|AA Ad 33|0.0| 22 envelopes in 1 box(es); spanning depths of 0 to 147 feet; 2 sets (washed, unwashed); continuous coverage in 10 ft intervals 0-80 ft; variable intervals 80-147 ft .||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0002|39.21205225|-76.60635497|Anne Arundel|Maryland|AA Ad 33|Curtis Bay||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=391243076362401&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
905|AA Ad 69|25.0|||RSY12|AA Ad 69|0.0| 9 envelopes in 1 box(es); spanning depths of 0 to 135 feet; continuous coverage; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0003|39.16983059|-76.61746621|Anne Arundel|Maryland|AA Ad 69|Curtis Bay||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=391011076370401&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
906|AA Ad 89|25.0|||RSY12|AA Ad 89|0.0| 18 envelopes in 1 box(es); spanning depths of 0 to 336 feet; continuous coverage; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0004|39.17566368|-76.64941189|Anne Arundel|Maryland|AA Ad 89|Relay||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=391032076385901&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
907|AA Ad 90|25.0|||RSY12|AA Ad 90|0.0| 33 envelopes in 2 box(es); spanning depths of 2 to 474 feet; continuous coverage; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0005|39.176|-76.64922222|Anne Arundel|Maryland|AA Ad 90|Relay||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=391032076385902&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
908|AA Ad 93|25.0|||RSY12|AA Ad 93|0.0| 26 envelopes in 1 box(es); spanning depths of 0 to 260 feet; continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0006|39.20455247|-76.58468741|Anne Arundel|Maryland|AA Ad 93|Curtis Bay||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=391216076350601&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
909|AA Ae 35|25.0|||RSY12|AA Ae 35|0.0| 20 envelopes in 2 box(es); spanning depths of 85.9 to 567 feet; coverage from 85.9 to 235.5 ft and 485 to 567 ft; sampling intervals vary;.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0007|39.19649714|-76.56357544|Anne Arundel|Maryland|AA Ae 35|Curtis Bay||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=391147076335001&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
910|AA Bb 5|25.0|||RSY12|AA Bb 5|0.0| 16 envelopes in 1 box(es); spanning depths of 0 to 199 feet; continuous coverage.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0008|39.10121975|-76.78469338|Anne Arundel|Maryland|AA Bb 5|Laurel||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=390604076470601&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
911|AA Bb 24|25.0|||RSY12|AA Bb 24|0.0| 27 envelopes in 1 box(es); spanning depths of 0 to 180 feet; 2 sets (washed, unwashed); continuous coverage; sampling intervals vary .||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0009|39.14788579|-76.75330426|Anne Arundel|Maryland|AA Bb 24|Savage||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=390852076451301&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
912|AA Bb 26|25.0|||RSY12|AA Bb 26|0.0| 10 envelopes in 1 box(es); spanning depths of 7 to 188 feet; continuous coverage; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0010|39.12899719|-76.75052617|Anne Arundel|Maryland|AA Bb 26|Savage||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=390744076450301&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
913|AA Bb 33|25.0|||RSY12|AA Bb 33|0.0| 15 envelopes in 1 box(es); spanning depths of 0 to 193 feet; continuous coverage; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0011|39.09288648|-76.81608301|Anne Arundel|Maryland|AA Bb 33|Laurel||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=390534076485901&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
914|AA Bb 50|25.0|||RSY12|AA Bb 50|0.0| 16 envelopes in 1 box(es); spanning depths of 0 to 160 feet; continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0012|39.115664|-76.77413772|Anne Arundel|Maryland|AA Bb 50|Laurel||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=390656076462801&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
915|AA Bb 66|25.0|||RSY12|AA Bb 66|0.0| 15 envelopes in 1 box(es); spanning depths of 0 to 137 feet; continuous coverage; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0013|39.09205315|-76.82024978|Anne Arundel|Maryland|AA Bb 66|Laurel||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=390531076491401&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
916|AA Bb 67|25.0|||RSY12|AA Bb 67|0.0| 106 envelopes in 6 box(es); spanning depths of 0 to 514.2 feet; 2 sets; continuous converage, 0-482 ft and 0-514.2 ft; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0014|39.09463889|-76.75730556|Anne Arundel|Maryland|AA Bb 67|Laurel||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=390538076453001&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
917|AA Bb 67|25.0|||RSY12|AA Bb 67|0.0| 60 envelopes in 4 box(es); spanning depths of 0 to 604.33 feet; Continuous coverage in 10 ft intervals 0-361 ft and variable intervals 361-604.33 ft.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0015|39.09463889|-76.75730556|Anne Arundel|Maryland|AA Bb 67|Laurel||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=390538076453001&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
918|AA Bc 44|25.0|||RSY12|AA Bc 44|0.0| 24 envelopes in 1 box(es); spanning depths of 0 to 163 feet; 2 sets (washed and unwashed); continuous coverage; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0016|39.15788594|-76.69330223|Anne Arundel|Maryland|AA Bc 44|Relay||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=390928076413701&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
919|AA Bc 159|25.0|||RSY12|AA Bc 159|0.0| 37 envelopes in 2 box(es); spanning depths of 0 to 435.1 feet; continuous coverage; in 20 ft intervals 0-40 ft; variable intervals 40-435.1 ft.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0017|39.09038692|-76.69469046|Anne Arundel|Maryland|AA Bc 159|Odenton||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=390525076414201&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
920|AA Bc 160|25.0|||RSY12|AA Bc 160|0.0| 44 envelopes in 2 box(es); spanning depths of 0 to 700.6 feet; continuous coverage; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0018|39.10260902|-76.68385688|Anne Arundel|Maryland|AA Bc 160|Odenton||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=390609076410301&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
921|AA Bc 211|25.0|||RSY12|AA Bc 211|0.0| 43 envelopes in 3 box(es); spanning depths of 0 to 325 feet; continuous coverage in 10 ft intervals 0-220 ft and 5 ft intervals 220-325 ft.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0019|39.160386|-76.67330152|Anne Arundel|Maryland|AA Bc 211|Relay||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=390937076402501&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
922|AA Bc 233|25.0|||RSY12|AA Bc 233|0.0| 43 envelopes in 3 box(es); spanning depths of 0 to 330 feet; continuous coverage in 10 ft intervals 0-220 ft and 5 ft intervals 220-3305 ft.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0020|39.11733099|-76.69052393|Anne Arundel|Maryland|AA Bc 233|Odenton||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=390702076412701&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
923|AA Bc P1344|25.0|||RSY12|AA Bc P1344|0.0| 20 envelopes in 1 box(es); spanning depths of 0 to 195 feet; continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:43:21|DAS02|WP0021|39.08581111|-76.70168056|Anne Arundel|Maryland|AA Bc P1344|Odenton||cuttings|||||||||||||||||||||||||||||||||||||||||||
924|AA Bd 23|25.0|||RSY12|AA Bd 23|0.0| 103 envelopes in 3 box(es); spanning depths of 2 to 617 feet; 2 sets:  1 set continuous coverage; 1 set missing missing 496 to 522 ft interval.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0022|39.14538656|-76.60663231|Anne Arundel|Maryland|AA Bd 23|Curtis Bay||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=390843076362501&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
925|AA Be 47|25.0|||RSY12|AA Be 47|0.0| 3 envelopes in 1 box(es); spanning depths of 147 to 170 feet; select intervals only: 147ft, 148ft and 170ft.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0023|39.15649788|-76.53357416|Anne Arundel|Maryland|AA Be 47|Curtis Bay||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=390923076320201&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
926|AA Be 48|25.0|||RSY12|AA Be 48|0.0| 16 envelopes in 1 box(es); spanning depths of 69 to 254 feet; missing intervals 140-182 ft and 195-200 ft.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0024|39.15649788|-76.53357416|Anne Arundel|Maryland|AA Be 48|Curtis Bay||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=390923076320202&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
927|AA Cb 1|25.0|||RSY12|AA Cb 1|0.0| 52 envelopes in 2 box(es); spanning depths of 0 to 510 feet; missing intervals 335-340 ft and 349-351 ft.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0025|39.05011111|-76.77575|Anne Arundel|Maryland|AA Cb 1|Laurel||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=390303076463201&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
928|AA Cb 2|25.0|||RSY12|AA Cb 2|0.0| 18 envelopes in 1 box(es); spanning depths of 0 to 177 feet; missing 173-177 ft for pollen-spore analysis, 3/31/1966, H.J. Hansen..||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0026|39.04622062|-76.74996952|Anne Arundel|Maryland|AA Cb 2|Odenton||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=390246076450101&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
929|AA Cb 3|25.0|||RSY12|AA Cb 3|0.0| 62 envelopes in 2 box(es); spanning depths of 0 to 605 feet; continuous coverage in 5ft and 10 ft intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0027|39.07038682|-76.82080512|Anne Arundel|Maryland|AA Cb 3|Laurel||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=390413076491601&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
930|AA Cc 6|25.0|||RSY12|AA Cc 6|0.0| 34 envelopes in 1 box(es); spanning depths of 0 to 171 feet; 2 sets (washed and unwashed); continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0028|39.04122111|-76.66802243|Anne Arundel|Maryland|AA Cc 6|Odenton||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=390228076400601&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
931|AA Cc 23|25.0|||RSY12|AA Cc 23|0.0| 56 envelopes in 2 box(es); spanning depths of 10 to 290 feet; 2 sets; continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0029|39.07038728|-76.68107869|Anne Arundel|Maryland|AA Cc 23|Odenton||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=390413076405301&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
932|AA Cc 85|25.0|||RSY12|AA Cc 85|0.0| 147 envelopes in 5 box(es); spanning depths of 0 to 1069 feet; missing 252-296 ft, 480-495 ft, 946-952 ft, 972-978ft, 1037-1044 ft.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0030|39.00288817|-76.69885633|Anne Arundel|Maryland|AA Cc 85|Odenton||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=390010076415701&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
933|AA Cc 86|25.0|||RSY12|AA Cc 86|0.0| 48 envelopes in 2 box(es); spanning depths of 142 to 1040 feet; continuous coverage; sampling interval vary; core sample at 280 ft.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0031|39.00288817|-76.69885633|Anne Arundel|Maryland|AA Cc 86|Odenton||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_21.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=390010076415702&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
934|AA Cc 101|25.0|||RSY12|AA Cc 101|0.0| 81 envelopes in 5 box(es); spanning depths of 0 to 1017 feet; some intervals missing.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0032|39.01399922|-76.67913363|Anne Arundel|Maryland|AA Cc 101|Odenton||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=390050076404601&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
935|AA Cc 104|25.0|||RSY12|AA Cc 104|0.0| 45 envelopes in 2 box(es); spanning depths of 20 to 1264 feet; some intervals missing.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0033|39.01788808|-76.67413351|Anne Arundel|Maryland|AA Cc 104|Odenton||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=390104076402801&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
936|AA Cc 107|25.0|||RSY12|AA Cc 107|0.0| 58 envelopes in 4 box(es); spanning depths of 36 to 1281 feet; continuous coverage; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0034|39.0131659|-76.67996698|Anne Arundel|Maryland|AA Cc 107|Odenton||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_21.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=390047076404901&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
937|AA Cc 113|25.0|||RSY12|AA Cc 113|0.0| 103 envelopes in 5 box(es); spanning depths of 0 to 1003 feet; continuous coverage.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0035|39.04900833|-76.69180556|Anne Arundel|Maryland|AA Cc 113|Odenton||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=390256076413101&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
938|AA Cc 114|25.0|||RSY12|AA Cc 114|0.0| 113 envelopes in 5 box(es); spanning depths of 0 to 1025 feet; nearly continuous coverage in 10 ft intervals; missing 1017-1020 ft interval.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0036|39.0484431|-76.69135658|Anne Arundel|Maryland|AA Cc 114|Odenton||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=390254076413001&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
939|AA Cc 118|25.0|||RSY12|AA Cc 118|0.0| 68 envelopes in 4 box(es); spanning depths of 0 to 680 feet; continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0037|39.07705364|-76.7227468|Anne Arundel|Maryland|AA Cc 118|Odenton||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=390437076432301&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
940|AA Cc 119|25.0|||RSY12|AA Cc 119|0.0| 69 envelopes in 4 box(es); spanning depths of 0 to 687 feet; continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0038|39.07766667|-76.72336111|Anne Arundel|Maryland|AA Cc 119|Odenton||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=390437076432302&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
941|AA Cd 5|25.0|||RSY12|AA Cd 5|0.0| 57 envelopes in 2 box(es); spanning depths of 0 to 142 feet; nearly continuous coverage in 5 ft intervals; missing 100-105 ft interval.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0039|39.08316535|-76.5871868|Anne Arundel|Maryland|AA Cd 5|Round Bay||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=390459076351501&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
942|AA Cd 53|25.0|||RSY12|AA Cd 53|0.0| 20 envelopes in 1 box(es); spanning depths of 0 to 200 feet; nearly continuous coverage in 10 ft intervals; missing 150-160 ft interval.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0040|39.00677757|-76.58885307|Anne Arundel|Maryland|AA Cd 53|Round Bay||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=390024076352101&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
943|AA Cd 72|25.0|||RSY12|AA Cd 72|0.0| 28 envelopes in 2 box(es); spanning depths of 0 to 296 feet; missing 176-186 ft, 206-216 ft.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0041|39.0203884|-76.60413139|Anne Arundel|Maryland|AA Cd 72|Round Bay||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=390113076361601&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
944|AA Cd 83|25.0|||RSY12|AA Cd 83|0.0| 17 envelopes in 1 box(es); spanning depths of 2 to 106 feet; continuous coverage; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0042|39.01955502|-76.6160762|Anne Arundel|Maryland|AA Cd 83|Round Bay||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=390110076365901&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
945|AA Ce 6|25.0|||RSY12|AA Ce 6|0.0| 40 envelopes in 2 box(es); spanning depths of 0 to 170 feet; continuous coverage; mostly 10 ft intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0043|39.04788822|-76.5599635|Anne Arundel|Maryland|AA Ce 6|Round Bay||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=390252076333701&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
946|AA Ce 80|25.0|||RSY12|AA Ce 80|0.0| 86 envelopes in 3 box(es); spanning depths of 0 to 602 feet; 2 sets; some intervals missing; samplying intervals vary.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0044|39.08066544|-76.5760753|Anne Arundel|Maryland|AA Ce 80|Round Bay||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=390450076343501&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
947|AA Ce 116|25.0|||RSY12|AA Ce 116|0.0| 30 envelopes in 1 box(es); spanning depths of 0 to 348 feet; missing 33-40 ft, 45-62 ft, 71-74 ft, 273-292 ft.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0045|39.05483252|-76.56996386|Anne Arundel|Maryland|AA Ce 116|Round Bay||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=390317076341301&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
948|AA Ce 120|25.0|||RSY12|AA Ce 120|0.0| 53 envelopes in 4 box(es); spanning depths of 800 to 1340 feet; continuous coverage in 10 ftintervals to 1260 ft then missing1260-1270 ft, 1280-1290 ft.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0046|39.05088889|-76.57844444|Anne Arundel|Maryland|AA Ce 120|Round Bay||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=390303076344301&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
949|AA Cf 100|25.0|||RSY12|AA Cf 100|0.0| 82 envelopes in 4 box(es); spanning depths of 0 to 410 feet; missing 150-160 ft and385-390 ft.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0047|39.03066661|-76.47468304|Anne Arundel|Maryland|AA Cf 100|Gibson Island||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_21.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=390150076283001&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
950|AA Cf 101|25.0|||RSY12|AA Cf 101|0.0| 59 envelopes in 3 box(es); spanning depths of 5 to 377 feet; missing intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0048|39.03066662|-76.47384968|Anne Arundel|Maryland|AA Cf 101|Gibson Island||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=390150076282701&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
951|AA Cg 18|25.0|||RSY12|AA Cg 18|0.0| 49 envelopes in 2 box(es); spanning depths of 0 to 499 feet; missing 238-240 ft, 474-479 ft.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0049|39.00788929|-76.40968109|Anne Arundel|Maryland|AA Cg 18|Gibson Island||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=390028076243601&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
952|AA Dc 7|25.0|||RSY12|AA Dc 7|0.0| 13 envelopes in 1 box(es); spanning depths of 0 to 160 feet; missing 50-60 ft, 70-110 ft.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0050|38.96677791|-76.68413335|Anne Arundel|Maryland|AA Dc 7|Bowie||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385800076410401&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
953|AA Dc 13|25.0|||RSY12|AA Dc 13|0.0| 31 envelopes in 1 box(es); spanning depths of 0 to 270 feet; continuous coverage; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0051|38.96677791|-76.68385556|Anne Arundel|Maryland|AA Dc 13|Bowie||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_21.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385800076410301&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
954|AA Dd 36|25.0|||RSY12|AA Dd 36|0.0| 18 envelopes in 1 box(es); spanning depths of 0 to 338 feet; continuous coverage; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0052|38.91816817|-76.63885341|Anne Arundel|Maryland|AA Dd 36|Bowie||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385505076382101&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
955|AA Dd 41|25.0|||RSY12|AA Dd 41|0.0| 33 envelopes in 2 box(es); spanning depths of 70 to 480 feet; missing intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0053|38.96900041|-76.62607589|Anne Arundel|Maryland|AA Dd 41|Bowie||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_21.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385808076373501&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
956|AA De 44|25.0|||RSY12|AA De 44|0.0| 86 envelopes in 3 box(es); spanning depths of 5 to 792 feet; missing intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0054|38.98705586|-76.56857437|Anne Arundel|Maryland|AA De 44|South River||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385913076340802&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
957|AA De 91|25.0|||RSY12|AA De 91|0.0| 11 envelopes in 1 box(es); spanning depths of 3 to 229 feet; continuous coverage; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0055|38.98177838|-76.53773995|Anne Arundel|Maryland|AA De 91|South River||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385854076321702&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
958|AA De 93|25.0|||RSY12|AA De 93|0.0| 46 envelopes in 2 box(es); spanning depths of 0 to 470 feet; nearly continuous coverage in 10 ft intervals; missing 380-385 ft.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0056|38.99594466|-76.54496274|Anne Arundel|Maryland|AA De 93|South River||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385945076324301&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
959|AA De 95|25.0|||RSY12|AA De 95|0.0| 35 envelopes in 2 box(es); spanning depths of 5 to 511 feet; continuous coverage; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0057|38.98172222|-76.55777778|Anne Arundel|Maryland|AA De 95|South River||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385853076333001&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
960|AA De 97|25.0|||RSY12|AA De 97|0.0| 36 envelopes in 2 box(es); spanning depths of 0 to 563 feet; missing 203-211 ft, 241-244 ft.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0058|38.98150049|-76.55996287|Anne Arundel|Maryland|AA De 97|South River||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385853076333701&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
961|AA De 100|25.0|||RSY12|AA De 100|0.0| 104 envelopes in 3 box(es); spanning depths of 0 to 436 feet; missing intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0059|38.95566809|-76.50746049|Anne Arundel|Maryland|AA De 100|South River||cuttings||||http://www.mgs.md.gov/output/reports/RI/RI_22.pdf|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385720076302801&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
962|AA De 101|25.0|||RSY12|AA De 101|0.0| 214 envelopes in 12 box(es); spanning depths of 0 to 534 feet; 2 sets; nearly continuous coverage in 5 ft intervals; 1 set missing 391-394 ft interval.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0060|38.92011312|-76.55412796|Anne Arundel|Maryland|AA De 101|South River||cuttings||||http://ww.mgs.md.gov/publications/report_pages/BDR_21.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385512076331601&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
963|AA De 101|25.0|||RSY12|AA De 101|0.0| 194 envelopes in 9 box(es); spanning depths of 0 to 534 feet; 2 sets; missing intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0061|38.92011312|-76.55412796|Anne Arundel|Maryland|AA De 101|South River||cuttings||||http://ww.mgs.md.gov/publications/report_pages/BDR_21.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385512076331601&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
964|AA De 104|25.0|||RSY12|AA De 104|0.0| 86 envelopes in 4 box(es); spanning depths of 5 to 468 feet; missing intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0062|38.91955759|-76.55357237|Anne Arundel|Maryland|AA De 104|South River||cuttings||||http://www.mgs.md.gov/publications/report_pages/OFR_12-02-20.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385510076331401&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
965|AA De 106|25.0|||RSY12|AA De 106|0.0| 57 envelopes in 3 box(es); spanning depths of 0 to 285 feet; nearly continuous coverage.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0063|38.95566809|-76.50746049|Anne Arundel|Maryland|AA De 106|South River||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385720076302803&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
966|AA De 113|25.0|||RSY12|AA De 113|0.0| 31 envelopes in 2 box(es); spanning depths of 0 to 351 feet; missing intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0064|38.99150031|-76.54662935|Anne Arundel|Maryland|AA De 113|South River||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_21.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385929076324901&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
967|AA De 124|25.0|||RSY12|AA De 124|0.0| 33 envelopes in 2 box(es); spanning depths of 0 to 1100 feet; missing 500-940 ft.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0065|38.92455556|-76.56219444|Anne Arundel|Maryland|AA De 124|South River||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_46.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385528076334601&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
968|AA De 125|25.0|||RSY12|AA De 125|0.0| 47 envelopes in 2 box(es); spanning depths of 0 to 940 feet; continuous coverage in 20 ft intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0066|38.92400186|-76.56301728|Anne Arundel|Maryland|AA De 125|South River||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385526076334801&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
969|AA Df 10|25.0|||RSY12|AA Df 10|0.0| 27 envelopes in 1 box(es); spanning depths of 0 to 350 feet; continuous coverage; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0067|38.98344523|-76.4885718|Anne Arundel|Maryland|AA Df 10|Annapolis||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385900076292008&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
970|AA Df 12|25.0|||RSY12|AA Df 12|0.0| 20 envelopes in 1 box(es); spanning depths of 0 to 584 feet; missing 125-170 ft.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0068|38.98344523|-76.4885718|Anne Arundel|Maryland|AA Df 12|Annapolis||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_21.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385900076292010&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
971|AA Df 19|25.0|||RSY12|AA Df 19|0.0| 17 envelopes in 1 box(es); spanning depths of 0 to 530 feet; missing intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0069|38.98955556|-76.45194444|Anne Arundel|Maryland|AA Df 19|Annapolis||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385921076270701&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
972|AA Df 20|25.0|||RSY12|AA Df 20|0.0| 87 envelopes in 2 box(es); spanning depths of 0 to 680 feet; missing intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0070|38.98816667|-76.45188889|Anne Arundel|Maryland|AA Df 20|Annapolis||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385916076270702&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
973|AA Df 65|25.0|||RSY12|AA Df 65|0.0| 48 envelopes in 3 box(es); spanning depths of 0 to 612 feet; continuous coverage; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0071|38.98705629|-76.47023803|Anne Arundel|Maryland|AA Df 65|Annapolis||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_21.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385913076281401&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
974|AA Df 79|25.0|||RSY12|AA Df 79|0.0| 37 envelopes in 2 box(es); spanning depths of 45 to 660 feet; missing intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0072|38.98486111|-76.49325|Anne Arundel|Maryland|AA Df 79|Annapolis||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385905076293601&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
975|AA Df 83|25.0|||RSY12|AA Df 83|0.0| 36 envelopes in 2 box(es); spanning depths of 0 to 751 feet; missing intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0073|38.98844508|-76.49912781|Anne Arundel|Maryland|AA Df 83|Annapolis||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_21.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385918076295801&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
976|AA Df 89|25.0|||RSY12|AA Df 89|0.0| 27 envelopes in 1 box(es); spanning depths of 0 to 270 feet; continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0074|38.993|-76.46186111|Anne Arundel|Maryland|AA Df 89|Annapolis||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385934076274302&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
977|AA Df 90|25.0|||RSY12|AA Df 90|0.0| 101 envelopes in 4 box(es); spanning depths of 1 to 510 feet; missing intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0075|38.92122462|-76.47329181|Anne Arundel|Maryland|AA Df 90|Annapolis||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385516076282501&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
978|AA Ed 16|25.0|||RSY12|AA Ed 16|0.0| 38 envelopes in 1 box(es); spanning depths of 0 to 190 feet; continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0076|38.91066834|-76.63829773|Anne Arundel|Maryland|AA Ed 16|Bowie||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385438076381901&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
979|AA Ed 19|25.0|||RSY12|AA Ed 19|0.0| 22 envelopes in 1 box(es); spanning depths of 240 to 455 feet; continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0077|38.88566922|-76.59607339|Anne Arundel|Maryland|AA Ed 19|South River||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385308076354701&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
980|AA Ed 39|25.0|||RSY12|AA Ed 39|0.0| 41 envelopes in 4 box(es); spanning depths of 0 to 480 feet; continuous coverage; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0078|38.86955831|-76.61912967|Anne Arundel|Maryland|AA Ed 39|Deale||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_21.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385210076371002&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
981|AA Ed 45|25.0|||RSY12|AA Ed 45|0.0| 11 envelopes in 1 box(es); spanning depths of 0 to 220 feet; continuous coverage in 20 ft intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0079|38.90204167|-76.64363889|Anne Arundel|Maryland|AA Ed 45|Bowie||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385406076383901&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
982|AA Ee 58|25.0|||RSY12|AA Ee 58|0.0| 16 envelopes in 1 box(es); spanning depths of 0 to 167 feet; nearly continuous coverage; missing 75-79 ft interval.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0080|38.84539275|-76.5502372|Anne Arundel|Maryland|AA Ee 58|Deale||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385043076330201&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
983|AA Ef 13|25.0|||RSY12|AA Ef 13|0.0| 18 envelopes in 1 box(es); spanning depths of 0 to 180 feet; continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0081|38.83456011|-76.49440105|Anne Arundel|Maryland|AA Ef 13|See Deale - See Clairborne||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385004076294101&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
984|AA Ef 15|25.0|||RSY12|AA Ef 15|0.0| 6 envelopes in 1 box(es); spanning depths of 20 to 312 feet; missing intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0082|38.91372482|-76.4713471|Anne Arundel|Maryland|AA Ef 15|Annapolis||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385449076281801&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
985|AA Fe 28|25.0|||RSY12|AA Fe 28|0.0| 40 envelopes in 1 box(es); spanning depths of 8 to 202 feet; 2 sets (washed and unwashed); samples from first 4 ft of each 10 ft interval.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0083|38.79872752|-76.51690107|Anne Arundel|Maryland|AA Fe 28|Deale||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=384755076310201&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
986|AA Fe 29|25.0|||RSY12|AA Fe 29|0.0| 26 envelopes in 1 box(es); spanning depths of 0 to 273 feet; 2 sets (washed and unwashed); continuous coverage in 20 ft intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0084|38.7562282|-76.55690218|Anne Arundel|Maryland|AA Fe 29|Deale||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=384522076332601&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
987|AA Fe 35|25.0|||RSY12|AA Fe 35|0.0| 43 envelopes in 2 box(es); spanning depths of 19 to 231 feet; 2 sets; samples from first 2 ft of each 10 ft interval; missing 139-141 ft.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0085|38.81400443|-76.57384876|Anne Arundel|Maryland|AA Fe 35|Deale||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=384850076342701&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
988|AA Fe 41|25.0|||RSY12|AA Fe 41|0.0| 15 envelopes in 1 box(es); spanning depths of 0 to 160 feet; missing 120-130 ft.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0086|38.83067072|-76.5707934|Anne Arundel|Maryland|AA Fe 41|Deale||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=384950076341601&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
989|AA Fe 47|25.0|||RSY12|AA Fe 47|0.0| 69 envelopes in 3 box(es); spanning depths of 0 to 700 feet; nearly continuous coverage in 10 ft intervals; missing 500-510 ft interval.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0087|38.81236111|-76.52386111|Anne Arundel|Maryland|AA Fe 47|Deale||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=384843076312601&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
990|AA Ge 3|25.0|||RSY12|AA Ge 3|0.0| 36 envelopes in 1 box(es); spanning depths of 0 to 315 feet; 2 sets (washed and unwashed); continuous coverage; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0088|38.74400625|-76.55801316|Anne Arundel|Maryland|AA Ge 3|North Beach||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=384438076333001&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
991|AA Ge 4|25.0|||RSY12|AA Ge 4|0.0| 70 envelopes in 2 box(es); spanning depths of 0 to 354 feet; 2 sets; continuous coverage; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0089|38.74400624|-76.55940213|Anne Arundel|Maryland|AA Ge 4|North Beach||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_8.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=384438076333501&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
992|AL Ac 53|25.0|||RSY12|AL Ac 53|0.0| 15 envelopes in 1 box(es); spanning depths of 0 to 150 feet; continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0090|39.69953034|-78.89196676|Allegheny|Maryland|AL Ac 53|Frostburg||cuttings||||http://www.mgs.md.gov/publications/report_pages/BULL_24.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=394158078533201&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
993|AL Ag 19|25.0|||RSY12|AL Ag 19|0.0| 9 envelopes in 1 box(es); spanning depths of 0 to 90 feet; continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0091|39.69703261|-78.55668222|Allegheny|Maryland|AL Ag 19|Flintstone||cuttings||||http://www.mgs.md.gov/publications/report_pages/BULL_24.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=394149078332501&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
994|AL Bc 64|25.0|||RSY12|AL Bc 64|0.0| 12 envelopes in 1 box(es); spanning depths of 1 to 118 feet; continuous coverage; generally in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:43:21|DAS02|WP0092|39.60629167|-78.84129167|Allegheny|Maryland|AL Bc 64|Cresaptown||cuttings||||http://www.mgs.md.gov/publications/report_pages/BULL_24.html|||||||||||||||||||||||||||||||||||||||
995|AL Be 47|25.0|||RSY12|AL Be 47|0.0| 5 envelopes in 1 box(es); spanning depths of 0 to 125 feet; continuous coverage in 5 ft intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0093|39.62536625|-78.72418421|Allegheny|Maryland|AL Be 47|Evitts Creek||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=393731078432801&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
996|AL Bi 15|25.0|||RSY12|AL Bi 15|0.0| 29 envelopes in 2 box(es); spanning depths of 0 to 145 feet; continuous coverage in 5 ft intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0094|39.62731409|-78.36167746|Allegheny|Maryland|AL Bi 15|Bellegrove||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=393738078214301&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
997|AL Bi 18|25.0|||RSY12|AL Bi 18|0.0| 24 envelopes in 1 box(es); spanning depths of 0 to 125 feet; nearly continuous coverage in 5 ft intervals; missing 80-85 ft interval.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0095|39.58398155|-78.39778858|Allegheny|Maryland|AL Bi 18|Paw Paw||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=393502078235301&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
998|AL Cc 25|25.0|||RSY12|AL Cc 25|0.0| 32 envelopes in 2 box(es); spanning depths of 0 to 37 feet; continuous coverage; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:43:21|DAS02|WP0096|39.56616667|-78.850425|Allegheny|Maryland|AL Cc 25|Cresaptown||cuttings||||http://www.mgs.md.gov/publications/report_pages/BULL_24.html|||||||||||||||||||||||||||||||||||||||
999|AL Cf 53|25.0|||RSY12|AL Cf 53|0.0| 10 envelopes in 1 box(es); spanning depths of 0 to 120 feet; missing 20-30 ft, 50-60 ft.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0097|39.53064764|-78.58918078|Allegheny|Maryland|AL Cf 53|Oldtown||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=393150078352201&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1000|AL Cf 54|25.0|||RSY12|AL Cf 54|0.0| 29 envelopes in 1 box(es); spanning depths of 0 to 145 feet; continuous coverage in 5 ft intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0098|39.53870231|-78.65029337|Allegheny|Maryland|AL Cf 54|Patterson Creek||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=393219078390201&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1001|AL Ch 13|25.0|||RSY12|AL Ch 13|0.0| 6 envelopes in 1 box(es); spanning depths of 0 to 180 feet; missing intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0099|39.57175911|-78.45362287|Allegheny|Maryland|AL Ch 13|Paw Paw||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=393418078271401&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1002|AL Ch 14|25.0|||RSY12|AL Ch 14|0.0| 30 envelopes in 2 box(es); spanning depths of 0 to 155 feet; continuous coverage in 5ft and 10 ft intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0100|39.54870408|-78.46334491|Allegheny|Maryland|AL Ch 14|Paw Paw||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=393255078274901&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1003|AL Ch 15|25.0|||RSY12|AL Ch 15|0.0| 23 envelopes in 1 box(es); spanning depths of 0 to 125 feet; missing 5-10 ft and 30-35 ft intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0101|39.53564887|-78.46390026|Allegheny|Maryland|AL Ch 15|Paw Paw||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=393208078275101&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1004|AL G 74|25.0|||RSY12|AL G 74|0.0| 268 envelopes in 9 box(es); spanning depths of 1070 to 4670 feet; missing intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:43:21|DAS02|WP0102|39.70953312|-78.45918085|Allegheny|Maryland|AL G 74|Artemas||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_5.html|||||||||||||||||||||||||||||||||||||||
1005|BA Cc 225|25.0|||RSY12|BA Cc 225|0.0| 36 envelopes in 2 box(es); spanning depths of 12 to 195 feet; continuous coverage; generally in 5 ft intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0103|39.53038304|-76.73664127|Baltimore|Maryland|BA Cc 225|Hereford||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=393149076441301&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1006|BA Cd 208|25.0|||RSY12|BA Cd 208|0.0| 41 envelopes in 2 box(es); spanning depths of 6 to 250 feet; continuous coverage; generally in 6 ft intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:43:21|DAS02|WP0104|39.50334722|-76.59161111|Baltimore|Maryland|BA Cd 208|Phoenix||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_1.html|||||||||||||||||||||||||||||||||||||||
1007|BA Ce 21|25.0|||RSY12|BA Ce 21|0.0| 23 envelopes in 1 box(es); spanning depths of 120 to 350 feet; continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0105|39.51658889|-76.57138333|Baltimore|Maryland|BA Ce 21|Phoenix||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_1.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=393102076341801&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1008|BA Dc 74|25.0|||RSY12|BA Dc 74|0.0| 40 envelopes in 1 box(es); spanning depths of 0 to 400 feet; continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0106|39.46010581|-76.72052921|Baltimore|Maryland|BA Dc 74|Cockeysville||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_1.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=392736076431501&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1009|BA Dc 75|25.0|||RSY12|BA Dc 75|0.0| 34 envelopes in 1 box(es); spanning depths of 0 to 350 feet; continuous coverage; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0107|39.45510578|-76.73025176|Baltimore|Maryland|BA Dc 75|Cockeysville||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=392718076435001&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1010|BA Df 39|25.0|||RSY12|BA Df 39|0.0| 70 envelopes in 3 box(es); spanning depths of 0 to 164 feet; nearly continuous coverage; missing interval 110-113 ft.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0108|39.4834401|-76.49329818|Baltimore|Maryland|BA Df 39|White Marsh||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_1.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=392900076293701&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1011|BA Df 54|25.0|||RSY12|BA Df 54|0.0| 35 envelopes in 1 box(es); spanning depths of 20 to 200 feet; continuous coverage in 5 ft intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0109|39.44760718|-76.45496304|Baltimore|Maryland|BA Df 54|White Marsh||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_1.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=392651076271901&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1012|BA Ea 16|25.0|||RSY12|BA Ea 16|0.0| 16 envelopes in 1 box(es); spanning depths of 0 to 150 feet; continuous coverage; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0110|39.35510516|-76.85358699|Baltimore|Maryland|BA Ea 16|Ellicott City||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_1.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=392118076511401&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1013|BA Ea 17|25.0|||RSY12|BA Ea 17|0.0| 25 envelopes in 2 box(es); spanning depths of 0 to 250 feet; continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0111|39.34482745|-76.85636469|Baltimore|Maryland|BA Ea 17|Ellicott City||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_1.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=392041076512401&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1014|BA Ed 27|25.0|||RSY12|BA Ed 27|0.0| 32 envelopes in 1 box(es); spanning depths of 0 to 160 feet; continuous coverage in 5 ft intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0112|39.38427333|-76.60719033|Baltimore|Maryland|BA Ed 27|Towson||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_1.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=392303076362701&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1015|BA Fg 15|25.0|||RSY12|BA Fg 15|0.0| 20 envelopes in 1 box(es); spanning depths of 30 to 280 feet; missing intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0113|39.26733037|-76.38745887|Baltimore|Maryland|BA Fg 15|Middle River||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_1.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=391602076231601&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1016|BA Fg 66|25.0|||RSY12|BA Fg 66|0.0| 80 envelopes in 4 box(es); spanning depths of 0 to 790 feet; missing intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0114|39.25677474|-76.41523737|Baltimore|Maryland|BA Fg 66|Middle River||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_1.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=391524076245601&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1017|BA Gc 34|25.0|||RSY12|BA Gc 34|0.0| 25 envelopes in 2 box(es); spanning depths of 0 to 160 feet; missing 97-100 ft interval.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0115|39.22121837|-76.68996943|Baltimore|Maryland|BA Gc 34|Relay||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=391316076412501&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1018|BA Gc 35|25.0|||RSY12|BA Gc 35|0.0| 24 envelopes in 2 box(es); spanning depths of 0 to 114 feet; continuous coverage; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0116|39.22205175|-76.67746895|Baltimore|Maryland|BA Gc 35|Relay||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=391319076404001&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1019|BA Gg 3|25.0|||RSY12|BA Gg 3|0.0| 10 envelopes in 1 box(es); spanning depths of 0 to 180 feet; missing intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0117|39.33888889|-76.36333333|Baltimore|Maryland|BA Gg 3|Gunpowder Neck||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_1.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=391353076292701&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1020|CA Bb 9|25.0|||RSY12|CA Bb 9|0.0| 22 envelopes in 2 box(es); spanning depths of 0 to 288 feet; continuous coverage; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0118|38.7353947|-76.62662808|Calvert|Maryland|CA Bb 9|Lower Marlboro||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_14.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=384407076373701&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1021|CA Bb 10|25.0|||RSY12|CA Bb 10|0.0| 39 envelopes in 1 box(es); spanning depths of 640 to 711 feet; 2 sets (washed and unwashed); continuous coverage; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0119|38.67419444|-76.59422222|Calvert|Maryland|CA Bb 10|North Beach||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_21.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=384028076354201&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1022|CA Bb 23|25.0|||RSY12|CA Bb 23|0.0| 54 envelopes in 4 box(es); spanning depths of 0 to 540 feet; continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0120|38.74927778|-76.63297222|Calvert|Maryland|CA Bb 23|Lower Marlboro||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_21.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=384458076375501&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1023|CA Bb 25|25.0|||RSY12|CA Bb 25|0.0| 62 envelopes in 3 box(es); spanning depths of 0 to 668 feet; continuous coverage; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0121|38.68536111|-76.65227778|Calvert|Maryland|CA Bb 25|Lower Marlboro||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_21.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=384109076391101&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1024|CA Bb 27|25.0|||RSY12|CA Bb 27|0.0| 11 envelopes in 1 box(es); spanning depths of 220 to 440 feet; continuous coverage in 20 ft intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0122|38.72611111|-76.66338889|Calvert|Maryland|CA Bb 27|Lower Marlboro||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_21.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=384333076394701&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1025|CA Bb 28|25.0|||RSY12|CA Bb 28|0.0| 10 envelopes in 1 box(es); spanning depths of 10 to 200 feet; nearly continuous coverage in 20 ft intervals; missing 0-10 ft interval.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0123|38.72616667|-76.66341667|Calvert|Maryland|CA Bb 28|Lower Marlboro||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_21.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=384333076394702&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1026|CA Bc 14|25.0|||RSY12|CA Bc 14|0.0| 61 envelopes in 2 box(es); spanning depths of 0 to 315 feet; 2 sets (washed and unwashed); continuous coverage in washed set.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0124|38.71317361|-76.55662393|Calvert|Maryland|CA Bc 14|North Beach||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_14.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=384247076332501&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1027|CA Bc 15|25.0|||RSY12|CA Bc 15|0.0| 28 envelopes in 1 box(es); spanning depths of 0 to 210 feet; 2 sets (washed and unwashed); continuous coverage; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0125|38.68678547|-76.53412246|Calvert|Maryland|CA Bc 15|North Beach||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_14.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=384112076320401&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1028|CA Bc 25|25.0|||RSY12|CA Bc 25|0.0| 11 envelopes in 1 box(es); spanning depths of 0 to 365 feet; continuous coverage; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0126|38.68734102|-76.53384467|Calvert|Maryland|CA Bc 25|North Beach||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_14.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=384114076320301&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1029|CA Ca 2|25.0|||RSY12|CA Ca 2|0.0| 85 envelopes in 3 box(es); spanning depths of 0 to 458 feet; missing intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0127|38.62623054|-76.67162943|Calvert|Maryland|CA Ca 2|Lower Marlboro||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_14.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383734076401901&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1030|CA Cc 1|25.0|||RSY12|CA Cc 1|0.0| 42 envelopes in 1 box(es); spanning depths of 8 to 211 feet; washed and unwashed; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0128|38.60567621|-76.50384239|Calvert|Maryland|CA Cc 1|Prince Frederick||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_14.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383620076301501&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1031|CA Cc 8|25.0|||RSY12|CA Cc 8|0.0| 42 envelopes in 1 box(es); spanning depths of 0 to 210 feet; washed and unwashed; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0129|38.62900901|-76.51689883|Calvert|Maryland|CA Cc 8|North Beach||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_14.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383744076310201&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1032|CA Cc 28|25.0|||RSY12|CA Cc 28|0.0| 52 envelopes in 2 box(es); spanning depths of 0 to 273 feet; continuous coverage; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0130|38.66567484|-76.5296776|Calvert|Maryland|CA Cc 28|North Beach||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_14.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383956076314801&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1033|CA Cc 36|25.0|||RSY12|CA Cc 36|0.0| 40 envelopes in 1 box(es); spanning depths of 0 to 310 feet; 2 sets (washed and unwashed); continuous coverage in 10 to 20 ft intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0131|38.64789745|-76.52662173|Calvert|Maryland|CA Cc 36|North Beach||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_14.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383852076313701&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1034|CA Cc 37|25.0|||RSY12|CA Cc 37|0.0| 65 envelopes in 2 box(es); spanning depths of 0 to 330 feet; continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0132|38.6103977|-76.6544061|Calvert|Maryland|CA Cc 37|Benedict||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_14.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383637076391701&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1035|CA Cc 55|25.0|||RSY12|CA Cc 55|0.0| 97 envelopes in 4 box(es); spanning depths of 0 to 1017 feet; missing intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0133|38.65997222|-76.53286111|Calvert|Maryland|CA Cc 55|North Beach||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_14.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383934076320201&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1036|CA Cc 57|25.0|||RSY12|CA Cc 57|0.0| 37 envelopes in 2 box(es); spanning depths of 0 to 577 feet; missing 137-157 ft.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0134|38.60119444|-76.57969444|Calvert|Maryland|CA Cc 57|Prince Frederick||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_14.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383605076344601&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1037|CA Db 3|25.0|||RSY12|CA Db 3|0.0| 41 envelopes in 2 box(es); spanning depths of 0 to 419 feet; continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0135|38.51928895|-76.65329397|Calvert|Maryland|CA Db 3|Benedict||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_14.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383109076391301&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1038|CA Db 3|25.0|||RSY12|CA Db 3|0.0| 41 envelopes in 2 box(es); spanning depths of 0 to 419 feet; continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0136|38.51928895|-76.65329397|Calvert|Maryland|CA Db 3|Benedict||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_14.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383109076391301&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1039|CA Db 12|25.0|||RSY12|CA Db 12|0.0| 32 envelopes in 1 box(es); spanning depths of 0 to 330 feet; continuous coverage; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0137|38.50595597|-76.66190539|Calvert|Maryland|CA Db 12|Benedict||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_14.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383021076394401&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1040|CA Db 36|25.0|||RSY12|CA Db 36|0.0| 324 envelopes in 16 box(es); spanning depths of 0 to 1508 feet; 2 sets provide continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0138|38.55456596|-76.5849574|Calvert|Maryland|CA Db 36|Prince Frederick||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_14.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383316076350701&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1041|CA Db 47|25.0|||RSY12|CA Db 47|0.0| 35 envelopes in 2 box(es); spanning depths of 0 to 680 feet; continuous coverage generally in 20 ft intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0139|38.54355556|-76.59466667|Calvert|Maryland|CA Db 47|Prince Frederick||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_14.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383239076354201&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1042|CA Dc 16|25.0|||RSY12|CA Dc 16|0.0| 72 envelopes in 2 box(es); spanning depths of 0 to 360 feet; continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0140|38.5117892|-76.51717572|Calvert|Maryland|CA Dc 16|Prince Frederick||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_14.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383042076310301&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1043|CA Dc 17|25.0|||RSY12|CA Dc 17|0.0| 116 envelopes in 4 box(es); spanning depths of 0 to 555.3 feet; missing intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0141|38.53817746|-76.58217933|Calvert|Maryland|CA Dc 17|Prince Frederick||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_14.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383217076345701&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1044|CA Dc 35|25.0|||RSY12|CA Dc 35|0.0| 101 envelopes in 5 box(es); spanning depths of 0 to 1000 feet; continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0142|38.51419444|-76.51441667|Calvert|Maryland|CA Dc 35|Prince Frederick||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_14.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383050076305501&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1045|CA Eb 4|25.0|||RSY12|CA Eb 4|0.0| 80 envelopes in 3 box(es); spanning depths of 0 to 399 feet; 2 sets (washed and unwashed); missing 330-340 ft interval.||WJUNKIN|2021-08-19 16:38:48|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0143|38.47678985|-76.59634654|Calvert|Maryland|CA Eb 4|Broomes Island||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=382836076354801&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1046|CA Ec 3|25.0|||RSY12|CA Ec 3|0.0| 80 envelopes in 3 box(es); spanning depths of 0 to 345 feet; 2 sets; missing 155-165 ft interval.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0144|38.47206754|-76.50578633|Calvert|Maryland|CA Ec 3|Broomes Island||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_14.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=382819076302201&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1047|CA Ec 19|25.0|||RSY12|CA Ec 19|0.0| 50 envelopes in 2 box(es); spanning depths of 9 to 251 feet; 2 sets (washed and unwashed); samples collected about every 10 ft.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0145|38.42373506|-76.5674565|Calvert|Maryland|CA Ec 19|Broomes Island||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_14.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=382525076340401&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1048|CA Ed 2|25.0|||RSY12|CA Ed 2|0.0| 30 envelopes in 1 box(es); spanning depths of 1 to 300 feet; samples collected about every 10 ft.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0146|38.46984518|-76.47050733|Calvert|Maryland|CA Ed 2|Cove Point||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=382811076281501&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1049|CA Ed 5|25.0|||RSY12|CA Ed 5|0.0| 66 envelopes in 2 box(es); spanning depths of 8 to 330 feet; 2 sets (washed and unwashed); samples collected about every 10 ft.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0147|38.42262354|-76.48550808|Calvert|Maryland|CA Ed 5|Cove Point||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_14.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=382521076290901&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1050|CA Ed 6|25.0|||RSY12|CA Ed 6|0.0| 51 envelopes in 2 box(es); spanning depths of 0 to 273 feet; 2 sets; continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0148|38.46067859|-76.46689615|Calvert|Maryland|CA Ed 6|Cove Point||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_14.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=382738076280201&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1051|CA Ed 8|25.0|||RSY12|CA Ed 8|0.0| 18 envelopes in 1 box(es); spanning depths of 5 to 273 feet; continuous coverage; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0149|38.41734565|-76.45745162|Calvert|Maryland|CA Ed 8|Cove Point||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_14.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=382502076272801&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1052|CA Ed 22|25.0|||RSY12|CA Ed 22|0.0| 46 envelopes in 2 box(es); spanning depths of 0 to 789 feet; continuous coverage; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0150|38.43428985|-76.44495113|Calvert|Maryland|CA Ed 22|Cove Point||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_21.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=382603076264301&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1053|CA Ed 23|25.0|||RSY12|CA Ed 23|0.0| 19 envelopes in 1 box(es); spanning depths of 0 to 400 feet; nearly continuous coverage in 20 ft intervals; missing 300-320 ft interval.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0151|38.43567872|-76.44383997|Calvert|Maryland|CA Ed 23|Cove Point||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_21.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=382608076263901&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1054|CA Ed 47|25.0|||RSY12|CA Ed 47|0.0| 46 envelopes in 3 box(es); spanning depths of 0 to 565 feet; nearly continuous coverage; sampling intervals vary; missing 440-455 ft interval.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0152|38.4331787|-76.43745089|Calvert|Maryland|CA Ed 47|Cove Point||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=382559076261601&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1055|CA Fd 4|25.0|||RSY12|CA Fd 4|0.0| 50 envelopes in 1 box(es); spanning depths of 8 to 252 feet; 2 sets (washed and unwashed); samples collected about every 10 ft.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0153|38.40512374|-76.48745269|Calvert|Maryland|CA Fd 4|Cove Point||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_14.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=382418076291601&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1056|CA Fd 5|25.0|||RSY12|CA Fd 5|0.0| 62 envelopes in 3 box(es); spanning depths of 0 to 325.6 feet; 2 sets; continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0154|38.35345748|-76.46634113|Calvert|Maryland|CA Fd 5|Solomons Island||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_14.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=382112076280001&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1057|CA Fd 7|25.0|||RSY12|CA Fd 7|0.0| 56 envelopes in 3 box(es); spanning depths of 10 to 294 feet; 2 sets; continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0155|38.33956868|-76.45772978|Calvert|Maryland|CA Fd 7|Solomons Island||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_14.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=382022076272901&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1058|CA Fd 19|25.0|||RSY12|CA Fd 19|0.0| 57 envelopes in 2 box(es); spanning depths of 25 to 309.1 feet; 2 sets; continuous coverage in 10 to 11 ft intervals.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0156|38.38734621|-76.49717536|Calvert|Maryland|CA Fd 19|Cove Point||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_14.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=382314076295101&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1059|CA Fd 22|25.0|||RSY12|CA Fd 22|0.0| 84 envelopes in 3 box(es); spanning depths of 0 to 441 feet; 2 sets; continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0157|38.38679026|-76.43356205|Calvert|Maryland|CA Fd 22|Cove Point||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_14.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=382312076260201&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1060|CA Fd 54|25.0|||RSY12|CA Fd 54|0.0| 41 envelopes in 2 box(es); spanning depths of 0 to 698 feet; nearly continuous coverage; sampling intervals vary; missing515-518 ft interval.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0158|38.40225|-76.43461111|Calvert|Maryland|CA Fd 54|Cove Point||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_14.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=382407076260301&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1061|CA Fe 3|25.0|||RSY12|CA Fe 3|0.0|  envelopes in 1 box(es); spanning depths of 0 to 462 feet; samples from 0-199.5 ft only; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0159|38.38151225|-76.38911608|Calvert|Maryland|CA Fe 3|Cove Point||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_14.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=382253076232202&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1062|CA Fe 29|25.0|||RSY12|CA Fe 29|0.0| 148 envelopes in 9 box(es); spanning depths of 0 to 1500 feet; missing 1420-1470 ft interval; otherwise continuous in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:21|DAS02|WP0160|38.38617222|-76.40800278|Calvert|Maryland|CA Fe 29|Cove Point||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_14.html|||||||||||||||||||||||||||||||||||||||
1063|CA Gd 4|25.0|||RSY12|CA Gd 4|0.0| 56 envelopes in 2 box(es); spanning depths of 0 to 280 feet; 2 sets; continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0161|38.3290132|-76.45356301|Calvert|Maryland|CA Gd 4|Solomons Island||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_14.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=381944076271401&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1064|CA Gd 30|25.0|||RSY12|CA Gd 30|0.0| 47 envelopes in 2 box(es); spanning depths of 63 to 315 feet; 2 sets; continuous coverage in 10 to 11 ft intervals.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0162|38.32401329|-76.45967437|Calvert|Maryland|CA Gd 30|Solomons Island||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_14.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=381926076273601&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1065|CA Gd 48|25.0|||RSY12|CA Gd 48|0.0| 60 envelopes in 3 box(es); spanning depths of 0 to 600 feet; continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0163|38.32679096|-76.44745168|Calvert|Maryland|CA Gd 48|Solomons Island||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_14.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=381936076265201&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1066|CA Gd 50|25.0|||RSY12|CA Gd 50|0.0| 11 envelopes in 1 box(es); spanning depths of 40 to 270 feet; nearly continuous coverage in 20 ft intervals; missing 60-70 ft interval.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0164|38.33262422|-76.44578493|Calvert|Maryland|CA Gd 50|Solomons Island||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_14.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=381957076264601&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1067|CE Ac 26|25.0|||RSY12|CE Ac 26|0.0| 19 envelopes in 1 box; spanning depths of 2 to 95 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:21|DAS02|WP0165|39.69934167|-76.05632778|Cecil|Maryland|CE Ac 26|Rising Sun||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_16.html|||||||||||||||||||||||||||||||||||||||
1068|CE Ac 118|25.0|||RSY12|CE Ac 118|0.0| 66 envelopes in 4 boxes; spanning depths of 0 to 350 feet; generally 5 ft samping intervals to 240; variable intervals below.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0166|39.69538707|-76.0657822|Cecil|Maryland|CE Ac 118|Rising Sun||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=394143076035801&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1069|CE Bd 11|25.0|||RSY12|CE Bd 11|0.0| 6 envelopes in 1 box; spanning depths of 0 to 78 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0167|39.60927972|-75.94633293|Cecil|Maryland|CE Bd 11|North East||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_16.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=393633075564801&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1070|CE Bd 65|25.0|||RSY12|CE Bd 65|0.0| 12 envelopes in 1 box; spanning depths of 6 to 182 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0168|39.60844644|-75.95049981|Cecil|Maryland|CE Bd 65|North East||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_16.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=393630075570301&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1071|CE Be 46|25.0|||RSY12|CE Be 46|0.0| 39 envelopes in 2 boxes; spanning depths of 10 to 205 feet; 2 sets in a mix of 5 ft and 10 ft intervals.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0169|39.60455706|-75.87716283|Cecil|Maryland|CE Be 46|North East||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_16.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=393616075523901&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1072|CE Be 62|25.0|||RSY12|CE Be 62|0.0| 13 envelopes in 1 box; spanning depths of 0 to 130 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0170|39.6065012|-75.84299447|Cecil|Maryland|CE Be 62|Elkton||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_16.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=393623075503601&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1073|CE Be 73|25.0|||RSY12|CE Be 73|0.0| 14 envelopes in 1 box; spanning depths of 0 to 175 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0171|39.61039044|-75.89688604|Cecil|Maryland|CE Be 73|North East||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=393637075535001&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1074|CE Bf 81|25.0|||RSY12|CE Bf 81|0.0| 12 envelopes in 1 box; spanning depths of 0 to 95 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0172|39.60427865|-75.79938118|Cecil|Maryland|CE Bf 81|Elkton||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=393615075475901&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1075|CE Bf 82|25.0|||RSY12|CE Bf 82|0.0| 20 envelopes in 2 boxes; spanning depths of 0 to 280 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0173|39.59361111|-75.82211111|Cecil|Maryland|CE Bf 82|Elkton||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=393537075492001&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1076|CE Cc 17|25.0|||RSY12|CE Cc 17|0.0| 6 envelopes in 1 box; spanning depths of 0 to 28 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0174|39.56872354|-76.07856091|Cecil|Maryland|CE Cc 17|Havre De Grace||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_16.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=393407076044401&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1077|CE Cd 33|25.0|||RSY12|CE Cd 33|0.0| 30 envelopes in 1 box; spanning depths of 1 to 175 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:21|DAS02|WP0175|39.51966944|-75.98020556|Cecil|Maryland|CE Cd 33|North East||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_16.html|||||||||||||||||||||||||||||||||||||||
1078|CE Cd 51|25.0|||RSY12|CE Cd 51|0.0| 28 envelopes in 2 boxes; spanning depths of 0 to 159 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0176|39.57567001|-75.99300206|Cecil|Maryland|CE Cd 51|North East||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=393432075593601&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1079|CE Cd 53|25.0|||RSY12|CE Cd 53|0.0| 39 envelopes in 3 boxes; spanning depths of 0 to 495 feet; sampling intervals vary; missing 325 to 330 ft interval.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0177|39.53789262|-75.94466632|Cecil|Maryland|CE Cd 53|North East||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=393216075564201&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1080|CE Ce 2|25.0|||RSY12|CE Ce 2|0.0| 10 envelopes in 1 box; spanning depths of 0 to 120 feet; samples in 10 ft intervals to 90 ft depth; samping interval 30 ft below||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0178|39.57983477|-75.83382724|Cecil|Maryland|CE Ce 2|Elkton||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_16.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=393447075500301&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1081|CE Ce 22|25.0|||RSY12|CE Ce 22|0.0| 18 envelopes in 1 box; spanning depths of 0 to 201 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0179|39.5481688|-75.85577271|Cecil|Maryland|CE Ce 22|Elkton||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_16.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=393253075512201&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1082|CE Ce 54|25.0|||RSY12|CE Ce 54|0.0| 22 envelopes in 2 boxes; spanning depths of 0 to 285 feet; sampling interval varies to 155 ft depth; mix of 15 an 20 ft intervals below.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0180|39.57594685|-75.91327575|Cecil|Maryland|CE Ce 54|North East||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=393433075544901&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1083|CE Ce 55|25.0|||RSY12|CE Ce 55|0.0| 42 envelopes in 3 boxes; spanning depths of 0 to 622 feet; sampling interval varies to 205 ft depth; generally mix of 15 an 20 ft intervals below.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0181|39.54480556|-75.83369444|Cecil|Maryland|CE Ce 55|Elkton||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=393241075500201&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1084|CE Ce 56|25.0|||RSY12|CE Ce 56|0.0| 24 envelopes in 2 boxes; spanning depths of 0 to 420 feet; sampling intervals vary; a few intervals missing.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0182|39.50761111|-75.87491667|Cecil|Maryland|CE Ce 56|Elkton||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=393026075523101&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1085|CE Cf 5|25.0|||RSY12|CE Cf 5|0.0| 15 envelopes in 1 box; spanning depths of 0 to 150 feet; continuous coverage in 5 ft intervals.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:21|DAS02|WP0183|39.54130833|-75.78054167|Cecil|Maryland|CE Cf 5|Elkton||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_16.html|||||||||||||||||||||||||||||||||||||||
1086|CE Cf 48|25.0|||RSY12|CE Cf 48|0.0| 21 envelopes in 2 boxes; spanning depths of 0 to 695 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0184|39.53844578|-75.79771402|Cecil|Maryland|CE Cf 48|Elkton||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_16.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=393218075475301&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1087|CE Cf 53|25.0|||RSY12|CE Cf 53|0.0| 37 envelopes in 2 boxes; spanning depths of 0 to 430 feet; samples in 10 ft intervals to 310 ft depth; variable sampling intevals below.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0185|39.53872353|-75.79604727|Cecil|Maryland|CE Cf 53|Elkton||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_16.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=393219075474701&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1088|CE Dc 2|25.0|||RSY12|CE Dc 2|0.0| 23 envelopes in 1 box; spanning depths of 510 to 849 feet; sampling intervals vary; a few intervals missing.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:21|DAS02|WP0186|39.45455976|-76.00800239|Cecil|Maryland|CE Dc 2|Spesutie||cuttings||||http://www.mgs.md.gov/publications/report_pages/OFR_12-02-20.html|||||||||||||||||||||||||||||||||||||||
1089|CE Dd 47|25.0|||RSY12|CE Dd 47|0.0| 20 envelopes in 1 box; spanning depths of 0 to 93.1 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:21|DAS02|WP0187|39.43898333|-75.97765833|Cecil|Maryland|CE Dd 47|Earleville||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_16.html|||||||||||||||||||||||||||||||||||||||
1090|CE Dd 71|25.0|||RSY12|CE Dd 71|0.0| 57 envelopes in 3 boxes; spanning depths of 0 to 528 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0188|39.47233799|-75.98161248|Cecil|Maryland|CE Dd 71|Earleville||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_16.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=392820075585501&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1091|CE Dd 81|25.0|||RSY12|CE Dd 81|0.0| 35 envelopes in 3 boxes; spanning depths of 0 to 500 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0189|39.42688889|-75.99163889|Cecil|Maryland|CE Dd 81|Earleville||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=392536075593201&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1092|CE De 5|25.0|||RSY12|CE De 5|0.0| 4 envelopes in 1 box; spanning depths of 1 to 95 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:21|DAS02|WP0190|39.444775|-75.84160278|Cecil|Maryland|CE De 5|Cecilton||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_16.html|||||||||||||||||||||||||||||||||||||||
1093|CE De 14|25.0|||RSY12|CE De 14|0.0| 20 envelopes in 1 box; spanning depths of 0 to 124 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:21|DAS02|WP0191|39.46556944|-75.88297778|Cecil|Maryland|CE De 14|Earleville||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_16.html|||||||||||||||||||||||||||||||||||||||
1094|CE De 41|25.0|||RSY12|CE De 41|0.0| 103 envelopes in 7 boxes; spanning depths of 0 to 400 feet; largely continuous coverage in 3 ft intervals.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0192|39.44928077|-75.91605311|Cecil|Maryland|CE De 41|Earleville||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_16.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=392657075545901&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1095|CE Ec 6|25.0|||RSY12|CE Ec 6|0.0| 6 envelopes in 1 box; spanning depths of 0 to 55 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0193|39.38539063|-76.02966888|Cecil|Maryland|CE Ec 6|Spesutie||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_16.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=392307076014803&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1096|CE Ec 15|25.0|||RSY12|CE Ec 15|0.0| 26 envelopes in 1 box; spanning depths of 0 to 1107 feet; sampling intervals vary; a few intervals missing.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0194|39.40511349|-76.02466896|Cecil|Maryland|CE Ec 15|Spesutie||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_16.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=392418076013001&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1097|CE Ec 18|25.0|||RSY12|CE Ec 18|0.0| 14 envelopes in 1 box; spanning depths of 0 to 27 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0195|39.39705807|-76.00716815|Cecil|Maryland|CE Ec 18|Spesutie||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=392349076002701&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1098|CE Ec 19|25.0|||RSY12|CE Ec 19|0.0| 20 envelopes in 2 boxes; spanning depths of 0 to 47 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0196|39.39622435|-76.02466883|Cecil|Maryland|CE Ec 19|Spesutie||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=392346076013001&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1099|CE Ed 19|25.0|||RSY12|CE Ed 19|0.0| 15 envelopes in 1 box; spanning depths of 0 to 52 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0197|39.4017801|-75.95077656|Cecil|Maryland|CE Ed 19|Earleville||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=392404075570601&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1100|CE Ed 20|25.0|||RSY12|CE Ed 20|0.0| 10 envelopes in 1 box; spanning depths of 0 to 42 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0198|39.39955799|-75.96827741|Cecil|Maryland|CE Ed 20|Earleville||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=392358075580701&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1101|CE Ed 21|25.0|||RSY12|CE Ed 21|0.0| 8 envelopes in 1 box; spanning depths of 0 to 22 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0199|39.39789151|-75.99105632|Cecil|Maryland|CE Ed 21|Earleville||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=392352075592901&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1102|CE Ee 3|25.0|||RSY12|CE Ee 3|0.0| 33 envelopes in 2 boxes; spanning depths of 10 to 336 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:21|DAS02|WP0200|39.37594444|-75.87163056|Cecil|Maryland|CE Ee 3|Cecilton||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_16.html|||||||||||||||||||||||||||||||||||||||
1103|CE Ee 7|25.0|||RSY12|CE Ee 7|0.0| 26 envelopes in 1 box; spanning depths of 0 to 282 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:21|DAS02|WP0201|39.3683367|-75.87793889|Cecil|Maryland|CE Ee 7|Galena||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_16.html|||||||||||||||||||||||||||||||||||||||
1104|CE Ee 10|25.0|||RSY12|CE Ee 10|0.0| 7 envelopes in 1 box; spanning depths of 0 to 141 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0202|39.41344658|-75.90938569|Cecil|Maryland|CE Ee 10|Earleville||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_16.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=392448075543501&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1105|CE Ee 11|25.0|||RSY12|CE Ee 11|0.0| 25 envelopes in 1 box; spanning depths of 0 to 240 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0203|39.40372372|-75.86716122|Cecil|Maryland|CE Ee 11|Cecilton||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_16.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=392413075520301&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1106|CE Ee 29|25.0|||RSY12|CE Ee 29|0.0| 109 envelopes in 7 boxes; spanning depths of 0 to 1459 feet; largely continuous coverage in 10 and 15 ft intervals.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0204|39.40149693|-75.87154545|Cecil|Maryland|CE Ee 29|Cecilton||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_16.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=392403075521801&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1107|CE Ee 30|25.0|||RSY12|CE Ee 30|0.0| 14 envelopes in 1 box; spanning depths of 0 to 30 feet; sampling intervals vary; a few intervals missing.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0205|39.41111111|-75.91055556|Cecil|Maryland|CE Ee 30|Earleville||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_16.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=392407075541001&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1108|CH Ac 10|25.0|||RSY12|CH Ac 10|0.0| 9 envelopes in 1 box; spanning depths of 0 to 186 feet; continuous coverage in 20 and 21 ft intervals.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0206|38.68344951|-77.11581205|Charles|Maryland|CH Ac 10|Mount Vernon||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=384100077065801&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1109|CH Bc 12|25.0|||RSY12|CH Bc 12|0.0| 40 envelopes in 2 boxes; spanning depths of 50 to 233 feet; largely continuous coverage; generally 10 ft sampling intervals.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0207|38.59678545|-77.09747747|Charles|Maryland|CH Bc 12|Port Tobacco||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_76.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383548077055201&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1110|CH Bc 13|25.0|||RSY12|CH Bc 13|0.0| 54 envelopes in 2 boxes; spanning depths of 0 to 264 feet; 2 sets; one with continuous coverage, generally 10 ft intervals.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0208|38.60678512|-77.1199782|Charles|Maryland|CH Bc 13|Port Tobacco||cuttings||||https://waterdata.usgs.gov/nwis/inventory|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383624077071301&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1111|CH Bc 49|25.0|||RSY12|CH Bc 49|0.0| 29 envelopes in 2 boxes; spanning depths of 0 to 404 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0209|38.59456321|-77.15164566|Charles|Maryland|CH Bc 49|Indian Head||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_76.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383540077090701&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1112|CH Bc 52|25.0|||RSY12|CH Bc 52|0.0| 43 envelopes in 3 boxes; spanning depths of 0 to 430 feet; continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0210|38.59789653|-77.09803305|Charles|Maryland|CH Bc 52|Port Tobacco||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383552077055401&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1113|CH Bc 53|25.0|||RSY12|CH Bc 53|0.0| 34 envelopes in 2 boxes; spanning depths of 73 to 672 feet; sampling intervals vary; a few intervals missing.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0211|38.60872961|-77.05525412|Charles|Maryland|CH Bc 53|Port Tobacco||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383631077032001&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1114|CH Bc 54|25.0|||RSY12|CH Bc 54|0.0| 53 envelopes in 4 boxes; spanning depths of 0 to 532 feet; largely continous coverage mainly in 10 ft intervals||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0212|38.62289581|-77.08636623|Charles|Maryland|CH Bc 54|Port Tobacco||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383722077051201&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1115|CH Bc 58|25.0|||RSY12|CH Bc 58|0.0| 21 envelopes in 1 box; spanning depths of 0 to 205 feet; continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0213|38.64150633|-77.10720033|Charles|Maryland|CH Bc 58|Mount Vernon||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383829077062701&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1116|CH Bc 59|25.0|||RSY12|CH Bc 59|0.0| 20 envelopes in 1 box; spanning depths of 0 to 187 feet; largely continous coverage mainly in 10 ft intervals||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0214|38.64122856|-77.10886705|Charles|Maryland|CH Bc 59|Mount Vernon||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383828077063301&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1117|CH Bc 61|25.0|||RSY12|CH Bc 61|0.0| 22 envelopes in 1 box; spanning depths of 0 to 780 feet; sampling intervals vary; a few intervals missing.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0215|38.60984055|-77.14108995|Charles|Maryland|CH Bc 61|Indian Head||cuttings||||http://www.mgs.md.gov/publications/report_pages/OFR_12-02-20.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383635077082901&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1118|CH Bc 65|25.0|||RSY12|CH Bc 65|0.0| 66 envelopes in 3 boxes; spanning depths of 0 to 645 feet; largely continous coverage mainly in 10 ft intervals||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0216|38.62734012|-77.08553291|Charles|Maryland|CH Bc 65|Mount Vernon||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_69.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383738077050901&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1119|CH Bc 75|25.0|||RSY12|CH Bc 75|0.0| 80 envelopes in 3 boxes; spanning depths of 0 to 800 feet; largely continous coverage mainly in 10 ft intervals||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0217|38.61302778|-77.10594444|Charles|Maryland|CH Bc 75|Port Tobacco||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_69.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383645077062401&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1120|CH Bd 1|25.0|||RSY12|CH Bd 1|0.0| 5 envelopes in 1 box; spanning depths of 208 to 292 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0218|38.61789597|-77.07692148|Charles|Maryland|CH Bd 1|Port Tobacco||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383703077041402&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1121|CH Bd 11|25.0|||RSY12|CH Bd 11|0.0| 49 envelopes in 2 boxes; spanning depths of 0 to 270 feet; samples in 10 ft intervals; some intervals missing||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0219|38.61789597|-77.07692148|Charles|Maryland|CH Bd 11|Port Tobacco||cuttings||||http://www.mgs.md.gov/publications/report_pages/OFR_12-02-20.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383704077043801&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1122|CH Bd 14|25.0|||RSY12|CH Bd 14|0.0| 155 envelopes in 5 boxes; spanning depths of 0 to 1060 feet; largely continous coverage mainly in 10 ft intervals||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0220|38.58900802|-77.02719766|Charles|Maryland|CH Bd 14|Port Tobacco||cuttings||||http://www.mgs.md.gov/publications/report_pages/OFR_12-02-20.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383520077013901&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1123|CH Bd 29|25.0|||RSY12|CH Bd 29|0.0| 64 envelopes in 4 boxes; spanning depths of 0 to 628 feet; continous coverage mainly in 10 ft intervals||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0221|38.63483991|-77.0808106|Charles|Maryland|CH Bd 29|Mount Vernon||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_69.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383805077045201&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1124|CH Bd 31|25.0|||RSY12|CH Bd 31|0.0| 94 envelopes in 6 boxes; spanning depths of 0 to 879 feet; continous coverage mainly in 10 ft intervals||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0222|38.60428535|-77.02469766|Charles|Maryland|CH Bd 31|Port Tobacco||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383615077013001&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1125|CH Bd 32|25.0|||RSY12|CH Bd 32|0.0| 65 envelopes in 5 boxes; spanning depths of 0 to 654 feet; largely continuous coverage; sampling interval varies||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0223|38.61567382|-77.0741436|Charles|Maryland|CH Bd 32|Port Tobacco||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_69.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383656077042801&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1126|CH Bd 46|25.0|||RSY12|CH Bd 46|0.0| 85 envelopes in 5 boxes; spanning depths of 0 to 850 feet; continous coverage  in 10 ft intervals||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0224|38.62805556|-77.02055556|Charles|Maryland|CH Bd 46|Mount Vernon||cuttings||||http://www.mgs.md.gov/publications/report_pages/OFR_12-02-20.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383742077011101&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1127|CH Be 16|25.0|||RSY12|CH Be 16|0.0| 74 envelopes in 3 boxes; spanning depths of 45 to 490 feet; largely continuous coverage mainly in 10 ft intervals||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0225|38.62011831|-76.98830776|Charles|Maryland|CH Be 16|La Plata||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383712076591901&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1128|CH Be 36|25.0|||RSY12|CH Be 36|0.0| 82 envelopes in 6 boxes; spanning depths of 0 to 439 feet; sampling interval and coverage varies.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0226|38.62900714|-76.93552837|Charles|Maryland|CH Be 36|Piscataway||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383744076560901&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1129|CH Be 41|25.0|||RSY12|CH Be 41|0.0| 58 envelopes in 4 boxes; spanning depths of 0 to 580 feet; continuous coverage; samping interval varies.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0227|38.64872876|-76.94052864|Charles|Maryland|CH Be 41|Piscataway||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383855076562701&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1130|CH Be 42|25.0|||RSY12|CH Be 42|0.0| 46 envelopes in 2 boxes; spanning depths of 0 to 518 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0228|38.64872876|-76.94052864|Charles|Maryland|CH Be 42|Piscataway||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383855076562702&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1131|CH Be 48|25.0|||RSY12|CH Be 48|0.0| 33 envelopes in 2 boxes; spanning depths of 1 to 900 feet; sampling intervals vary; some intervals missing.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0229|38.61372983|-76.92941698|Charles|Maryland|CH Be 48|La Plata||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383649076554701&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1132|CH Be 57|25.0|||RSY12|CH Be 57|0.0| 166 envelopes in 12 boxes; spanning depths of 0 to 1813 feet; coverage varies; many missing intervals; samping intervals vary.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0230|38.61777778|-76.96388889|Charles|Maryland|CH Be 57|La Plata||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383706076575601&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1133|CH Be 58|25.0|||RSY12|CH Be 58|0.0| 103 envelopes in 7 boxes; spanning depths of 50 to 1160 feet; coverage varies; a few missing intervals; generally 10 and 20 ft intervals.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0231|38.61783333|-76.964|Charles|Maryland|CH Be 58|La Plata||cuttings||||http://www.mgs.md.gov/publications/report_pages/OFR_12-02-20.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383706076575602&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1134|CH Be 59|25.0|||RSY12|CH Be 59|0.0| 62 envelopes in 5 boxes; spanning depths of 0 to 715 feet; largely continuous coverage; mainly 10 ft intervals.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0232|38.61845178|-76.96525147|Charles|Maryland|CH Be 59|La Plata||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383649076554702&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1135|CH Be 61|25.0|||RSY12|CH Be 61|0.0| 80 envelopes in 5 boxes; spanning depths of 0 to 700 feet; continuous coverage; mainly 5 and 10 ft intervals.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0233|38.64872876|-76.94052864|Charles|Maryland|CH Be 61|Piscataway||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383855076562703&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1136|CH Bf 5|25.0|||RSY12|CH Bf 5|0.0| 119 envelopes in 4 boxes; spanning depths of 0 to 440 feet; largely continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0234|38.65122892|-76.87941569|Charles|Maryland|CH Bf 5|Piscataway||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383904076524702&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1137|CH Bf 15|25.0|||RSY12|CH Bf 15|0.0| 140 envelopes in 6 boxes; spanning depths of 0 to 393 feet; continuous coverage; sampling interval varies||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0235|38.62289631|-76.90913862|Charles|Maryland|CH Bf 15|La Plata||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383722076543402&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1138|CH Bf 127|25.0|||RSY12|CH Bf 127|0.0| 60 envelopes in 2 boxes; spanning depths of 1 to 517 feet; sampling intervals vary; many intervals missing.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0236|38.65372886|-76.87413778|Charles|Maryland|CH Bf 127|Brandywine||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383913076522801&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1139|CH Bf 131|25.0|||RSY12|CH Bf 131|0.0| 39 envelopes in 2 boxes; spanning depths of 0 to 930 feet; sampling intervals vary; many intervals missing.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0237|38.61095221|-76.91080526|Charles|Maryland|CH Bf 131|La Plata||cuttings||||http://www.mgs.md.gov/publications/report_pages/OFR_12-02-20.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383639076544001&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1140|CH Bf 133|25.0|||RSY12|CH Bf 133|0.0| 28 envelopes in 1 box; spanning depths of 250 to 500 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0238|38.611|-76.91591667|Charles|Maryland|CH Bf 133|La Plata||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383640076545901&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1141|CH Bf 134|25.0|||RSY12|CH Bf 134|0.0| 53 envelopes in 3 boxes; spanning depths of 0 to 547 feet; sampling generally 10 ft intervals; several intervals missing.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0239|38.62500039|-76.88774918|Charles|Maryland|CH Bf 134|Piscataway||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_76.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383728076531701&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1142|CH Bf 141|25.0|||RSY12|CH Bf 141|0.0| 70 envelopes in 3 boxes; spanning depths of 0 to 662 feet; sampling intervals vary; many intervals missing.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0240|38.63872945|-76.8366365|Charles|Maryland|CH Bf 141|Brandywine||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383819076501302&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1143|CH Bf 142|25.0|||RSY12|CH Bf 142|0.0| 58 envelopes in 3 boxes; spanning depths of 0 to 570 feet; continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0241|38.62484077|-76.88830465|Charles|Maryland|CH Bf 142|La Plata||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383732076531901&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1144|CH Bf 144|25.0|||RSY12|CH Bf 144|0.0| 176 envelopes in 11 boxes; spanning depths of 0 to 1967 feet; samples mainly in 10 ft intervals; some missing intervals.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0242|38.65372896|-76.85024816|Charles|Maryland|CH Bf 144|Brandywine||cuttings||||http://www.mgs.md.gov/reports/RI_44.pdf|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383913076510201&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1145|CH Bf 145|25.0|||RSY12|CH Bf 145|0.0| 76 envelopes in 5 boxes; spanning depths of 0 to 750 feet; continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0243|38.59956378|-76.87885971|Charles|Maryland|CH Bf 145|La Plata||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383558076524501&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1146|CH Bf 146|25.0|||RSY12|CH Bf 146|0.0| 203 envelopes in 15 boxes; spanning depths of 0 to 1650 feet; largely continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0244|38.58588889|-76.90083333|Charles|Maryland|CH Bf 146|La Plata||cuttings||||http://www.mgs.md.gov/output/reports/OFR/OFR_86-02-2.pdf|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383508076540701&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1147|CH Bf 150|25.0|||RSY12|CH Bf 150|0.0| 128 envelopes in 11 boxes; spanning depths of 220 to 1350 feet; largely continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0245|38.65036111|-76.87811111|Charles|Maryland|CH Bf 150|Piscataway||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383901076524301&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1148|CH Bf 151|25.0|||RSY12|CH Bf 151|0.0| 58 envelopes in 5 boxes; spanning depths of 0 to 700 feet; sampling intervals vary; many intervals missing.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0246|38.58583333|-76.901|Charles|Maryland|CH Bf 151|La Plata||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383508076540703&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1149|CH Bf 157|25.0|||RSY12|CH Bf 157|0.0| 44 envelopes in 3 boxes; spanning depths of 0 to 635 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0247|38.61091667|-76.91611111|Charles|Maryland|CH Bf 157|La Plata||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_76.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383637076545803&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1150|CH Bf 158|25.0|||RSY12|CH Bf 158|0.0| 43 envelopes in 2 boxes; spanning depths of 0 to 800 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0248|38.62563889|-76.88819444|Charles|Maryland|CH Bf 158|Piscataway||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383732076531902&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1151|CH Cb 8|25.0|||RSY12|CH Cb 8|0.0| 57 envelopes in 3 boxes; spanning depths of 0 to 620 feet; sampling mainly in 10 ft intervals; many intervals missing.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0249|38.57678588|-77.2010913|Charles|Maryland|CH Cb 8|Indian Head||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_76.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383436077120501&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1152|CH Cb 9|25.0|||RSY12|CH Cb 9|0.0| 65 envelopes in 4 boxes; spanning depths of 0 to 621 feet; continuous coverage, mainly in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0250|38.56456403|-77.20414679|Charles|Maryland|CH Cb 9|Indian Head||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_76.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383354077121501&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1153|CH Cb 26|25.0|||RSY12|CH Cb 26|0.0| 62 envelopes in 3 boxes; spanning depths of 0 to 600 feet; continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0251|38.55428653|-77.22164714|Charles|Maryland|CH Cb 26|Indian Head||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383315077131901&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1154|CH Cb 27|25.0|||RSY12|CH Cb 27|0.0| 43 envelopes in 3 boxes; spanning depths of 0 to 300 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0252|38.5545643|-77.22025822|Charles|Maryland|CH Cb 27|Indian Head||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383316077131401&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1155|CH Cc 5|25.0|||RSY12|CH Cc 5|0.0| 37 envelopes in 2 boxes; spanning depths of 18 to 215 feet; largely continuous coverage in 7 and 10 ft intervals.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0253|38.54984242|-77.08358786|Charles|Maryland|CH Cc 5|Port Tobacco||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_76.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383259077050202&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1156|CH Cc 21|25.0|||RSY12|CH Cc 21|0.0| 67 envelopes in 4 boxes; spanning depths of 0 to 680 feet; continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0254|38.56206428|-77.08331016|Charles|Maryland|CH Cc 21|Port Tobacco||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383343077050101&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1157|CH Cc 22|25.0|||RSY12|CH Cc 22|0.0| 7 envelopes in 1 box; spanning depths of 0 to 43 feet; continuous coverage in 5 to 8 ft intervals.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0255|38.55373113|-77.1283113|Charles|Maryland|CH Cc 22|Indian Head||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383313077075101&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1158|CH Cc 31|25.0|||RSY12|CH Cc 31|0.0| 56 envelopes in 3 boxes; spanning depths of 0 to 560 feet; continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0256|38.58202018|-77.12825099|Charles|Maryland|CH Cc 31|Indian Head||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383455077074401&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1159|CH Cd 8|25.0|||RSY12|CH Cd 8|0.0| 40 envelopes in 2 boxes; spanning depths of 1 to 400 feet; continuous coverage in 9 and 10 ft intervals.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0257|38.55650891|-77.06969864|Charles|Maryland|CH Cd 8|Port Tobacco||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383323077041201&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1160|CH Cd 9|25.0|||RSY12|CH Cd 9|0.0| 42 envelopes in 3 boxes; spanning depths of 0 to 420 feet; continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0258|38.5095659|-77.03830866|Charles|Maryland|CH Cd 9|Port Tobacco||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_76.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383037077021401&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1161|CH Ce 8|25.0|||RSY12|CH Ce 8|0.0| 164 envelopes in 6 boxes; spanning depths of 0 to 1076 feet; sampling intervals vary; two intervals missing.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0259|38.53206541|-76.96886227|Charles|Maryland|CH Ce 8|La Plata||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_69.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383155076580901&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1162|CH Ce 15|25.0|||RSY12|CH Ce 15|0.0| 82 envelopes in 3 boxes; spanning depths of 0 to 410 feet; continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0260|38.54734268|-76.98608515|Charles|Maryland|CH Ce 15|La Plata||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383250076591101&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1163|CH Ce 18|25.0|||RSY12|CH Ce 18|0.0| 114 envelopes in 4 boxes; spanning depths of 0 to 1219 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0261|38.54428736|-76.94886165|Charles|Maryland|CH Ce 18|La Plata||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383239076565701&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1164|CH Ce 34|25.0|||RSY12|CH Ce 34|0.0| 44 envelopes in 3 boxes; spanning depths of 0 to 441 feet; continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0262|38.54762045|-76.98414064|Charles|Maryland|CH Ce 34|La Plata||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383251076590401&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1165|CH Ce 35|25.0|||RSY12|CH Ce 35|0.0| 94 envelopes in 5 boxes; spanning depths of 0 to 1252 feet; largley continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0263|38.52019444|-76.97975|Charles|Maryland|CH Ce 35|La Plata||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_69.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383111076584801&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1166|CH Ce 36|25.0|||RSY12|CH Ce 36|0.0| 31 envelopes in 2 boxes; spanning depths of 400 to 690 feet; continuous coverage in 5 and 10 ft intervals.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0264|38.53234318|-76.96886227|Charles|Maryland|CH Ce 36|La Plata||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383156076580901&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1167|CH Ce 37|25.0|||RSY12|CH Ce 37|0.0| 222 envelopes in 10 boxes; spanning depths of 0 to 2020 feet; sampling mainly in 10 ft intervals; many intervals missing.||WJUNKIN|2021-08-19 16:38:49|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0265|38.54345407|-76.94386147|Charles|Maryland|CH Ce 37|La Plata||cuttings||||http://www.mgs.md.gov/publications/report_pages/OFR_12-02-20.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383236076563901&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1168|CH Ce 38|25.0|||RSY12|CH Ce 38|0.0| 70 envelopes in 3 boxes; spanning depths of 0 to 700 feet; continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0266|38.57650874|-76.92080535|Charles|Maryland|CH Ce 38|La Plata||cuttings||||http://www.mgs.md.gov/publications/report_pages/OFR_2000-02-12.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383435076551601&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1169|CH Ce 51|25.0|||RSY12|CH Ce 51|0.0| 132 envelopes in 9 boxes; spanning depths of 70 to 1500 feet; largely continuous coverage mainly in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0267|38.51984362|-76.95163939|Charles|Maryland|CH Ce 51|La Plata||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_69.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383111076570701&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1170|CH Cf 9|25.0|||RSY12|CH Cf 9|0.0| 52 envelopes in 2 boxes; spanning depths of 0 to 679.5 feet; sampling intervals vary; two missing itnervals||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0268|38.53901018|-76.83635776|Charles|Maryland|CH Cf 9|Hughesville||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383220076501201&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1171|CH Cg 1|25.0|||RSY12|CH Cg 1|0.0| 233 envelopes in 9 boxes; spanning depths of 0 to 546 feet; largely continuous coverage; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0269|38.53345499|-76.78580041|Charles|Maryland|CH Cg 1|Hughesville||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383200076471001&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1172|CH Cg 18|25.0|||RSY12|CH Cg 18|0.0| 102 envelopes in 5 boxes; spanning depths of 0 to 1030 feet; largely continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0270|38.52234434|-76.75357694|Charles|Maryland|CH Cg 18|Hughesville||cuttings||||http://www.mgs.md.gov/publications/report_pages/OFR_2000-02-12.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383120076451401&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1173|CH Da 1|25.0|||RSY12|CH Da 1|0.0| 36 envelopes in 2 boxes; spanning depths of 0 to 210 feet; continuous coverage; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0271|38.45595615|-77.26414719|Charles|Maryland|CH Da 1|Widewater||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=382721077155201&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1174|CH Db 10|25.0|||RSY12|CH Db 10|0.0| 21 envelopes in 1 box; spanning depths of 1 to 215 feet; largely continous coverage in 9 to 10 ft intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0272|38.45762276|-77.18081191|Charles|Maryland|CH Db 10|Nanjemoy||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=382727077105201&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1175|CH Dc 16|25.0|||RSY12|CH Dc 16|0.0| 40 envelopes in 3 boxes; spanning depths of 0 to 400 feet; continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0273|38.47123358|-77.1241439|Charles|Maryland|CH Dc 16|Mathias Point||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=382816077072801&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1176|CH Dc 20|25.0|||RSY12|CH Dc 20|0.0| 35 envelopes in 2 boxes; spanning depths of 0 to 350 feet; largely continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0274|38.45762288|-77.11636586|Charles|Maryland|CH Dc 20|Mathias Point||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=382727077070001&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1177|CH Dc 21|25.0|||RSY12|CH Dc 21|0.0| 27 envelopes in 2 boxes; spanning depths of 0 to 274 feet; largely continuous coverage mainly in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0275|38.45095641|-77.11469912|Charles|Maryland|CH Dc 21|Mathias Point||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=382703077065401&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1178|CH Dd 9|25.0|||RSY12|CH Dd 9|0.0| 40 envelopes in 2 boxes; spanning depths of 0 to 249 feet; continuous coverate; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0276|38.45484535|-77.02469689|Charles|Maryland|CH Dd 9|Mathias Point||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=382717077013001&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1179|CH Dd 10|25.0|||RSY12|CH Dd 10|0.0| 81 envelopes in 3 boxes; spanning depths of 0 to 404 feet; 2 sets, continous coverage in 10 ft intervals||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0277|38.45317875|-77.01302992|Charles|Maryland|CH Dd 10|Mathias Point||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=382711077004801&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1180|CH Dd 20|25.0|||RSY12|CH Dd 20|0.0| 104 envelopes in 6 boxes; spanning depths of 0 to 518.67 feet; continuous coverage in 5 ft intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0278|38.48012231|-77.05664228|Charles|Maryland|CH Dd 20|Mathias Point||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=382848077032501&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1181|CH De 1|25.0|||RSY12|CH De 1|0.0| 114 envelopes in 3 boxes; spanning depths of 0 to 521 feet; sampling intervals vary; two intervals missing||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0279|38.49067769|-76.98497375|Charles|Maryland|CH De 1|Popes Creek||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=382926076590701&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1182|CH De 4|25.0|||RSY12|CH De 4|0.0| 33 envelopes in 1 box; spanning depths of 0 to 415 feet; continuous coverage; samping intervals vary.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0280|38.42512416|-76.97219521|Charles|Maryland|CH De 4|Popes Creek||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=382530076582101&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1183|CH De 27|25.0|||RSY12|CH De 27|0.0| 41 envelopes in 2 boxes; spanning depths of 0 to 793 feet; samping intervals vary; one interval missing||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0281|38.48401127|-76.97386221|Charles|Maryland|CH De 27|Popes Creek||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=382902076582701&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1184|CH Eb 3|25.0|||RSY12|CH Eb 3|0.0| 20 envelopes in 1 box; spanning depths of 1 to 97 feet; continuous coverage; samping intervals vary.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0282|38.36179206|-77.20970108|Charles|Maryland|CH Eb 3|King George||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=382142077123601&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1185|CH Ec 5|25.0|||RSY12|CH Ec 5|0.0| 66 envelopes in 2 boxes; spanning depths of 0 to 324 feet; 2 sets, largely continuous coverage in 10 ft intervals||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0283|38.41095747|-77.16136675|Charles|Maryland|CH Ec 5|Nanjemoy||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=382439077094201&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1186|CH Ee 39|25.0|||RSY12|CH Ee 39|0.0| 72 envelopes in 2 boxes; spanning depths of 0 to 310 feet; continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0284|38.34901543|-76.92774916|Charles|Maryland|CH Ee 39|Colonial Beach North||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=382056076554101&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1187|CH Ee 40|25.0|||RSY12|CH Ee 40|0.0| 17 envelopes in 1 box; spanning depths of 0 to 346 feet; continuous coverage; samping intervals vary.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0285|38.3801255|-76.98469536|Charles|Maryland|CH Ee 40|Popes Creek||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=382248076590601&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1188|CH Ee 43|25.0|||RSY12|CH Ee 43|0.0| 22 envelopes in 1 box; spanning depths of 0 to 236 feet; continuous coverage; samping intervals vary.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0286|38.33790463|-76.93747162|Charles|Maryland|CH Ee 43|Colonial Beach North||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=382016076561602&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1189|CH Ee 44|25.0|||RSY12|CH Ee 44|0.0| 50 envelopes in 2 boxes; spanning depths of 0 to 293 feet; continuous coverage; samping intervals vary.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0287|38.3962362|-76.95052775|Charles|Maryland|CH Ee 44|Popes Creek||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=382346076570301&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1190|CH Ee 56|25.0|||RSY12|CH Ee 56|0.0| 49 envelopes in 3 boxes; spanning depths of 0 to 504 feet; largely continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0288|38.40595812|-76.95386122|Charles|Maryland|CH Ee 56|Popes Creek||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=382421076571501&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1191|CH Ee 59|25.0|||RSY12|CH Ee 59|0.0| 21 envelopes in 1 box; spanning depths of 0 to 335 feet; largely continuous coverage; samping intervals vary.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0289|38.37790341|-76.95386111|Charles|Maryland|CH Ee 59|Popes Creek||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=382240076571501&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1192|CH Ee 68|25.0|||RSY12|CH Ee 68|0.0| 116 envelopes in 7 boxes; spanning depths of 0 to 1152 feet; continuous coverage in 10 ft intervals||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0290|38.36457044|-76.97275049|Charles|Maryland|CH Ee 68|Colonial Beach North||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_69.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=382152076582301&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1193|CH Ee 74|25.0|||RSY12|CH Ee 74|0.0| 60 envelopes in 3 boxes; spanning depths of 0 to 600 feet; continuous coverage in 10 ft intervals||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0291|38.3609595|-76.94024955|Charles|Maryland|CH Ee 74|Colonial Beach North||cuttings||||http://www.mgs.md.gov/publications/report_pages/OFR_2000-02-12.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=382139076562601&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1194|CH Ee 91|25.0|||RSY12|CH Ee 91|0.0| 45 envelopes in 4 boxes; spanning depths of 0 to 1214 feet; largely continuous coverage; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0292|38.37734781|-76.98108413|Charles|Maryland|CH Ee 91|Popes Creek||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_69.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=382238076585301&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1195|CH Ef 4|25.0|||RSY12|CH Ef 4|0.0| 72 envelopes in 3 boxes; spanning depths of 1 to 330 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0293|38.36318178|-76.87635884|Charles|Maryland|CH Ef 4|Colonial Beach North||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=382147076523601&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1196|CH Ef 9|25.0|||RSY12|CH Ef 9|0.0| 78 envelopes in 2 boxes; spanning depths of 0 to 390 feet; continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0294|38.3951253|-76.88080341|Charles|Maryland|CH Ef 9|Popes Creek||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=382342076525201&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1197|CH Fe 5|25.0|||RSY12|CH Fe 5|0.0| 89 envelopes in 6 boxes; spanning depths of 0 to 900 feet; largely continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0295|38.30133333|-76.91780556|Charles|Maryland|CH Fe 5|Colonial Beach North||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_76.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=381803076550801&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1198|CH Ff 13|25.0|||RSY12|CH Ff 13|0.0| 54 envelopes in 2 boxes; spanning depths of 0 to 277.25 feet; 2 sets; continuous coverage in roughly 10 ft intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0296|38.26374022|-76.84108025|Charles|Maryland|CH Ff 13|Rock Point||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=381549076502901&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1199|CH Ff 14|25.0|||RSY12|CH Ff 14|0.0| 54 envelopes in 2 boxes; spanning depths of 0 to 266 feet; continuous coverage roughly 10 ft intervals||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0297|38.26374022|-76.84108025|Charles|Maryland|CH Ff 14|Rock Point||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=381549076502902&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1200|CH Ff 20|25.0|||RSY12|CH Ff 20|0.0| 43 envelopes in 1 box; spanning depths of 0 to 275 feet; sampling intervals vary; missing intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0298|38.26457352|-76.85469168|Charles|Maryland|CH Ff 20|Rock Point||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=381552076511801&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1201|CH Ff 21|25.0|||RSY12|CH Ff 21|0.0| 46 envelopes in 2 boxes; spanning depths of 0 to 272 feet; continuous coverage; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0299|38.27651761|-76.88302568|Charles|Maryland|CH Ff 21|Colonial Beach North||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=381635076530001&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1202|CH Ff 26|25.0|||RSY12|CH Ff 26|0.0| 54 envelopes in 2 boxes; spanning depths of 0 to 272 feet; continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0300|38.31873862|-76.87441435|Charles|Maryland|CH Ff 26|Rock Point||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=381907076522901&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1203|CH Ff 36|25.0|||RSY12|CH Ff 36|0.0| 52 envelopes in 2 boxes; spanning depths of 0 to 260 feet; 2 sets; continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0301|38.27568433|-76.845247|Charles|Maryland|CH Ff 36|Rock Point||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=381632076504401&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1204|CH Ff 40|25.0|||RSY12|CH Ff 40|0.0| 54 envelopes in 2 boxes; spanning depths of 0 to 267 feet; 2 sets; sampling intervals vary; two intervals missing||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0302|38.32457174|-76.90635965|Charles|Maryland|CH Ff 40|Colonial Beach North||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=381928076542401&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1205|CH Ff 48|25.0|||RSY12|CH Ff 48|0.0| 43 envelopes in 2 boxes; spanning depths of 0 to 265 feet; continuous coverage; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0303|38.25818482|-76.84913601|Charles|Maryland|CH Ff 48|Rock Point||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=381529076505801&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1206|CL Ad 47|25.0|||RSY12|CL Ad 47|0.0| 23 envelopes in 1 box; spanning depths of 200 to 310 feet; continuous coverage in 5 ft intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0304|39.66898968|-77.01525958|Carroll|Maryland|CL Ad 47|Littlestown||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_12.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=394008077005601&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1207|CL Af 91|25.0|||RSY12|CL Af 91|0.0| 43 envelopes in 2 boxes; spanning depths of 0 to 215 feet; continuous coverage in 5 ft intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:43:21|DAS02|WP0305|39.67629167|-76.84467222|Carroll|Maryland|CL Af 91|Lineboro||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_12.html|||||||||||||||||||||||||||||||||||||||
1208|CL Bb 38|25.0|||RSY12|CL Bb 38|0.0| 312 envelopes in 6 boxes; spanning depths of 20 to 6205 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:43:21|DAS02|WP0306|39.60565537|-77.23442784|Carroll|Maryland|CL Bb 38|Union Bridge||cuttings|||||||||||||||||||||||||||||||||||||||||||
1209|CL Bc 16|25.0|||RSY12|CL Bc 16|0.0| 52 envelopes in 2 boxes; spanning depths of 275 to 535 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0307|39.63287804|-77.11248264|Carroll|Maryland|CL Bc 16|Littlestown||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_12.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=393754077064601&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1210|CL Bc 171|25.0|||RSY12|CL Bc 171|0.0| 56 envelopes in 2 boxes; spanning depths of 0 to 280 feet; continuous coverage in 5 ft intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0308|39.59954482|-77.14498267|Carroll|Maryland|CL Bc 171|Union Bridge||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_12.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=393558077084301&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1211|CL Bf 27|25.0|||RSY12|CL Bf 27|0.0| 34 envelopes in 2 boxes; spanning depths of 0 to 100 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:43:21|DAS02|WP0309|39.59410833|-76.85020556|Carroll|Maryland|CL Bf 27|Hampstead||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_12.html|||||||||||||||||||||||||||||||||||||||
1212|CL Bf 28|25.0|||RSY12|CL Bf 28|0.0| 11 envelopes in 1 box; spanning depths of 0 to 37 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:43:21|DAS02|WP0310|39.59118889|-76.84876111|Carroll|Maryland|CL Bf 28|Hampstead||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_12.html|||||||||||||||||||||||||||||||||||||||
1213|CL Bf 29|25.0|||RSY12|CL Bf 29|0.0| 7 envelopes in 1 box; spanning depths of 120 to 151 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:43:21|DAS02|WP0311|39.59278333|-76.85356667|Carroll|Maryland|CL Bf 29|Hampstead||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_12.html|||||||||||||||||||||||||||||||||||||||
1214|CL Bf 135|25.0|||RSY12|CL Bf 135|0.0| 40 envelopes in 2 boxes; spanning depths of 0 to 200 feet; continuous coverage in 5 ft intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:43:21|DAS02|WP0312|39.66015556|-76.89542222|Carroll|Maryland|CL Bf 135|Manchester||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_12.html|||||||||||||||||||||||||||||||||||||||
1215|CL Bf 164|25.0|||RSY12|CL Bf 164|0.0| 40 envelopes in 2 boxes; spanning depths of 0 to 200 feet; continuous coverage in 5 ft intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:43:21|DAS02|WP0313|39.60283333|-76.84387222|Carroll|Maryland|CL Bf 164|Hampstead||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_12.html|||||||||||||||||||||||||||||||||||||||
1216|CL Bf 178|25.0|||RSY12|CL Bf 178|0.0| 49 envelopes in 2 boxes; spanning depths of 0 to 250 feet; largely continuous coverage in 5 ft intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:43:21|DAS02|WP0314|39.66523889|-76.89210278|Carroll|Maryland|CL Bf 178|Manchester||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_12.html|||||||||||||||||||||||||||||||||||||||
1217|CL Bf 184|25.0|||RSY12|CL Bf 184|0.0| 44 envelopes in 2 boxes; spanning depths of 0 to 340 feet; continuous coverage in 5 ft intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0315|39.63176952|-76.85636636|Carroll|Maryland|CL Bf 184|Lineboro||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_12.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=393754076512401&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1218|CL Ce 3|25.0|||RSY12|CL Ce 3|0.0| 132 envelopes in 5 boxes; spanning depths of 0 to 840 feet; missing 0 to 185 ft; continuous in 5 ft intervals below.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:43:21|DAS02|WP0316|39.57885036|-76.9927007|Carroll|Maryland|CL Ce 3|Westminister||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_79.html|||||||||||||||||||||||||||||||||||||||
1219|CL Dd 16|25.0|||RSY12|CL Dd 16|0.0| 10 envelopes in 1 box; spanning depths of 10 to 102 feet; largley continous coverage in 2 and 10 ft intervals; missing upper 10 ft||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:43:21|DAS02|WP0317|39.42050278|-77.05027222|Carroll|Maryland|CL Dd 16|Winfield||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_12.html|||||||||||||||||||||||||||||||||||||||
1220|CL Df 9|25.0|||RSY12|CL Df 9|0.0| 29 envelopes in 1 box; spanning depths of 0 to 135 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0318|39.45149255|-76.89775612|Carroll|Maryland|CL Df 9|Finksburg||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_12.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=392705076535301&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1221|CL Ec 75|25.0|||RSY12|CL Ec 75|0.0| 45 envelopes in 2 boxes; spanning depths of 0 to 248 feet; sampling intervals vary; many intervals missing.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0319|39.38304778|-77.08953645|Carroll|Maryland|CL Ec 75|Winfield||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_12.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=392259077052401&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1222|CL Ee 29|25.0|||RSY12|CL Ee 29|0.0| 25 envelopes in 1 box; spanning depths of 0 to 156 feet; continuous coverage in 6 ft intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0320|39.3645488|-76.92914443|Carroll|Maryland|CL Ee 29|Sykesville||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_12.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=392152076554602&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1223|CL Ef 15|25.0|||RSY12|CL Ef 15|0.0| 44 envelopes in 2 boxes; spanning depths of 0 to 178.6 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0321|39.37343787|-76.89886608|Carroll|Maryland|CL Ef 15|Sykesville||cuttings||||http://www.mgs.md.gov/publications/report_pages/BDR_12.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=392224076535701&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1224|CO Ad 17|25.0|||RSY12|CO Ad 17|0.0| 8 envelopes in 1 box(es); spanning depths of 0 to 40 feet; missing intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0322|39.13233428|-75.79104473|Caroline|Maryland|CO Ad 17|Sudlersville||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=390756075472901&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1225|CO Ad 18|25.0|||RSY12|CO Ad 18|0.0| 6 envelopes in 1 box(es); spanning depths of 0 to 40 feet; continuous coverage; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0323|39.1387233|-75.75659894|Caroline|Maryland|CO Ad 18|Sudlersville||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=390819075452501&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1226|CO Bc 16|25.0|||RSY12|CO Bc 16|0.0| 21 envelopes in 4 box(es); spanning depths of 10 to 685 feet; missing intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0324|39.00289093|-75.88326958|Caroline|Maryland|CO Bc 16|Price||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=390010075531101&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1227|CO Bd 18|25.0|||RSY12|CO Bd 18|0.0| 39 envelopes in 1 box; spanning depths of 0 to 390 feet; samples generally in 10 ft intervals ; several intervals missing.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0325|39.03372444|-75.78743292|Caroline|Maryland|CO Bd 18|Goldsboro||cuttings||||http://www.mgs.md.gov/publications/report_pages/BULL_18.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=390201075471601&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1228|CO Bd 53|25.0|||RSY12|CO Bd 53|0.0| 32 envelopes in 2 box(es); spanning depths of 0 to 320 feet; continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0326|39.04066667|-75.78322222|Caroline|Maryland|CO Bd 53|Goldsboro||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=390227075470201&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1229|CO Cc 2|25.0|||RSY12|CO Cc 2|0.0| 24 envelopes in 1 box; spanning depths of 0 to 350 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:43:21|DAS02|WP0327|38.94481944|-75.89089444|Caroline|Maryland|CO Cc 2|Ridgely||cuttings||||http://www.mgs.md.gov/publications/report_pages/BULL_18.html|||||||||||||||||||||||||||||||||||||||
1230|CO Cc 54|25.0|||RSY12|CO Cc 54|0.0| 28 envelopes in 2 box(es); spanning depths of 0 to 125 feet; continuous coverage in 5 ft intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0328|38.92066916|-75.86715768|Caroline|Maryland|CO Cc 54|Denton||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385514075520301&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1231|CO Cc 60|25.0|||RSY12|CO Cc 60|0.0| 10 envelopes in 1 box(es); spanning depths of 0 to 52 feet; missing intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0329|38.91816896|-75.99771752|Caroline|Maryland|CO Cc 60|Ridgely||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385505075595301&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1232|CO Cc 61|25.0|||RSY12|CO Cc 61|0.0| 38 envelopes in 2 box(es); spanning depths of 0 to 80 feet; missing intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0330|38.93388889|-75.90388889|Caroline|Maryland|CO Cc 61|Ridgely||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385500075541201&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1233|CO Cc 63|25.0|||RSY12|CO Cc 63|0.0| 13 envelopes in 1 box(es); spanning depths of 0 to 77 feet; continuous coverage; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0331|38.93483571|-75.89410306|Caroline|Maryland|CO Cc 63|Ridgely||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385605075534001&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1234|CO Cc 64|25.0|||RSY12|CO Cc 64|0.0| 12 envelopes in 1 box(es); spanning depths of 0 to 90 feet; missing intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0332|38.93055556|-75.90777778|Caroline|Maryland|CO Cc 64|Ridgely||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385949075543001&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1235|CO Cc 65|25.0|||RSY12|CO Cc 65|0.0| 14 envelopes in 1 box(es); spanning depths of 0 to 42 feet; missing intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0333|38.95372462|-75.85604626|Caroline|Maryland|CO Cc 65|Denton||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385713075512301&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1236|CO Cc 66|25.0|||RSY12|CO Cc 66|0.0| 15 envelopes in 1 box(es); spanning depths of 0 to 75 feet; continuous coverage in 5 ft intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0334|38.96983555|-75.88632513|Caroline|Maryland|CO Cc 66|Ridgely||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385811075531201&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1237|CO Cc 67|25.0|||RSY12|CO Cc 67|0.0| 16 envelopes in 1 box(es); spanning depths of 0 to 80 feet; continuous coverage in 5 ft intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0335|38.97039105|-75.89799221|Caroline|Maryland|CO Cc 67|Ridgely||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=390000075535401&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1238|CO Cc 68|25.0|||RSY12|CO Cc 68|0.0| 15 envelopes in 1 box(es); spanning depths of 0 to 75 feet; continuous coverage in 5 ft intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0336|38.97927989|-75.89799224|Caroline|Maryland|CO Cc 68|Ridgely||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385845075535401&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1239|CO Cc 69|25.0|||RSY12|CO Cc 69|0.0| 17 envelopes in 1 box(es); spanning depths of 0 to 85 feet; continuous coverage in 5 ft intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0337|38.96427997|-75.89910334|Caroline|Maryland|CO Cc 69|Ridgely||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385751075535801&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1240|CO Cc 70|25.0|||RSY12|CO Cc 70|0.0| 14 envelopes in 1 box(es); spanning depths of 0 to 70 feet; continuous coverage in 5 ft intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0338|38.96677995|-75.89910335|Caroline|Maryland|CO Cc 70|Ridgely||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385800075535801&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1241|CO Cc 71|25.0|||RSY12|CO Cc 71|0.0| 15 envelopes in 1 box(es); spanning depths of 0 to 75 feet; continuous coverage in 5 ft intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0339|38.96566884|-75.90077007|Caroline|Maryland|CO Cc 71|Ridgely||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385756075540401&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1242|CO Cc 72|25.0|||RSY12|CO Cc 72|0.0| 16 envelopes in 1 box(es); spanning depths of 0 to 80 feet; continuous coverage in 5 ft intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0340|38.96927993|-75.90132566|Caroline|Maryland|CO Cc 72|Ridgely||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385809075540601&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1243|CO Cc 74|25.0|||RSY12|CO Cc 74|0.0| 15 envelopes in 1 box(es); spanning depths of 0 to 75 feet; continuous coverage in 5 ft intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0341|38.97483543|-75.90660364|Caroline|Maryland|CO Cc 74|Ridgely||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385829075542501&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1244|CO Cc 75|25.0|||RSY12|CO Cc 75|0.0| 13 envelopes in 1 box(es); spanning depths of 0 to 65 feet; continuous coverage in 5 ft intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0342|38.9773354|-75.90882596|Caroline|Maryland|CO Cc 75|Ridgely||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385838075543301&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1245|CO Cc 76|25.0|||RSY12|CO Cc 76|0.0| 15 envelopes in 1 box(es); spanning depths of 0 to 80 feet; missing 70-75 ft interval; otherwise continuous coveragein 5 ft intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0343|38.98289091|-75.91077049|Caroline|Maryland|CO Cc 76|Ridgely||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385858075544001&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1246|CO Cc 77|25.0|||RSY12|CO Cc 77|0.0| 12 envelopes in 1 box(es); spanning depths of 0 to 61 feet; continuous coverage in 5 ft intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0344|38.98705757|-75.90799263|Caroline|Maryland|CO Cc 77|Ridgely||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385913075543001&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1247|CO Cc 78|25.0|||RSY12|CO Cc 78|0.0| 12 envelopes in 1 box(es); spanning depths of 0 to 60 feet; continuous coverage in 5 ft intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0345|38.991502|-75.9046592|Caroline|Maryland|CO Cc 78|Ridgely||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385929075541801&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1248|CO Cc 79|25.0|||RSY12|CO Cc 79|0.0| 15 envelopes in 1 box(es); spanning depths of 0 to 75 feet; continuous coverage in 5 ft intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0346|38.98733541|-75.89632555|Caroline|Maryland|CO Cc 79|Ridgely||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385914075534801&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1249|CO Cc 80|25.0|||RSY12|CO Cc 80|0.0| 20 envelopes in 1 box(es); spanning depths of 0 to 100 feet; continuous coverage in 5 ft intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0347|38.97983546|-75.89410322|Caroline|Maryland|CO Cc 80|Ridgely||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385847075534001&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1250|CO Cc 81|25.0|||RSY12|CO Cc 81|0.0| 18 envelopes in 1 box(es); spanning depths of 0 to 90 feet; continuous coverage in 5 ft intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0348|38.97372436|-75.89771444|Caroline|Maryland|CO Cc 81|Ridgely||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385825075535301&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1251|CO Cc 82|25.0|||RSY12|CO Cc 82|0.0| 18 envelopes in 1 box(es); spanning depths of 0 to 90 feet; continuous coverage in 5 ft intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0349|38.97289102|-75.90104788|Caroline|Maryland|CO Cc 82|Ridgely||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385822075540501&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1252|CO Cc 83|25.0|||RSY12|CO Cc 83|0.0| 10 envelopes in 1 box(es); spanning depths of 35 to 84 feet; continuous coverage; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0350|38.94900234|-75.88104711|Caroline|Maryland|CO Cc 83|Ridgely||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385656075525301&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1253|CO Cc 97|25.0|||RSY12|CO Cc 97|0.0| 31 envelopes in 2 box(es); spanning depths of 0 to 416 feet; continuous coverage; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0351|38.94885|-75.88077778|Caroline|Maryland|CO Cc 97|Ridgely||cuttings||||http://www.mgs.md.gov/publications/report_pages/OFR_12-02-20.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385653075525001&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1254|CO Cc 98|25.0|||RSY12|CO Cc 98|0.0| 32 envelopes in 2 box(es); spanning depths of 0 to 395 feet; continuous coverage; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:43:21|DAS02|WP0352|38.94571667|-75.87819722|Caroline|Maryland|CO Cc 98|Ridgely||cuttings|||||||||||||||||||||||||||||||||||||||||||
1255|CO Cc 99|25.0|||RSY12|CO Cc 99|0.0| 25 envelopes in 2 box(es); spanning depths of 0 to 395 feet; continuous coverage; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:43:21|DAS02|WP0353|38.94173611|-75.87409722|Caroline|Maryland|CO Cc 99|Denton||cuttings|||||||||||||||||||||||||||||||||||||||||||
1256|CO Cd 55|25.0|||RSY12|CO Cd 55|0.0| 7 envelopes in 1 box(es); spanning depths of 0 to 25 feet; missing 0-4 ft interval.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0354|38.96344697|-75.81493374|Caroline|Maryland|CO Cd 55|Denton||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385748075485501&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1257|CO Cd 56|25.0|||RSY12|CO Cd 56|0.0| 8 envelopes in 1 box(es); spanning depths of 0 to 62 feet; missing intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0355|38.96261384|-75.76354306|Caroline|Maryland|CO Cd 56|Denton||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385745075455001&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1258|CO Ce 8|25.0|||RSY12|CO Ce 8|0.0| 8 envelopes in 1 box(es); spanning depths of 8 to 67 feet; missing intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0356|38.95650272|-75.73326423|Caroline|Maryland|CO Ce 8|Burrsville||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385723075440101&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1259|CO Ce 9|25.0|||RSY12|CO Ce 9|0.0| 5 envelopes in 1 box(es); spanning depths of 0 to 10 feet; continuous coverage.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0357|38.95650272|-75.73326423|Caroline|Maryland|CO Ce 9|Burrsville||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385723075440102&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1260|CO Dc 122|25.0|||RSY12|CO Dc 122|0.0| 180 envelopes in 8 boxes; spanning depths of 5 to 976.6 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:43:21|DAS02|WP0358|38.88511375|-75.84162902|Caroline|Maryland|CO Dc 122|Denton||cuttings|||||||||||||||||||||||||||||||||||||||||||
1261|CO Dc 131|25.0|||RSY12|CO Dc 131|0.0| 53 envelopes in 2 boxes; spanning depths of 0 to 516 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:43:21|DAS02|WP0359|38.88457778|-75.84051389|Caroline|Maryland|CO Dc 131|Denton||cuttings|||||||||||||||||||||||||||||||||||||||||||
1262|CO Dc 135|25.0|||RSY12|CO Dc 135|0.0| 12 envelopes in 1 box(es); spanning depths of 0 to 50 feet; missing intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0360|38.93511355|-75.86854665|Caroline|Maryland|CO Dc 135|Denton||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385606075520801&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1263|CO Dc 136|25.0|||RSY12|CO Dc 136|0.0| 14 envelopes in 1 box(es); spanning depths of 0 to 77 feet; missing 62-70 ft interval.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0361|38.91511359|-75.89521414|Caroline|Maryland|CO Dc 136|Ridgely||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385454075534401&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1264|CO Dc 137|25.0|||RSY12|CO Dc 137|0.0| 10 envelopes in 1 box(es); spanning depths of 0 to 62 feet; missing 50-60 ft interval.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0362|38.84400285|-75.88632474|Caroline|Maryland|CO Dc 137|Fowling Creek||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385038075531201&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1265|CO Dc 138|25.0|||RSY12|CO Dc 138|0.0| 8 envelopes in 1 box(es); spanning depths of 0 to 32 feet; missing 23-30 ft intervai.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0363|38.88233599|-75.84993483|Caroline|Maryland|CO Dc 138|Denton||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385256075510101&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1266|CO Dd 46|25.0|||RSY12|CO Dd 46|0.0| 61 envelopes in 3 box(es); spanning depths of 0 to 435 feet; missing some intervals between 240 and 340 feet.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0364|38.87678044|-75.82493405|Caroline|Maryland|CO Dd 46|Denton||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385236075493101&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1267|CO Dd 47|25.0|||RSY12|CO Dd 47|0.0| 38 envelopes in 2 box(es); spanning depths of 0 to 380 feet; continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0365|38.87150266|-75.81798939|Caroline|Maryland|CO Dd 47|Hobbs||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385217075490601&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1268|CO Dd 48|25.0|||RSY12|CO Dd 48|0.0| 11 envelopes in 1 box(es); spanning depths of 0 to 62 feet; nearly continuous coverage.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0366|38.88122487|-75.82104504|Caroline|Maryland|CO Dd 48|Denton||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385252075491701&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1269|CO Dd 49|25.0|||RSY12|CO Dd 49|0.0| 12 envelopes in 1 box(es); spanning depths of 0 to 45 feet; missing intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0367|38.85122491|-75.81521153|Caroline|Maryland|CO Dd 49|Hobbs||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385104075485601&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1270|CO Dd 50|25.0|||RSY12|CO Dd 50|0.0| 15 envelopes in 1 box(es); spanning depths of 0 to 47 feet; missing intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0368|38.83844708|-75.78548843|Caroline|Maryland|CO Dd 50|Hobbs||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=385018075470901&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1271|CO Ec 14|25.0|||RSY12|CO Ec 14|0.0| 24 envelopes in 2 boxes; spanning depths of 0 to 120 feet; largley continuous coverage in 5 ft intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0369|38.83178061|-75.85465712|Caroline|Maryland|CO Ec 14|Hobbs||cuttings||||http://www.mgs.md.gov/publications/report_pages/BULL_18.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=384954075511801&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1272|CO Ec 17|25.0|||RSY12|CO Ec 17|0.0| 12 envelopes in 1 box; spanning depths of 0 to 75 feet; sampling intervals vary; one 12 to 20 ft interval.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0370|38.7626143|-75.87437973|Caroline|Maryland|CO Ec 17|Hobbs||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=384545075522901&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1273|CO Ec 18|25.0|||RSY12|CO Ec 18|0.0| 8 envelopes in 1 box; spanning depths of 0 to 44 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0371|38.76872521|-75.84410118|Caroline|Maryland|CO Ec 18|Hobbs||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=384607075504001&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1274|CO Ec 19|25.0|||RSY12|CO Ec 19|0.0| 11 envelopes in 1 box; spanning depths of 0 to 77 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0372|38.76316983|-75.8693796|Caroline|Maryland|CO Ec 19|Hobbs||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=384547075521101&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1275|CO Ec 20|25.0|||RSY12|CO Ec 20|0.0| 16 envelopes in 1 box; spanning depths of 1 to 100 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0373|38.76566984|-75.87271303|Caroline|Maryland|CO Ec 20|Hobbs||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=384556075522301&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1276|CO Ec 24|25.0|||RSY12|CO Ec 24|0.0| 10 envelopes in 1 box; spanning depths of 0 to 52 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0374|38.79066972|-75.8707686|Caroline|Maryland|CO Ec 24|Hobbs||cuttings||||http://www.mgs.md.gov/publications/report_pages/OFR_12-02-20.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=384726075521601&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1277|CO Ed 26|25.0|||RSY12|CO Ed 26|0.0| 8 envelopes in 1 box; spanning depths of 0 to 60 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0375|38.76761396|-75.82048945|Caroline|Maryland|CO Ed 26|Hobbs||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=384603075491501&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1278|CO Ed 27|25.0|||RSY12|CO Ed 27|0.0| 13 envelopes in 1 box; spanning depths of 0 to 62 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0376|38.82816925|-75.76521008|Caroline|Maryland|CO Ed 27|Hobbs||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=384941075455601&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1279|CO Ed 28|25.0|||RSY12|CO Ed 28|0.0| 15 envelopes in 1 box; spanning depths of 0 to 60 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0377|38.81761363|-75.75048747|Caroline|Maryland|CO Ed 28|Hobbs||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=384903075450301&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1280|CO Ee 17|25.0|||RSY12|CO Ee 17|0.0| 18 envelopes in 1 box; spanning depths of 0 to 67 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0378|38.80483581|-75.73465362|Caroline|Maryland|CO Ee 17|Hickman||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=384817075440601&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1281|CO Ee 18|25.0|||RSY12|CO Ee 18|0.0| 12 envelopes in 1 box; spanning depths of 0 to 82 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0379|38.80261358|-75.72354212|Caroline|Maryland|CO Ee 18|Hickman||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=384809075432601&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1282|CO Ee 19|25.0|||RSY12|CO Ee 19|0.0| 9 envelopes in 1 box; spanning depths of 0 to 82 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0380|38.79928025|-75.72104205|Caroline|Maryland|CO Ee 19|Hickman||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=384757075431701&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1283|CO Fb 2|25.0|||RSY12|CO Fb 2|0.0| 12 envelopes in 1 box; spanning depths of 0 to 230 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:43:21|DAS02|WP0381|38.696325|-75.92050556|Caroline|Maryland|CO Fb 2|Preston||cuttings||||http://www.mgs.md.gov/publications/report_pages/BULL_18.html|||||||||||||||||||||||||||||||||||||||
1284|CO Fc 1|25.0|||RSY12|CO Fc 1|0.0| 54 envelopes in 2 boxes; spanning depths of 0 to 270 feet; continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:43:21|DAS02|WP0382|38.70013333|-75.86183333|Caroline|Maryland|CO Fc 1|Federalsburg||cuttings||||http://www.mgs.md.gov/publications/report_pages/BULL_18.html|||||||||||||||||||||||||||||||||||||||
1285|CO Fc 29|25.0|||RSY12|CO Fc 29|0.0| 51 envelopes in 2 boxes; spanning depths of 0 to 520 feet; largley continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0383|38.70455958|-75.9029915|Caroline|Maryland|CO Fc 29|Preston||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=384216075541201&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1286|CO Fd 5|25.0|||RSY12|CO Fd 5|0.0| 31 envelopes in 2 boxes; spanning depths of 0 to 300 feet; continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:43:21|DAS02|WP0384|38.69552778|-75.76435833|Caroline|Maryland|CO Fd 5|Federalsburg||cuttings||||http://www.mgs.md.gov/publications/report_pages/BULL_18.html|||||||||||||||||||||||||||||||||||||||
1287|CO Fd 36|25.0|||RSY12|CO Fd 36|0.0| 31 envelopes in 2 boxes; spanning depths of 0 to 155 feet; continuous coverage in 5 ft intervals.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0385|38.69928075|-75.76159923|Caroline|Maryland|CO Fd 36|Federalsburg||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=384157075454301&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1288|DO Ag 8|25.0|||RSY12|DO Ag 8|0.0| 4 envelopes in 1 box; spanning depths of 0 to 60 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:50|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0386|38.6742821|-75.89215789|Dorchester|Maryland|DO Ag 8|Preston||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=384027075533301&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1289|DO Ag 9|25.0|||RSY12|DO Ag 9|0.0| 5 envelopes in 1 box; spanning depths of 1 to 15 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0387|38.6670601|-75.90743602|Dorchester|Maryland|DO Ag 9|Preston||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=384001075542801&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1290|DO Ag 10|25.0|||RSY12|DO Ag 10|0.0| 2 envelopes in 1 box; spanning depths of 1 to 9 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0388|38.68150427|-75.89688023|Dorchester|Maryland|DO Ag 10|Preston||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=384053075535001&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1291|DO Ah 6|25.0|||RSY12|DO Ah 6|0.0| 7 envelopes in 1 box; spanning depths of 1 to 80 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0389|38.69233687|-75.82243403|Dorchester|Maryland|DO Ah 6|Federalsburg||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=384132075492201&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1292|DO Bb 1|25.0|||RSY12|DO Bb 1|0.0| 63 envelopes in 3 boxes; spanning depths of 180 to 523 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0390|38.58678718|-76.25827942|Dorchester|Maryland|DO Bb 1|Hudson||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383512076153101&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1293|DO Bb 8|25.0|||RSY12|DO Bb 8|0.0| 17 envelopes in 1 box; spanning depths of 300 to 480 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0391|38.59150934|-76.25550161|Dorchester|Maryland|DO Bb 8|Hudson||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383529076152101&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1294|DO Bc 6|25.0|||RSY12|DO Bc 6|0.0| 104 envelopes in 4 boxes; spanning depths of 0 to 520 feet; 2 sets; continuous coverate in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0392|38.59900878|-76.21077804|Dorchester|Maryland|DO Bc 6|Church Creek||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383556076124001&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1295|DO Bd 4|25.0|||RSY12|DO Bd 4|0.0| 19 envelopes in 1 box; spanning depths of 617 to 1041 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0393|38.59539682|-76.13410887|Dorchester|Maryland|DO Bd 4|Church Creek||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383543076080401&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1296|DO Bd 10|25.0|||RSY12|DO Bd 10|0.0| 33 envelopes in 2 boxes; spanning depths of 0 to 630 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0394|38.60484122|-76.1413314|Dorchester|Maryland|DO Bd 10|Church Creek||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_17.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383617076083001&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1297|DO Bf 36|25.0|||RSY12|DO Bf 36|0.0| 44 envelopes in 3 boxes; spanning depths of 150 to 580 feet; continuous coverage from 150 to 580 ft in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0395|38.59888889|-75.92888889|Dorchester|Maryland|DO Bf 36|East New Market||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383534075565001&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1298|DO Bf 37|25.0|||RSY12|DO Bf 37|0.0| 44 envelopes in 3 boxes; spanning depths of 150 to 590 feet; continuous coverage from 150 to 590 ft in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0396|38.6084501|-75.94577011|Dorchester|Maryland|DO Bf 37|East New Market||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383630075564601&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1299|DO Bg 33|25.0|||RSY12|DO Bg 33|0.0| 11 envelopes in 1 box; spanning depths of 0 to 96 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0397|38.63400455|-75.86271278|Dorchester|Maryland|DO Bg 33|Federalsburg||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_17.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383802075514702&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1300|DO Bg 59|25.0|||RSY12|DO Bg 59|0.0| 33 envelopes in 2 boxes; spanning depths of 0 to 560 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0398|38.61766667|-75.84305556|Dorchester|Maryland|DO Bg 59|Rhodesdale||cuttings||||http://www.mgs.md.gov/publications/report_pages/OFR_12-02-20.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383708075503801&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1301|DO Bg 60|25.0|||RSY12|DO Bg 60|0.0| 23 envelopes in 2 boxes; spanning depths of 0 to 115 feet; continuous coverage in 5 ft intervals.||WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0399|38.59456075|-75.8796576|Dorchester|Maryland|DO Bg 60|East New Market||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383540075524801&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1302|DO Bg 66|25.0|||RSY12|DO Bg 66|0.0| 6 envelopes in 1 box; spanning depths of 1 to 45 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0400|38.66233755|-75.86326834|Dorchester|Maryland|DO Bg 66|Federalsburg||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383944075514901&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1303|DO Bg 67|25.0|||RSY12|DO Bg 67|0.0| 4 envelopes in 1 box; spanning depths of 1 to 9 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0401|38.66372686|-75.91438062|Dorchester|Maryland|DO Bg 67|Preston||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383949075545301&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1304|DO Bg 69|25.0|||RSY12|DO Bg 69|0.0| 34 envelopes in 3 boxes; spanning depths of 0 to 175 feet; continuous coverage in 5 ft intervals.||WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0402|38.66567099|-75.88021317|Dorchester|Maryland|DO Bg 69|Preston||cuttings||||http://www.mgs.md.gov/publications/report_pages/OFR_12-02-20.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383956075525001&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1305|DO Bh 9|25.0|||RSY12|DO Bh 9|0.0| 20 envelopes in 1 box; spanning depths of 0 to 100 feet; continuous coverage in 5 ft intervals.||WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0403|38.61955934|-75.7632662|Dorchester|Maryland|DO Bh 9|Rhodesdale||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_17.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383710075454901&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1306|DO Bh 15|25.0|||RSY12|DO Bh 15|0.0| 12 envelopes in 1 box; spanning depths of 0 to 70 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0404|38.61761489|-75.76048837|Dorchester|Maryland|DO Bh 15|Rhodesdale||cuttings||||http://www.mgs.md.gov/publications/report_pages/OFR_12-02-20.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383703075453901&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1307|DO Cb 2|25.0|||RSY12|DO Cb 2|0.0| 46 envelopes in 2 boxes; spanning depths of 0 to 470 feet; largely continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:21|DAS02|WP0405|38.5705|-76.28774444|Dorchester|Maryland|DO Cb 2|Hudson||cuttings|||||||||||||||||||||||||||||||||||||||||||
1308|DO Cc 10|25.0|||RSY12|DO Cc 10|0.0| 69 envelopes in 2 boxes; spanning depths of 10 to 370 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0406|38.50400964|-76.17910954|Dorchester|Maryland|DO Cc 10|Church Creek||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383014076104601&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1309|DO Cd 5|25.0|||RSY12|DO Cd 5|0.0| 38 envelopes in 1 box; spanning depths of 0 to 380 feet; continuous coverage in 5 ft intervals.||WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:21|DAS02|WP0407|38.57399444|-76.14792222|Dorchester|Maryland|DO Cd 5|Church Creek||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_17.html|||||||||||||||||||||||||||||||||||||||
1310|DO Ce 1|25.0|||RSY12|DO Ce 1|0.0| 125 envelopes in 4 boxes; spanning depths of 13 to 965.9 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0408|38.5626188|-76.07438454|Dorchester|Maryland|DO Ce 1|Cambridge||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_17.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383345076042901&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1311|DO Ce 3|25.0|||RSY12|DO Ce 3|0.0| 214 envelopes in 8 boxes; spanning depths of 20 to 977 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0409|38.56484092|-76.06799546|Dorchester|Maryland|DO Ce 3|Cambridge||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383353076040602&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1312|DO Ce 60|25.0|||RSY12|DO Ce 60|0.0| 27 envelopes in 1 box; spanning depths of 0 to 280 feet; largely continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0410|38.5023411|-76.00465991|Dorchester|Maryland|DO Ce 60|Cambridge||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383008076001801&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1313|DO Ce 61|25.0|||RSY12|DO Ce 61|0.0| 83 envelopes in 4 boxes; spanning depths of 0 to 449.5 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0411|38.55984097|-76.06605093|Dorchester|Maryland|DO Ce 61|Cambridge||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_17.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383335076035901&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1314|DO Ce 77|25.0|||RSY12|DO Ce 77|0.0| 240 envelopes in 13 boxes; spanning depths of 0 to 1505 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0412|38.56150733|-76.04105016|Dorchester|Maryland|DO Ce 77|Cambridge||cuttings||||http://www.mgs.md.gov/publications/report_pages/OFR_12-02-20.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383341076022901&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1315|DO Ce 78|25.0|||RSY12|DO Ce 78|0.0| 107 envelopes in 6 boxes; spanning depths of 0 to 517 feet; largely continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0413|38.5453968|-76.07271772|Dorchester|Maryland|DO Ce 78|Cambridge||cuttings||||http://www.mgs.md.gov/publications/report_pages/OFR_12-02-20.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383243076042301&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1316|DO Ce 88|25.0|||RSY12|DO Ce 88|0.0| 317 envelopes in 18 boxes; spanning depths of 100 to 3316 feet; largely continuous coverage in 10 ft intervals below 100 ft depth.||WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0414|38.56706297|-76.0552173|Dorchester|Maryland|DO Ce 88|Cambridge||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383401076032001&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1317|DO Cf 34|25.0|||RSY12|DO Cf 34|0.0| 10 envelopes in 1 box; spanning depths of 1.5 to 75.5 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0415|38.56567225|-75.88382434|Dorchester|Maryland|DO Cf 34|East New Market||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383356075530301&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1318|DO Cg 21|25.0|||RSY12|DO Cg 21|0.0| 24 envelopes in 1 box; spanning depths of 0 to 120 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0416|38.55845043|-75.91326937|Dorchester|Maryland|DO Cg 21|East New Market||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_17.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383330075544901&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1319|DO Cg 22|25.0|||RSY12|DO Cg 22|0.0| 24 envelopes in 1 box; spanning depths of 0 to 120 feet; continuous coverage in 5 ft intervals.||WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0417|38.55483902|-75.88076873|Dorchester|Maryland|DO Cg 22|East New Market||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_17.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383317075525201&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1320|DO Cg 23|25.0|||RSY12|DO Cg 23|0.0| 11 envelopes in 1 box; spanning depths of 0 to 110 feet; continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0418|38.57261668|-75.89076893|Dorchester|Maryland|DO Cg 23|East New Market||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_17.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383421075532801&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1321|DO Ch 26|25.0|||RSY12|DO Ch 26|0.0| 20 envelopes in 1 box; spanning depths of 0 to 100 feet; continuous coverage in 5 ft intervals.||WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0419|38.56428253|-75.80215605|Dorchester|Maryland|DO Ch 26|Rhodesdale||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383351075480901&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1322|DO Ci 3|25.0|||RSY12|DO Ci 3|0.0| 32 envelopes in 2 boxes; spanning depths of 0 to 73 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0420|38.5615042|-75.72937637|Dorchester|Maryland|DO Ci 3|Sharptown||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=383341075434701&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1323|DO Db 7|25.0|||RSY12|DO Db 7|0.0| 30 envelopes in 1 box; spanning depths of 10 to 300 feet; largely continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:00|DAS02|WP0421|38.45012219|-76.2955018|Dorchester|Maryland|DO Db 7|Taylors Island||cuttings|||||||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=382700076174501&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1324|DO Db 17|25.0|||RSY12|DO Db 17|0.0| 28 envelopes in 2 boxes; spanning depths of 50 to 320 feet; largely continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0422|38.46658333|-76.30141667|Dorchester|Maryland|DO Db 17|Taylors Island||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_31.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=382800076180701&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1325|DO Dd 1|25.0|||RSY12|DO Dd 1|0.0| 38 envelopes in 2 boxes; spanning depths of 0 to 384 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0423|38.47373182|-76.14244159|Dorchester|Maryland|DO Dd 1|Golden Hill||cuttings||||https://waterdata.usgs.gov/nwis/inventory|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=382825076083401&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1326|DO De 3|25.0|||RSY12|DO De 3|0.0| 43 envelopes in 2 boxes; spanning depths of 0 to 434 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0424|38.4473427|-76.08105064|Dorchester|Maryland|DO De 3|Blackwater River||cuttings||||https://waterdata.usgs.gov/nwis/inventory|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=382650076045301&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1327|DO Dg 23|25.0|||RSY12|DO Dg 23|0.0| 25 envelopes in 2 boxes; spanning depths of 0 to 260 feet; continuous coverage in 10 ft intervals.||WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0425|38.47817298|-75.83798982|Dorchester|Maryland|DO Dg 23|Mardela Springs||cuttings||||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=382841076501801&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1328|DO Ec 4|25.0|||RSY12|DO Ec 4|0.0| 78 envelopes in 3 boxes; spanning depths of 0 to 393 feet; largely continous coverage in 10 and 13 ft intervals||WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0426|38.38456649|-76.18855368|Dorchester|Maryland|DO Ec 4|Golden Hill||cuttings||||https://waterdata.usgs.gov/nwis/inventory|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=382304076112001&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1329|DO Ed 3|25.0|||RSY12|DO Ed 3|0.0| 21 envelopes in 1 box; spanning depths of 230 to 437 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0427|38.34345559|-76.14855212|Dorchester|Maryland|DO Ed 3|Honga||cuttings||||https://waterdata.usgs.gov/nwis/inventory|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=382036076085601&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1330|DO Ed 8|25.0|||RSY12|DO Ed 8|0.0| 94 envelopes in 3 boxes; spanning depths of 0 to 800 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0428|38.34928854|-76.08660561|Dorchester|Maryland|DO Ed 8|Wingate||cuttings||||https://waterdata.usgs.gov/nwis/inventory|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=382057076051301&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1331|DO Ed 9|25.0|||RSY12|DO Ed 9|0.0| 65 envelopes in 3 boxes; spanning depths of 0 to 465 feet; sampling intervals vary.||WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0429|38.35734411|-76.10993979|Dorchester|Maryland|DO Ed 9|Wingate||cuttings||||https://waterdata.usgs.gov/nwis/inventory|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=382126076063701&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1332|DO Fc 2|25.0|||RSY12|DO Fc 2|0.0| 19 envelopes in 1 box; spanning depths of 1 to 183 feet; largely continous coverage mainly in 10 ft intervals||WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0430|38.25984548|-76.17910829|Dorchester|Maryland|DO Fc 2|Honga||cuttings||||https://waterdata.usgs.gov/nwis/inventory|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=381535076104601&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1333|DO Fc 10|25.0|||RSY12|DO Fc 10|0.0| 17 envelopes in 1 box; spanning depths of 0 to 200 feet; sampling in 10 ft intervals; sevearl intervals missing||WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:41:08.000001|DAS02|WP0431|38.32484504|-76.23161044|Dorchester|Maryland|DO Fc 10|Honga||cuttings||||https://waterdata.usgs.gov/nwis/inventory|||http://waterdata.usgs.gov/md/nwis/inventory/?site_no=381929076135501&agency_cd=USGS&amp;||||||||||||||||||||||||||||||||||||
1334|AA Cc 115|25.0|||RSY10|AA Cc 115|0.0|2 boxes, generally in 2-ft segments from limited intervals from depths of 13 to 663 feet.|Global Positioning System (GPS), Standard Positioning Service (SPS) or Precise Positioning Service (PPS)|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0432|39.01769444|-76.67388889|Anne Arundel|Maryland|AA Cc 115|Odenton||sediment core|1.5|Core in good condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=390103076402601&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1335|AA Ce 120|25.0|||RSY10|AA Ce 120|0.0|includes end of core plus approx. 22 feet of core from depths of 1310 to 1342 feet.|Global Positioning System (GPS), Standard Positioning Service (SPS) or Precise Positioning Service (PPS)|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0433|39.05088889|-76.57844444|Anne Arundel|Maryland|AA Ce 120|Round Bay||sediment core||Core in good condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=390303076344301&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1336|AA Cf 101|25.0|||RSY10|AA Cf 101|0.0|approx. 19 core segments from limited intervals from depths of 54 to 377 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0434|39.03066662|-76.47384968|Anne Arundel|Maryland|AA Cf 101|Gibson Island||sediment core|1.5|Core in good condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=390150076282701&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1337|AA Cf 136|25.0|||RSY10|AA Cf 136|0.0|1 box of core from limited intervals from depths of 252 to 1575 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0435|39.03483319|-76.49051685|Anne Arundel|Maryland|AA Cf 136|Gibson Island||sediment core|1.5|Core in fair to poor condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=390205076292701&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1338|AA Cg 22|25.0|||RSY10|AA Cg 22|0.0|2 boxes of core from limited intervals from depths of 1037 to 1770 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0436|39.02316687|-76.4041254|Anne Arundel|Maryland|AA Cg 22|Gibson Island||sediment core||Core in fair to poor condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=390123076241601&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1339|AA Cg 23|25.0|||RSY10|AA Cg 23|0.0|2 boxes of core from limited intervals from depths of 210 to 973 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0437|39.02316687|-76.4041254|Anne Arundel|Maryland|AA Cg 23|Gibson Island||sediment core||Core in fair to poor condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=390123076241602&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1340|AA Dd 43|25.0|||RSY10|AA Dd 43|0.0|approx. 19 core segments from limited intervals from depths of 103 to 503 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0438|38.96900041|-76.62607589|Anne Arundel|Maryland|AA Dd 43|Bowie||sediment core|1.75|Core in good condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=385808076373503&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1341|AA De 100|25.0|||RSY10|AA De 100|0.0|53 boxes of core in plastic bags by sub intervals (generally poor condition) from depths of 6 to 436 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0439|38.95566809|-76.50746049|Anne Arundel|Maryland|AA De 100|South River||sediment core|2.5; 3|Bags in very poor to good condition, ||http://www.mgs.md.gov/output/reports/RI/RI_22.pdf|http://www.mgs.md.gov/publications/report_pages/OFR_12-02-20.html||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=385720076302801&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1342|AA De 104|25.0|||RSY10|AA De 104|0.0|5 boxes of core from approx. 37 intervals from depths of 20 to 459 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0440|38.91955759|-76.55357237|Anne Arundel|Maryland|AA De 104|South River||sediment core||Core in fair condition||http://www.mgs.md.gov/publications/report_pages/OFR_12-02-20.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=385510076331401&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1343|AA De 140|25.0|||RSY10|AA De 140|0.0|approx. 7 core segments from limited intervals from depths of 29 to 51.5 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0441|38.98872265|-76.53885127|Anne Arundel|Maryland|AA De 140|South River||sediment core||Core in fair condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=385920076322401&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1344|AA De 144|25.0|||RSY10|AA De 144|0.0|2 boxes of core from limited intervals from depths of 14 to 100.5 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0442|38.98872265|-76.53885127|Anne Arundel|Maryland|AA De 144|South River||sediment core|1.5|Core in fair condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=385920076322402&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1345|AA De 159|25.0|||RSY10|AA De 159|0.0|2 boxes of core from limited intervals from depths of 18.2 to 110 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0443|38.99122258|-76.53885133|Anne Arundel|Maryland|AA De 159|South River||sediment core||Core in fair condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=385928076321703&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1346|AA Df 90|25.0|||RSY10|AA Df 90|0.0|3 boxes containing core from approx. 21 intervals from depths of 80 to 497 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0444|38.92122462|-76.47329181|Anne Arundel|Maryland|AA Df 90|Annapolis||sediment core||Core in fair condition, plastic disintegrating|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=385516076282501&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1347|CA Db 65|25.0|||RSY10|CA Db 65|0.0|core from limited intervals  from depths of 4 to 51 feet.|Global Positioning System (GPS), Standard Positioning Service (SPS) or Precise Positioning Service (PPS)|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0445|38.53772222|-76.58688889|Calvert|Maryland|CA Db 65|Prince Frederick||sediment core||Core in fair condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=383216076351401&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1348|CA Db 71|25.0|||RSY10|CA Db 71|0.0|core from limited intervals  from depths of 0 to 40.5 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0446|38.53817745|-76.58773518|Calvert|Maryland|CA Db 71|Prince Frederick||sediment core||Core in fair condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=383217076351701&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1349|CA Db 72|25.0|||RSY10|CA Db 72|0.0|core from limited intervals  from depths of 28 to 29 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0447|38.53817745|-76.58773518|Calvert|Maryland|CA Db 72|Prince Frederick||sediment core||Core in fair condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=383217076351702&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1350|CA Db 73|25.0|||RSY10|CA Db 73|0.0|core from limited intervals  from depths of 1 to 2.5 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0448|38.53817745|-76.58773518|Calvert|Maryland|CA Db 73|Prince Frederick||sediment core||Core in fair condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=383217076351703&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1351|CE Be 155|25.0|||RSY11|CE Be 155|0.0|11 boxes of nearly continuous core (includes weathered bedrock at base) from depths of 4 to 202.83 feet.|Global Positioning System (GPS), Standard Positioning Service (SPS) or Precise Positioning Service (PPS)|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0449|39.60008333|-75.83761111|Cecil|Maryland|CE Be 155|Elkton||sediment core;rock core|2.25|Core in fair to good condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=393600075501501&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1352|CE Be 73|25.0|||RSY10|CE Be 73|0.0|4 segments from limited intervals from depths of 43 to 112 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0450|39.61039044|-75.89688604|Cecil|Maryland|CE Be 73|North East||sediment core|1.5|Core in good condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=393637075535001&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1353|CE Bf 156|25.0|||RSY11|CE Bf 156|0.0|15 boxes of nearly continuous core (includes weathered bedrock at base) from depths of 4 to 200 feet.|Global Positioning System (GPS), Standard Positioning Service (SPS) or Precise Positioning Service (PPS)|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0451|39.602225|-75.79347222|Cecil|Maryland|CE Bf 156|Elkton||sediment core;rock core|2.25|Core in fair to good condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=393608075473901&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1354|CE Bf 81|25.0|||RSY10|CE Bf 81|0.0|core from limited intervals  from depths of 50 to 50 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0452|39.60427865|-75.79938118|Cecil|Maryland|CE Bf 81|Elkton||sediment core|1.5|Core in good condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=393615075475901&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1355|CE Bf 82|25.0|||RSY10|CE Bf 82|0.0|core from 4 intervals from depths of 60 to 200 feet.|Global Positioning System (GPS), Standard Positioning Service (SPS) or Precise Positioning Service (PPS)|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0453|39.59361111|-75.82211111|Cecil|Maryland|CE Bf 82|Elkton||sediment core|1.5|Core in good condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=393537075492001&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1356|CE Cd 51|25.0|||RSY10|CE Cd 51|0.0|core from 3 intervals from depths of 15 to 89 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0454|39.57567001|-75.99300206|Cecil|Maryland|CE Cd 51|North East||sediment core|1.5|Core in good condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=393432075593601&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1357|CE Cd 53|25.0|||RSY10|CE Cd 53|0.0|core from 3 intervals from depths of 97 to 279 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0455|39.53789262|-75.94466632|Cecil|Maryland|CE Cd 53|North East||sediment core|1.5|Core in good condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=393216075564201&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1358|CE Cd 91|25.0|||RSY11|CE Cd 91|0.0|51 boxes of nearly continuous core (includes weathered bedrock at base) from depths of 5 to 590 feet.|Global Positioning System (GPS), Standard Positioning Service (SPS) or Precise Positioning Service (PPS)|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:21|DAS03|WP0456|39.54527905|-75.94288749|Cecil|Maryland|CE Cd 91|North East||sediment core;rock core|2|Core in good condition|||||||||||||||||||||||||||||||||||||||||
1359|CE Ce 54|25.0|||RSY10|CE Ce 54|0.0|core from 3 intervals from depths of 20 to 171 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0457|39.57594685|-75.91327575|Cecil|Maryland|CE Ce 54|North East||sediment core|1.5|Core in good condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=393433075544901&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1360|CE Ce 55|25.0|||RSY10|CE Ce 55|0.0|core from 7 intervals from depths of 100 to 604 feet.|Interpolated from digital map|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0458|39.54480556|-75.83369444|Cecil|Maryland|CE Ce 55|Elkton||sediment core|1.5|Core in good condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=393241075500201&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1361|CE Ce 56|25.0|||RSY10|CE Ce 56|0.0|core from 7 intervals from depths of 100 to 420 feet.|Global Positioning System (GPS), Standard Positioning Service (SPS) or Precise Positioning Service (PPS)|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0459|39.50761111|-75.87491667|Cecil|Maryland|CE Ce 56|Elkton||sediment core|1.5|Core in good condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=393026075523101&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1362|CE Dc 2|25.0|||RSY09|CE Dc 2|0.0|5 boxes of core from limited intervals (subsampled for thin sections) from depths of 849 to 936 feet.|Reported|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:21|DAS03|WP0460|39.45455976|-76.00800239|Cecil|Maryland|CE Dc 2|Spesutie||rock core|1.75|Core in fair to good condition||http://www.mgs.md.gov/publications/report_pages/OFR_12-02-20.html|http://www.mgs.md.gov/publications/report_pages/RI_30.html||||||||||||||||||||||||||||||||||||||
1363|CE Dd 81|25.0|||RSY10|CE Dd 81|0.0|core from 8 intervals from depths of 20 to 500 feet.|Global Positioning System (GPS), Standard Positioning Service (SPS) or Precise Positioning Service (PPS)|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0461|39.42688889|-75.99163889|Cecil|Maryland|CE Dd 81|Earleville||sediment core|1.5|Core in good condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=392536075593201&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1364|CE De 60|25.0|||RSY10|CE De 60|0.0|9 boxes of core from limited intervals from depths of 0 to 88 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:21|DAS03|WP0462|39.41941667|-75.85972222|Cecil|Maryland|CE De 60|Cecilton||sediment core|1.5|Core in fair to poor condition|||||||||||||||||||||||||||||||||||||||||
1365|CE Ec 17|25.0|||RSY11|CE Ec 17|0.0|5 boxes of core from limited intervals (subsampled for thin sections) from depths of 1022 to 1107 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0463|39.40511349|-76.02466896|Cecil|Maryland|CE Ec 17|Spesutie||sediment core;rock core|1.75|Core in poor to fair condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=392418076013003&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1366|CE Ec 18|25.0|||RSY10|CE Ec 18|0.0|1.3 feet of core from depths of 25 to 27 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0464|39.39705807|-76.00716815|Cecil|Maryland|CE Ec 18|Spesutie||sediment core||Core in poor condition||http://www.mgs.md.gov/publications/report_pages/RI_40.html|http://www.mgs.md.gov/publications/report_pages/OFR_12-02-20.html||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=392349076002701&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1367|CE Ec 19|25.0|||RSY10|CE Ec 19|0.0|3.2 feet of core from depths of 25 to 47 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0465|39.39622435|-76.02466883|Cecil|Maryland|CE Ec 19|Spesutie||sediment core|1.5|Core in fair to poor condition||http://www.mgs.md.gov/publications/report_pages/RI_40.html|http://www.mgs.md.gov/publications/report_pages/OFR_12-02-20.html||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=392346076013001&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1368|CE Ed 19|25.0|||RSY10|CE Ed 19|0.0|1.1 feet of core from depths of 50 to 52 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0466|39.4017801|-75.95077656|Cecil|Maryland|CE Ed 19|Earleville||sediment core||Core in poor condition||http://www.mgs.md.gov/publications/report_pages/RI_40.html|http://www.mgs.md.gov/publications/report_pages/OFR_12-02-20.html||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=392404075570601&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1369|CE Ed 20|25.0|||RSY10|CE Ed 20|0.0|1.2 feet of core from depths of 40 to 42 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0467|39.39955799|-75.96827741|Cecil|Maryland|CE Ed 20|Earleville||sediment core||Core in poor condition||http://www.mgs.md.gov/publications/report_pages/RI_40.html|http://www.mgs.md.gov/publications/report_pages/OFR_12-02-20.html||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=392358075580701&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1370|CE Ed 21|25.0|||RSY10|CE Ed 21|0.0|1.1 feet of core (depth uncertain).|Interpolated from map|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0468|39.39789151|-75.99105632|Cecil|Maryland|CE Ed 21|Earleville||sediment core|1.5|Core in fair condition||http://www.mgs.md.gov/publications/report_pages/RI_40.html|http://www.mgs.md.gov/publications/report_pages/OFR_12-02-20.html||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=392352075592901&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1371|CE Ee 55|25.0|||RSY10|CE Ee 55|0.0|28 boxes of nearly continuous core (subsampled for paleo) from depths of 3 to 320 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:21|DAS03|WP0469|39.40630833|-75.87629722|Cecil|Maryland|CE Ee 55|Earleville||sediment core|2, 2.5|Core in poor to good condition|||||||||||||||||||||||||||||||||||||||||
1372|CE Ee 56|25.0|||RSY10|CE Ee 56|0.0|6 boxes of nearly continuous core (fair to poor condition) from depths of 0 to 60 feet.|Reported|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:21|DAS03|WP0470|39.40194444|-75.84333333|Cecil|Maryland|CE Ee 56|Cecilton||sediment core|1.5|Core in fair to poor condition|||||||||||||||||||||||||||||||||||||||||
1373|CH Bb 22|25.0|||RSY10|CH Bb 22|0.0|1 box of core chips to disks from about 10 intervals from depths of 112 to 641.2 feet.|Reported|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0471|38.60095185|-77.17886989|Charles|Maryland|CH Bb 22|Indian Head||sediment core|2|Core in fair to good condition||https://pubs.usgs.gov/wri/1991/4059/report.pdf|http://www.mgs.md.gov/publications/report_pages/OFR_12-02-20.html|http://www.mgs.md.gov/publications/report_pages/RI_69.html|https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=383634077104501&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1374|CH Bc 80|25.0|||RSY10|CH Bc 80|0.0|1 box of split spoon samples from 10 intervals from depths of 564 to 1115 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0472|38.6126183|-77.10636674|Charles|Maryland|CH Bc 80|Port Tobacco||sediment core|1.5|Core in fair condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=383645077062402&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1375|CH Be 48|25.0|||RSY10|CH Be 48|0.0|1 box of core from 4 intervals from depths of 160 to 503 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0473|38.61372983|-76.92941698|Charles|Maryland|CH Be 48|La Plata||sediment core|1.5|Core in good condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=383649076554701&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1376|CH Be 57|25.0|||RSY10|CH Be 57|0.0|1 box of core from 11 intervals from depths of 425 to 1316 feet.|Interpolated from digital map|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0474|38.61777778|-76.96388889|Charles|Maryland|CH Be 57|La Plata||sediment core|1.5|Core in fair to poor condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=383706076575601&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1377|CH Be 59|25.0|||RSY10|CH Be 59|0.0|1 box of core from 4 intervals from depths of 375 to 474 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0475|38.61845178|-76.96525147|Charles|Maryland|CH Be 59|La Plata||sediment core|1.5|Core in fair condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=383649076554702&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1378|CH Bf 144|25.0|||RSY10|CH Bf 144|0.0|6 boxes of core from limited intervals from depths of 400 to 1722 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0476|38.65372896|-76.85024816|Charles|Maryland|CH Bf 144|Brandywine||sediment core|1.5, 1.75|Core in poor to good condition||http://www.mgs.md.gov/reports/RI_44.pdf|http://www.mgs.md.gov/output/reports/OFR/OFR_86-02-2.pdf|http://www.mgs.md.gov/publications/report_pages/RI_53.html#http://www.mgs.md.gov/publications/report_pages/RI_53.html#|https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=383913076510201&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1379|CH Bf 146|25.0|||RSY10|CH Bf 146|0.0|1 box of core from approx. 13 intervals from depths of 420 to 1632 feet.|Global Positioning System (GPS), Standard Positioning Service (SPS) or Precise Positioning Service (PPS)|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0477|38.58588889|-76.90083333|Charles|Maryland|CH Bf 146|La Plata||sediment core|1.5|Core in good condition||http://www.mgs.md.gov/output/reports/OFR/OFR_86-02-2.pdf|http://www.mgs.md.gov/publications/report_pages/RI_53.html||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=383508076540701&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1380|CH Bf 148|25.0|||RSY11|CH Bf 148|0.0|30 boxes of nearly continuous core from depths of 39.5 to 457 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0478|38.65095115|-76.87997126|Charles|Maryland|CH Bf 148|Piscataway||sediment core;rock core|1.5, 1.75|Core in poor to good condition||http://www.mgs.md.gov/publications/report_pages/RI_53.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=383903076524901&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1381|CH Bf 149|25.0|||RSY10|CH Bf 149|0.0|12 boxes of nearly continuous core from depths of 453 to 616 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0479|38.65095115|-76.87997126|Charles|Maryland|CH Bf 149|Piscataway||sediment core|1.75|Core in poor to good condition||http://www.mgs.md.gov/output/reports/OFR/OFR_86-02-2.pdf|http://www.mgs.md.gov/publications/report_pages/RI_53.html||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=383903076524902&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1382|CH Bf 150|25.0|||RSY10|CH Bf 150|0.0|1 box of core from 4 intervals from depths of 808 to 1012 feet.|Global Positioning System (GPS), Standard Positioning Service (SPS) or Precise Positioning Service (PPS)|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0480|38.65036111|-76.87811111|Charles|Maryland|CH Bf 150|Piscataway||sediment core|1.5|Core in good condition||http://www.mgs.md.gov/publications/report_pages/RI_53.html|http://www.mgs.md.gov/publications/report_pages/OFR_03-02-17.html||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=383901076524301&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1383|CH Bf 151|25.0|||RSY10|CH Bf 151|0.0|3 boxes of core from limited intervals from depths of 47 to 546 feet.|Global Positioning System (GPS), Standard Positioning Service (SPS) or Precise Positioning Service (PPS)|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0481|38.58583333|-76.901|Charles|Maryland|CH Bf 151|La Plata||sediment core|1.5|Core in fair condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=383508076540703&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1384|CH Bf 158|25.0|||RSY10|CH Bf 158|0.0|2 boxes of core from approx. 19 intervals from depths of 238 to 778 feet.|Interpolated from digital map|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0482|38.62563889|-76.88819444|Charles|Maryland|CH Bf 158|Piscataway||sediment core|1.5|Core in fair to good condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=383732076531902&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1385|CH Cd 55|25.0|||RSY10|CH Cd 55|0.0|shallow direct-push core in plastic tubes (missing interval from 8 to 12 feet) from depths of 0 to 24 feet.|Global Positioning System (GPS), Standard Positioning Service (SPS) or Precise Positioning Service (PPS)|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0483|38.50741667|-77.02544444|Charles|Maryland|CH Cd 55|Port Tobacco||sediment core|1.5|||https://pubs.er.usgs.gov/publication/ofr20101071|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=383027077013201&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1386|CH Cd 59|25.0|||RSY10|CH Cd 59|0.0|shallow direct-push core in plastic tubes (missing interval from 16 t0 20 feet) from depths of 0 to 28 feet.|Global Positioning System (GPS), Standard Positioning Service (SPS) or Precise Positioning Service (PPS)|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0484|38.50722222|-77.03055556|Charles|Maryland|CH Cd 59|Port Tobacco||sediment core|1.5|||https://pubs.er.usgs.gov/publication/ofr20101071|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=383026077015001&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1387|CH Cd 60|25.0|||RSY10|CH Cd 60|0.0|shallow direct-push core in plastic tubes from depths of 0 to 24 feet.|Global Positioning System (GPS), Standard Positioning Service (SPS) or Precise Positioning Service (PPS)|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0485|38.50611111|-77.03611111|Charles|Maryland|CH Cd 60|Port Tobacco||sediment core|1.5|||https://pubs.er.usgs.gov/publication/ofr20101071|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=383022077021002&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1388|CH Cd 65|25.0|||RSY10|CH Cd 65|0.0|shallow direct-push core in plastic tubes (missing interval from 20 to 24 feet) from depths of 0 to 28 feet.|Global Positioning System (GPS), Standard Positioning Service (SPS) or Precise Positioning Service (PPS)|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0486|38.50583333|-77.02638889|Charles|Maryland|CH Cd 65|Port Tobacco||sediment core|1.5|||https://pubs.er.usgs.gov/publication/ofr20101071|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=383021077013503&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1389|CH Cd 66|25.0|||RSY10|CH Cd 66|0.0|shallow direct-push core in plastic tubes from depths of 12 to 20 feet.|Global Positioning System (GPS), Standard Positioning Service (SPS) or Precise Positioning Service (PPS)|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0487|38.50777778|-77.02722222|Charles|Maryland|CH Cd 66|Port Tobacco||sediment core|1.5|||https://pubs.er.usgs.gov/publication/ofr20101071|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=383028077013801&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1390|CH Cd 67|25.0|||RSY10|CH Cd 67|0.0|shallow direct-push core in plastic tubes from depths of 0 to 12 feet.|Global Positioning System (GPS), Standard Positioning Service (SPS) or Precise Positioning Service (PPS)|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0488|38.50777778|-77.02722222|Charles|Maryland|CH Cd 67|Port Tobacco||sediment core|1.5|||https://pubs.er.usgs.gov/publication/ofr20101071|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=383028077013802&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1391|CH Cd 69|25.0|||RSY10|CH Cd 69|0.0|shallow direct-push core in plastic tubes from depths of 0 to 32 feet.|Global Positioning System (GPS), Standard Positioning Service (SPS) or Precise Positioning Service (PPS)|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0489|38.5025|-77.02611111|Charles|Maryland|CH Cd 69|Port Tobacco||sediment core|1.5|||https://pubs.er.usgs.gov/publication/ofr20101071|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=383009077013403&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1392|CH Cd 72|25.0|||RSY10|CH Cd 72|0.0|shallow direct-push core in plastic tubes from depths of 0 to 28 feet.|Global Positioning System (GPS), Standard Positioning Service (SPS) or Precise Positioning Service (PPS)|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0490|38.50694444|-77.02833333|Charles|Maryland|CH Cd 72|Port Tobacco||sediment core|1.5|||https://pubs.er.usgs.gov/publication/ofr20101071|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=383025077014203&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1393|CH Cd 74|25.0|||RSY10|CH Cd 74|0.0|shallow direct-push core in plastic tubes from depths of 0 to 32 feet.|Global Positioning System (GPS), Standard Positioning Service (SPS) or Precise Positioning Service (PPS)|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0491|38.50722222|-77.03666667|Charles|Maryland|CH Cd 74|Port Tobacco||sediment core|1.5|||https://pubs.er.usgs.gov/publication/ofr20101071|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=383026077021202&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1394|CH Cd 78|25.0|||RSY10|CH Cd 78|0.0|shallow direct-push core in plastic tubes from depths of 4 to 32 feet.|Global Positioning System (GPS), Standard Positioning Service (SPS) or Precise Positioning Service (PPS)|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0492|38.50305556|-77.02888889|Charles|Maryland|CH Cd 78|Port Tobacco||sediment core|1.5|||https://pubs.er.usgs.gov/publication/ofr20101071|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=383011077014403&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1395|CH Cd 82|25.0|||RSY10|CH Cd 82|0.0|shallow direct-push core in plastic tubes from depths of 0 to 28 feet.|Global Positioning System (GPS), Standard Positioning Service (SPS) or Precise Positioning Service (PPS)|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0493|38.50694444|-77.02472222|Charles|Maryland|CH Cd 82|Port Tobacco||sediment core|1.5|||https://pubs.er.usgs.gov/publication/ofr20101071|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=383025077012904&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1396|CL Bd 176|25.0|||RSY09|CL Bd 176|0.0|15 boxes of nearly continuous core from depths of 25 to 234.5 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:21|DAS03|WP0494|39.589|-77.01441667|Carroll|Maryland|CL Bd 176|New Windsor||rock core|2|Core in fair to good condition||http://www.mgs.md.gov/publications/report_pages/RI_56.html|||||||||||||||||||||||||||||||||||||||
1397|CL Bd 177|25.0|||RSY09|CL Bd 177|0.0|8 boxes of nearly continuous core (variable recovery) from depths of 62 to 228.5 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:21|DAS03|WP0495|39.58875|-77.014025|Carroll|Maryland|CL Bd 177|New Windsor||rock core|2|Core in poor to good condition||http://www.mgs.md.gov/publications/report_pages/RI_56.html|||||||||||||||||||||||||||||||||||||||
1398|CL Bd 178|25.0|||RSY09|CL Bd 178|0.0|14 boxes of nearly continuous core from depths of 12 to 191 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:21|DAS03|WP0496|39.58921111|-77.01465833|Carroll|Maryland|CL Bd 178|New Windsor||rock core|2, 2.5|Core in fair to good condition||http://www.mgs.md.gov/publications/report_pages/RI_56.html|||||||||||||||||||||||||||||||||||||||
1399|CL Be MES MW-19|25.0|||RSY09|CL Be MES MW-19|0.0|1 box of nearly continuous core (variable recovery) from depths of 88.5 to 107.7 feet.|Reported|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:21|DAS03|WP0497|39.64423773|-76.99418592|Carroll|Maryland|CL Be MES MW-19|Manchester||rock core|2|Core in good condition|||||||||||||||||||||||||||||||||||||||||
1400|CL Be MES MW-21|25.0|||RSY09|CL Be MES MW-21|0.0|4 boxes of nearly continuous core from depths of 55 to 130 feet.|Reported|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:21|DAS03|WP0498|39.64463124|-76.9950506|Carroll|Maryland|CL Be MES MW-21|Manchester||rock core|2|Core in fair to good condition|||||||||||||||||||||||||||||||||||||||||
1401|CL Bf 194|25.0|||RSY10|CL Bf 194|0.0|2 boxes of nearly continuous core from depths of 0 to 22 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0499|39.63649154|-76.86942228|Carroll|Maryland|CL Bf 194|Lineboro||sediment core|1.5|Core in fair condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=393811076521101&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1402|CL Bf 195|25.0|||RSY10|CL Bf 195|0.0|1 box of core from limited intervals from depths of 0 to 16 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0500|39.63649154|-76.86942228|Carroll|Maryland|CL Bf 195|Lineboro||sediment core|1.5|Core in fair condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=393811076521102&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1403|CL Bf 196|25.0|||RSY10|CL Bf 196|0.0|1 box of core from select intervals (nearly continuous in upper half) from depths of 0 to 24.7 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0501|39.63676933|-76.8688667|Carroll|Maryland|CL Bf 196|Lineboro||sediment core|1.5|Core in fair condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=393812076520901&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1404|CL Bf 198|25.0|||RSY10|CL Bf 198|0.0|1 box of nearly continuous core from depths of 0 to 14 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0502|39.63815821|-76.86858891|Carroll|Maryland|CL Bf 198|Lineboro||sediment core||Core in poor condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=393817076520801&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1405|CL Bf 200|25.0|||RSY10|CL Bf 200|0.0|2 boxes of nearly continuous core from depths of 0 to 27.7 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0503|39.63621377|-76.86914449|Carroll|Maryland|CL Bf 200|Lineboro||sediment core|1.5|Core in fair condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=393810076521002&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1406|CO Ad 18|25.0|||RSY10|CO Ad 18|0.0|2 feet of core from depths of 20 to 22 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0504|39.1387233|-75.75659894|Caroline|Maryland|CO Ad 18|Sudlersville||sediment core||Core in fair condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=390819075452501&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1407|CO Ad 19|25.0|||RSY10|CO Ad 19|0.0|limited core (25 to 27 and 45 to 47 feet) from depths of 25 to 47 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0505|39.1223345|-75.77604408|Caroline|Maryland|CO Ad 19|Goldsboro||sediment core||Core in fair condition, wrapped in plastic sheets||http://www.dgs.udel.edu/publications/ri72-geology-and-extent-confined-aquifers-kent-county-delaware|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=390720075463501&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1408|CO Cb 19|25.0|||RSY10|CO Cb 19|0.0|12 plastic tubes of nearly continuous core from depths of 0 to 56 feet.|Global Positioning System (GPS), Standard Positioning Service (SPS) or Precise Positioning Service (PPS)|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:21|DAS03|WP0506|38.95230556|-75.93438889|Caroline|Maryland|CO Cb 19|Ridgely||sediment core|1.5|Core in fair to good condition|||||||||||||||||||||||||||||||||||||||||
1409|CO Cb 20|25.0|||RSY10|CO Cb 20|0.0|11 plastic tubes of nearly continuous core from depths of 0 to 54 feet.|Global Positioning System (GPS), Standard Positioning Service (SPS) or Precise Positioning Service (PPS)|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:21|DAS03|WP0507|38.96605833|-75.94066667|Caroline|Maryland|CO Cb 20|Ridgely||sediment core|1.5|Core in poor to good condition|||||||||||||||||||||||||||||||||||||||||
1410|CO Cb 21|25.0|||RSY10|CO Cb 21|0.0|14 plastic tubes of nearly continuous core from depths of 0 to 69 feet.|Global Positioning System (GPS), Standard Positioning Service (SPS) or Precise Positioning Service (PPS)|WJUNKIN|2021-08-19 16:38:51.000001|WJUNKIN|2021-08-31 16:43:21|DAS03|WP0508|38.945475|-75.93967778|Caroline|Maryland|CO Cb 21|Ridgely||sediment core|1.5|Core in fair to good condition|||||||||||||||||||||||||||||||||||||||||
1411|CO Cc 54|25.0|||RSY10|CO Cc 54|0.0|3 boxes of core from approx. 15 intervals from depths of 5 to 122 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0509|38.92066916|-75.86715768|Caroline|Maryland|CO Cc 54|Denton||sediment core||Core in fair to good condition||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=385514075520301&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1412|CO Cc 60|25.0|||RSY10|CO Cc 60|0.0|2 feet of core (depth uncertain).|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0510|38.91816896|-75.99771752|Caroline|Maryland|CO Cc 60|Ridgely||sediment core|1.5|Core in fair condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=385505075595301&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1413|CO Cc 63|25.0|||RSY10|CO Cc 63|0.0|2-foot core segments from 4 intervals from depths of 20 to 77 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0511|38.93483571|-75.89410306|Caroline|Maryland|CO Cc 63|Ridgely||sediment core||Core in fair condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=385605075534001&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1414|CO Cc 64|25.0|||RSY10|CO Cc 64|0.0|11 feet of core (generally 2-foot segments) from depths of 20 to 82 feet.|Interpolated from digital map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0512|38.93055556|-75.90777778|Caroline|Maryland|CO Cc 64|Ridgely||sediment core||Core in fair condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=385949075543001&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1415|CO Cc 65|25.0|||RSY10|CO Cc 65|0.0|2-foot core segments from two intervals (25 to 27 feet and 40 to 42 feet) from depths of 25 to 42 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0513|38.95372462|-75.85604626|Caroline|Maryland|CO Cc 65|Denton||sediment core||Core in fair condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=385713075512301&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1416|CO Cd 56|25.0|||RSY10|CO Cd 56|0.0|6 feet of core from 3 intervals from depths of 35 to 62 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0514|38.96261384|-75.76354306|Caroline|Maryland|CO Cd 56|Denton||sediment core||Core in fair condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=385745075455001&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1417|CO Cd 66|25.0|||RSY10|CO Cd 66|0.0|limited core segments from 5 intervals from depths of 90 to 240.8 feet.|Global Positioning System (GPS), Standard Positioning Service (SPS) or Precise Positioning Service (PPS)|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0515|38.97202778|-75.80188889|Caroline|Maryland|CO Cd 66|Denton||sediment core|1.5|Core in good condition||http://www.mgs.md.gov/publications/report_pages/BDR_23.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=385819075480701&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1418|CO Ce 8|25.0|||RSY10|CO Ce 8|0.0|6 feet of core from 3 intervals from depths of 25 to 67 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0516|38.95650272|-75.73326423|Caroline|Maryland|CO Ce 8|Burrsville||sediment core||Core in fair condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=385723075440101&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1419|CO Ce 9|25.0|||RSY10|CO Ce 9|0.0|2-foot segment of core (10 to 12 feet) from depths of 10 to 12 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0517|38.95650272|-75.73326423|Caroline|Maryland|CO Ce 9|Burrsville||sediment core||Core in fair condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=385723075440102&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1420|CO Dc 135|25.0|||RSY10|CO Dc 135|0.0|5 feet of core from 2 intervals from depths of 40 to 50 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0518|38.93511355|-75.86854665|Caroline|Maryland|CO Dc 135|Denton||sediment core||Core in fair condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=385606075520801&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1421|CO Dc 136|25.0|||RSY10|CO Dc 136|0.0|6 feet of core from 3 intervals from depths of 35 to 77 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0519|38.91511359|-75.89521414|Caroline|Maryland|CO Dc 136|Ridgely||sediment core||Core in fair condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=385454075534401&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1422|CO Dc 137|25.0|||RSY10|CO Dc 137|0.0|approx. 5 feet of core from 2 intervals from depths of 33 to 60 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0520|38.84400285|-75.88632474|Caroline|Maryland|CO Dc 137|Fowling Creek||sediment core||Core in fair condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=385038075531201&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1423|CO Dc 138|25.0|||RSY10|CO Dc 138|0.0|1.6 feet of core from depths of 30 to 32 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0521|38.88233599|-75.84993483|Caroline|Maryland|CO Dc 138|Denton||sediment core|1.5|Core in fair condition||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=385256075510101&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1424|CO Dc 152|25.0|||RSY10|CO Dc 152|0.0|40 boxes of nearly continuous core (variable recovery) from depths of 0 to 396.6 feet.|Global Positioning System (GPS), Standard Positioning Service (SPS) or Precise Positioning Service (PPS)|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0522|38.86638889|-75.83944444|Caroline|Maryland|CO Dc 152|Hobbs||sediment core|2|Core in good condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/BDR_23.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=385159075502201&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1425|CO Dd 48|25.0|||RSY10|CO Dd 48|0.0|approx. 3 feet of core from depths of 45 to 62 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0523|38.88122487|-75.82104504|Caroline|Maryland|CO Dd 48|Denton||sediment core||Core in fair condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=385252075491701&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1426|CO Dd 49|25.0|||RSY10|CO Dd 49|0.0|approx. 1 foot of core from depths of 31.5 to 45 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0524|38.85122491|-75.81521153|Caroline|Maryland|CO Dd 49|Hobbs||sediment core||Core in fair condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=385104075485601&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1427|CO Dd 50|25.0|||RSY10|CO Dd 50|0.0|approx. 4 feet of core from depths of 30 to 47 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0525|38.83844708|-75.78548843|Caroline|Maryland|CO Dd 50|Hobbs||sediment core||Core in fair condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=385018075470901&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1428|CO Ec 17|25.0|||RSY10|CO Ec 17|0.0|approx. 10 feet of core (2-foot segments from 5 intervals) from depths of 70 to 97 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0526|38.7626143|-75.87437973|Caroline|Maryland|CO Ec 17|Hobbs||sediment core||Core in fair condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=384545075522901&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1429|CO Ec 18|25.0|||RSY10|CO Ec 18|0.0|1.2 feet of core from depths of 42 to 44 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0527|38.76872521|-75.84410118|Caroline|Maryland|CO Ec 18|Hobbs||sediment core||Core in fair condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=384607075504001&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1430|CO Ec 19|25.0|||RSY10|CO Ec 19|0.0|2.35 feet of core from depths of 22 to 77 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0528|38.76316983|-75.8693796|Caroline|Maryland|CO Ec 19|Hobbs||sediment core|1.375|Core in fair condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=384547075521101&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1431|CO Ec 20|25.0|||RSY10|CO Ec 20|0.0|6 feet of core (2-foot segments from 3 intervals) from depths of 25.5 to 82 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0529|38.76566984|-75.87271303|Caroline|Maryland|CO Ec 20|Hobbs||sediment core||Core in fair condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=384556075522301&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1432|CO Ec 24|25.0|||RSY10|CO Ec 24|0.0|6 feet of core (2-foot segments from 3 intervals) from depths of 8 to 52 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0530|38.79066972|-75.8707686|Caroline|Maryland|CO Ec 24|Hobbs||sediment core||Core in fair condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/OFR_12-02-20.html|http://www.mgs.md.gov/publications/report_pages/RI_40.html||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=384726075521601&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1433|CO Ec 25|25.0|||RSY10|CO Ec 25|0.0|3 boxes containing approx. 30 feet of core in 2-foot segments from select intervals from depths of 5 to 122 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0531|38.77511428|-75.87965768|Caroline|Maryland|CO Ec 25|Fowling Creek||sediment core|1.5|Core in good condition||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=384630075524801&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1434|CO Ed 26|25.0|||RSY10|CO Ed 26|0.0|2.4 feet of core from depths of 52 to 60 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0532|38.76761396|-75.82048945|Caroline|Maryland|CO Ed 26|Hobbs||sediment core||Core in fair condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=384603075491501&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1435|CO Ed 27|25.0|||RSY10|CO Ed 27|0.0|approx. 4 feet of core (2-foot segments from 2 intervals) from depths of 50 to 62 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0533|38.82816925|-75.76521008|Caroline|Maryland|CO Ed 27|Hobbs||sediment core||Core in fair condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=384941075455601&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1436|CO Ed 28|25.0|||RSY10|CO Ed 28|0.0|approx. 3 feet of core from depths of 50 to 60 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0534|38.81761363|-75.75048747|Caroline|Maryland|CO Ed 28|Hobbs||sediment core||Core in fair condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=384903075450301&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1437|CO Ed 29|25.0|||RSY10|CO Ed 29|0.0|approx. 6 feet of core from depths of 35 to 67 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0535|38.76400278|-75.80882247|Caroline|Maryland|CO Ed 29|Hobbs||sediment core||Core in fair condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=384550075483301&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1438|CO Ee 17|25.0|||RSY10|CO Ee 17|0.0|approx. 4 feet of core from depths of 60 to 67 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0536|38.80483581|-75.73465362|Caroline|Maryland|CO Ee 17|Hickman||sediment core||Core in fair condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=384817075440601&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1439|CO Ee 18|25.0|||RSY10|CO Ee 18|0.0|2 feet of core plus off auger samples from limited intervals from depths of 70 to 82 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0537|38.80261358|-75.72354212|Caroline|Maryland|CO Ee 18|Hickman||sediment core||Core in fair condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=384809075432601&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1440|CO Ee 19|25.0|||RSY10|CO Ee 19|0.0|2 feet of core from depths of 80 to 82 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0538|38.79928025|-75.72104205|Caroline|Maryland|CO Ee 19|Hickman||sediment core||Core in fair condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=384757075431701&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1441|CO Fc 32|25.0|||RSY10|CO Fc 32|0.0|4 feet of core from depths of 25 to 32 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0539|38.70428141|-75.85160138|Caroline|Maryland|CO Fc 32|Federalsburg||sediment core||Core in fair condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=384215075510701&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1442|CO Fd 31|25.0|||RSY10|CO Fd 31|0.0|4 feet of core from depths of 20 to 47 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0540|38.74816937|-75.79326653|Caroline|Maryland|CO Fd 31|Federalsburg||sediment core||Core in fair condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=384453075473701&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1443|DO Af 1|25.0|||RSY10|DO Af 1|0.0|4 feet of core from depths of 25 to 52 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0541|38.66789358|-75.92660313|Dorchester|Maryland|DO Af 1|Preston||sediment core||Core in fair condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=384004075553701&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1444|DO Ag 10|25.0|||RSY10|DO Ag 10|0.0|4 feet of core from depths of 15 to 27 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0542|38.68150427|-75.89688023|Dorchester|Maryland|DO Ag 10|Preston||sediment core||Core in fair condition, wrapped in plastic sheets|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=384053075535001&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1445|DO Ag 8|25.0|||RSY10|DO Ag 8|0.0|4 feet of core from depths of 64 to 66.5 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0543|38.6742821|-75.89215789|Dorchester|Maryland|DO Ag 8|Preston||sediment core||Core in fair condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=384027075533301&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1446|DO Ag 9|25.0|||RSY10|DO Ag 9|0.0|2 feet of core from depths of 44 to 47 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0544|38.6670601|-75.90743602|Dorchester|Maryland|DO Ag 9|Preston||sediment core||Core in fair condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=384001075542801&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1447|DO Ah 6|25.0|||RSY10|DO Ah 6|0.0|2 feet of core from depths of 80 to 82 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0545|38.69233687|-75.82243403|Dorchester|Maryland|DO Ah 6|Federalsburg||sediment core||Core in fair condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=384132075492201&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1448|DO Bg 60|25.0|||RSY10|DO Bg 60|0.0|approx. 36 feet of core (2-foot segments from 18 intervals) from depths of 5 to 112 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0546|38.59456075|-75.8796576|Dorchester|Maryland|DO Bg 60|East New Market||sediment core|1|Core in fair condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=383540075524801&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1449|DO Bg 66|25.0|||RSY10|DO Bg 66|0.0|4 feet of core from depths of 60 to 72 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0547|38.66233755|-75.86326834|Dorchester|Maryland|DO Bg 66|Federalsburg||sediment core||Core in fair condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=383944075514901&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1450|DO Bg 67|25.0|||RSY10|DO Bg 67|0.0|2 feet of core from depths of 60 to 62 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0548|38.66372686|-75.91438062|Dorchester|Maryland|DO Bg 67|Preston||sediment core||Core in fair condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=383949075545301&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1451|DO Bh 14|25.0|||RSY10|DO Bh 14|0.0|2 feet of core from depths of 55.5 to 57.5 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0549|38.61428225|-75.82993431|Dorchester|Maryland|DO Bh 14|Rhodesdale||sediment core||Core in fair condition, wrapped in plastic sheets|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=383651075494901&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1452|DO Bi 13|25.0|||RSY10|DO Bi 13|0.0|6 feet of core (2-foot segments from 3 intervals) from depths of 36 to 82 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0550|38.59011504|-75.72798734|Dorchester|Maryland|DO Bi 13|Sharptown||sediment core||Core in fair condition, wrapped in plastic sheets|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=383524075434201&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1453|DO Ce 88|25.0|||RSY11|DO Ce 88|0.0|4 boxes of core from limited intervals from depths of 139 to 3326 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0551|38.56706297|-76.0552173|Dorchester|Maryland|DO Ce 88|Cambridge||sediment core;rock core|1.5, 1.75|Core in good condition, some in 2 in steel tubes|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=383401076032001&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1454|DO Cf 34|25.0|||RSY10|DO Cf 34|0.0|approx. 6 feet of core from limited intervals from depths of 7.3 to 75.5 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0552|38.56567225|-75.88382434|Dorchester|Maryland|DO Cf 34|East New Market||sediment core||Core in fair condition, wrapped in plastic sheets|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=383356075530301&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1455|DO Df 12|25.0|||RSY10|DO Df 12|0.0|approx. 5 feet of core from limited intervals from depths of 46 to 400 feet.|Global Positioning System (GPS), Standard Positioning Service (SPS) or Precise Positioning Service (PPS)|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0553|38.49575|-75.95058333|Dorchester|Maryland|DO Df 12|Chicamacomico River||sediment core|1.5|Core in good condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=382945075570201&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1456|FR Bd Catoctin NP|25.0|||RSY09|FR Bd Catoctin NP|0.0|4 boxes of core from limited intervals from depths of 111 to 601 feet.|Reported|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:43:21|DAS03|WP0554|39.65454145|-77.46332152|Frederick|Maryland|FR Bd Catoctin NP|Blue Ridge Summit||rock core|2, 3|Core in fair to good condition|||||||||||||||||||||||||||||||||||||||||
1457|FR Cd SHA B-10 1345|25.0|||RSY09|FR Cd SHA B-10 1345|0.0|approx. 5 feet of core from depths of 4 to 9 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:43:21|DAS03|WP0555|39.51822783|-77.44198533|Frederick|Maryland|FR Cd SHA B-10 1345|Catoctin Furnace||rock core|2|Core in fair condition|||||||||||||||||||||||||||||||||||||||||
1458|FR Cd SHA B-13 1345|25.0|||RSY09|FR Cd SHA B-13 1345|0.0|approx. 5 feet of core from depths of 33.5 to 38.5 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:43:21|DAS03|WP0556|39.51986075|-77.43665672|Frederick|Maryland|FR Cd SHA B-13 1345|Catoctin Furnace||rock core|2|Core in fair condition|||||||||||||||||||||||||||||||||||||||||
1459|FR Cd SHA B-5 1346|25.0|||RSY09|FR Cd SHA B-5 1346|0.0|approx. 5 feet of core from depths of 9 to 14 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:43:21|DAS03|WP0557|39.5128642|-77.41760706|Frederick|Maryland|FR Cd SHA B-5 1346|Catoctin Furnace||rock core|2|Core in fair condition|||||||||||||||||||||||||||||||||||||||||
1460|FR Cd SHA B-6 1346|25.0|||RSY09|FR Cd SHA B-6 1346|0.0|approx. 5 feet of core from depths of 9 to 14 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:43:21|DAS03|WP0558|39.51340271|-77.41948752|Frederick|Maryland|FR Cd SHA B-6 1346|Catoctin Furnace||rock core|2|Core in fair condition|||||||||||||||||||||||||||||||||||||||||
1461|FR Cd SHA B-7 1346|25.0|||RSY09|FR Cd SHA B-7 1346|0.0|approx. 5 feet of core from depths of 19 to 24 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:43:21|DAS03|WP0559|39.51518607|-77.42269527|Frederick|Maryland|FR Cd SHA B-7 1346|Catoctin Furnace||rock core|2|Core in fair condition|||||||||||||||||||||||||||||||||||||||||
1462|FR Cd SHA B-8 1346|25.0|||RSY09|FR Cd SHA B-8 1346|0.0|approx. 5 feet of core from depths of 15.5 to 20.5 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:43:21|DAS03|WP0560|39.55275983|-77.41760209|Frederick|Maryland|FR Cd SHA B-8 1346|Catoctin Furnace||rock core|2|Core in fair condition|||||||||||||||||||||||||||||||||||||||||
1463|FR Cd SHA B-9b 1345|25.0|||RSY09|FR Cd SHA B-9b 1345|0.0|approx. 10 feet of core from depths of 29 to 39 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:43:21|DAS03|WP0561|39.52179603|-77.4293351|Frederick|Maryland|FR Cd SHA B-9b 1345|Catoctin Furnace||rock core|2|Core in fair condition|||||||||||||||||||||||||||||||||||||||||
1464|GA Bc G-50|25.0|||RSY09|GA Bc G-50|0.0|26 boxes of core from select intervals from depths of 7291 to 7579 feet.|Reported|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:43:21|DAS03|WP0562|39.61286359|-79.31003681|Garrett|Maryland|GA Bc G-50|McHenry||rock core|2.5|Core in fair to good condition|||||||||||||||||||||||||||||||||||||||||
1465|GA Fa 31|25.0|||RSY09|GA Fa 31|0.0|46 boxes of nearly continuous core from depths of 488 to 1131 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0563|39.26038355|-79.42893851|Garrett|Maryland|GA Fa 31|Table Rock||rock core|2|Core in fair to good condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=391539079254601&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1466|GA Fb 22|25.0|||RSY09|GA Fb 22|0.0|9 boxes of nearly continuous core from depths of 516.5 to 640 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0564|39.25843916|-79.41199318|Garrett|Maryland|GA Fb 22|Table Rock||rock core|1.75, 2|Core in good condition||http://www.mgs.md.gov/publications/report_pages/RI_41.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=391530079244401&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1467|GA Fb 23|25.0|||RSY09|GA Fb 23|0.0|3 boxes of nearly continuous core from depths of 461 to 495 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0565|39.25843916|-79.41199318|Garrett|Maryland|GA Fb 23|Table Rock||rock core|1.75|Core in good condition||http://www.mgs.md.gov/publications/report_pages/RI_41.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=391530079244402&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1468|GA Fb 24|25.0|||RSY09|GA Fb 24|0.0|4 boxes of core from limited intervals (some removed for analysis) from depths of 341 to 401 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0566|39.25843916|-79.41199318|Garrett|Maryland|GA Fb 24|Table Rock||rock core|1.75|Core in good condition||http://www.mgs.md.gov/publications/report_pages/RI_41.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=391530079244403&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1469|GA Fb 25|25.0|||RSY09|GA Fb 25|0.0|4 boxes of core from limited intervals (some removed for analysis) from depths of 121.5 to 181 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0567|39.25843916|-79.41199318|Garrett|Maryland|GA Fb 25|Table Rock||rock core|1.75|Core in good condition||http://www.mgs.md.gov/publications/report_pages/RI_41.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=391530079244404&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1470|GA Fb 26|25.0|||RSY09|GA Fb 26|0.0|two boxes of core from depths of 808 to 832 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0568|39.25371721|-79.40977094|Garrett|Maryland|GA Fb 26|Table Rock||rock core|2|Core in good condition||http://www.mgs.md.gov/publications/report_pages/RI_41.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=391513079243601&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1471|GA Fb Mettiki M-28|25.0|||RSY09|GA Fb Mettiki M-28|0.0|55 boxes of originally nearly continuous core (some  limited intervals removed for various analyses) from depths of 20 to 576 feet.|Interpolated from digital map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:43:21|DAS03|WP0569|39.30294892|-79.3817141|Garrett|Maryland|GA Fb Mettiki M-28|Table Rock||rock core|2|Core in fair to good condition|||||||||||||||||||||||||||||||||||||||||
1472|HA Dd 88|25.0|||RSY10|HA Dd 88|0.0|approx. 1.2 feet of core from depths of 40 to 41.2 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0570|39.41871927|-76.3146801|Harford|Maryland|HA Dd 88|Edgewood||sediment core|1.5|Core in good condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=392507076185401&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1473|HA Dd 89|25.0|||RSY10|HA Dd 89|0.0|approx. 1.7 feet of core from 4 intervals from depths of 140 to 211.7 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0571|39.42483045|-76.30217972|Harford|Maryland|HA Dd 89|Edgewood||sediment core|1.5|Core in good condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=392529076180901&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1474|HA Dd 91|25.0|||RSY10|HA Dd 91|0.0|approx. 2 feet of core from 5 intervals from depths of 20 to 124.8 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0572|39.45594185|-76.25051145|Harford|Maryland|HA Dd 91|Edgewood||sediment core|1.5|Core in good condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=392721076150301&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1475|HA De 130|25.0|||RSY09|HA De 130|0.0|approx. 33.5 feet of core from depths of 362.3 to 400 feet.|Reported|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:43:21|DAS03|WP0573|39.43677584|-76.2252326|Harford|Maryland|HA De 130|Perryman||rock core|2|Core in good condition||http://www.mgs.md.gov/publications/report_pages/RI_44.html|||||||||||||||||||||||||||||||||||||||
1476|HA De 131|25.0|||RSY09|HA De 131|0.0|approx. 28 feet of core (Denison sampler used at least in part) from depths of 375 to 441.3 feet.|Reported|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:43:21|DAS03|WP0574|39.43816478|-76.22356588|Harford|Maryland|HA De 131|Perryman||rock core|2, 3|Core in fair to good condition||http://www.mgs.md.gov/publications/report_pages/RI_44.html|||||||||||||||||||||||||||||||||||||||
1477|HA De 132|25.0|||RSY09|HA De 132|0.0|7 boxes of nearly continuous core from depths of 342 to 417.5 feet.|Reported|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:43:21|DAS03|WP0575|39.43844254|-76.22412146|Harford|Maryland|HA De 132|Perryman||rock core|2, 4|Core in good condition||http://www.mgs.md.gov/publications/report_pages/RI_44.html|||||||||||||||||||||||||||||||||||||||
1478|HA De 133|25.0|||RSY09|HA De 133|0.0|5 boxes of nearly continuous core from depths of 335 to 390 feet.|Reported|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:43:21|DAS03|WP0576|39.4376092|-76.22439925|Harford|Maryland|HA De 133|Perryman||rock core|4|Core in good condition||http://www.mgs.md.gov/publications/report_pages/RI_44.html|||||||||||||||||||||||||||||||||||||||
1479|HA De 134|25.0|||RSY09|HA De 134|0.0|7 boxes of nearly continuous core from depths of 322.2 to 393.2 feet.|Reported|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:43:21|DAS03|WP0577|39.43788702|-76.22273252|Harford|Maryland|HA De 134|Perryman||rock core|4|Core in good condition||http://www.mgs.md.gov/publications/report_pages/RI_44.html|||||||||||||||||||||||||||||||||||||||
1480|HA De 135|25.0|||RSY09|HA De 135|0.0|9 boxes of nearly continuous core from depths of 340 to 458 feet.|Reported|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:43:21|DAS03|WP0578|39.43677591|-76.22273251|Harford|Maryland|HA De 135|Perryman||rock core|3, 3.25, 3.5|Core in fair to good condition||http://www.mgs.md.gov/publications/report_pages/RI_44.html|||||||||||||||||||||||||||||||||||||||
1481|HA De 181|25.0|||RSY10|HA De 181|0.0|approx. 4.6 feet of core from select intervals from depths of 60 to 220.4 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0579|39.43510856|-76.24912239|Harford|Maryland|HA De 181|Perryman||sediment core|1.5|Core in good condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=392606076145801&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1482|HA De 195|25.0|||RSY10|HA De 195|0.0|approx. 3 feet of core from 4 intervals from depths of 64 to 135.8 feet.|Reported|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0580|39.48733284|-76.18384257|Harford|Maryland|HA De 195|Perryman||sediment core|1.5|Core in good condition||http://www.mgs.md.gov/publications/report_pages/RI_58.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=392914076110301&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1483|HA De 197|25.0|||RSY10|HA De 197|0.0|approx. 2.7 feet of core from 7 intervals from depths of 40 to 141.5 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0581|39.47205389|-76.21884372|Harford|Maryland|HA De 197|Perryman||sediment core|1.5|Core in good condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=392819076130901&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1484|HA De 198|25.0|||RSY10|HA De 198|0.0|approx. 2.4 feet of core from 3 intervals from depths of 15 to 26.9 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0582|39.47205389|-76.21884372|Harford|Maryland|HA De 198|Perryman||sediment core|1.5|Core in good condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=392819076130902&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1485|HA Dg 3|25.0|||RSY09|HA Dg 3|0.0|2 boxes of core from select intervals from depths of 757 to 777 feet.|Reported|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:43:21|DAS03|WP0583|39.44539114|-76.07050461|Harford|Maryland|HA Dg 3|Spesutie||rock core|1.75, 2|Core in fair condition||http://www.mgs.md.gov/publications/report_pages/RI_44.html|http://www.mgs.md.gov/publications/report_pages/OFR_12-02-20.html|http://www.mgs.md.gov/publications/report_pages/RI_30.html|||||||||||||||||||||||||||||||||||||
1486|HA Ec 46|25.0|||RSY10|HA Ec 46|0.0|approx. 1.2 feet of core from select intervals from depths of 40 to 48.3 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0584|39.4023302|-76.34995895|Harford|Maryland|HA Ec 46|Edgewood||sediment core|1.5|Core in good condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=392408076210101&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1487|HA Ec 47|25.0|||RSY10|HA Ec 47|0.0|approx. 1.8 feet of core from select intervals from depths of 5 to 118 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0585|39.4023302|-76.34995895|Harford|Maryland|HA Ec 47|Edgewood||sediment core|1.5|Core in good condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=392408076210102&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1488|HA Ed 47|25.0|||RSY10|HA Ed 47|0.0|approx. 0.3 feet of core from depths of 47 to 47.3 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0586|39.4153859|-76.32218033|Harford|Maryland|HA Ed 47|Edgewood||sediment core|1.5|Core in good condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=392455076192101&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1489|HA Ed 48|25.0|||RSY10|HA Ed 48|0.0|approx. 1.8 feet of core from select intervals from depths of 121 to 122.8 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0587|39.4153859|-76.32218033|Harford|Maryland|HA Ed 48|Edgewood||sediment core|1.5|Core in good condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=392455076192102&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1490|KE Bc 186|25.0|||RSY10|KE Bc 186|0.0|approx. 8 feet of core from 3 intervals from depths of 177 to 224 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0588|39.28066526|-76.08411422|Kent|Maryland|KE Bc 186|Betterton||sediment core||Core in fair condition, wrapped in plastic sheets|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=391650076050403&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1491|Ke Bc 187|25.0|||RSY10|Ke Bc 187|0.0|approx. 3.2 feet of core from 2 intervals from depths of 88 to 137 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0589|39.26872024|-76.1566173|Kent|Maryland|Ke Bc 187|Hanesville||sediment core||Core in fair to poor condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=391607076092501&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1492|KE Bd 171-173 pilot hole|25.0|||RSY10|KE Bd 171-173 pilot hole|0.0|approx. 6 feet of core in 2-foot segments from 3 intervals from depths of 25 to 37 feet.|Global Positioning System (GPS), Standard Positioning Service (SPS) or Precise Positioning Service (PPS)|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0590|39.28317778|-76.00485278|Kent|Maryland|KE Bd 171-173 pilot hole|Betterton||sediment core|1.75|Core in fair to poor condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=391659076001703&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1493|KE Bd 174-176 pilot hole|25.0|||RSY10|KE Bd 174-176 pilot hole|0.0|approx. 10 feet of core in 2-foot segments from 5 intervals from depths of 30 to 52 feet.|Global Positioning System (GPS), Standard Positioning Service (SPS) or Precise Positioning Service (PPS)|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0591|39.28342222|-76.00668889|Kent|Maryland|KE Bd 174-176 pilot hole|Betterton||sediment core|1.5|Core in fair to poor condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=391700076002403&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1494|KE Bd 177-179 pilot hole|25.0|||RSY10|KE Bd 177-179 pilot hole|0.0|3 boxes of core from select intervals from depths of 20 to 82 feet.|Global Positioning System (GPS), Standard Positioning Service (SPS) or Precise Positioning Service (PPS)|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0592|39.28376111|-76.00915278|Kent|Maryland|KE Bd 177-179 pilot hole|Betterton||sediment core|1.5|Core in fair to poor condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=391702076003303&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1495|KE Bd 183|25.0|||RSY10|KE Bd 183|0.0|7 boxes of nearly continuous core from depths of 0 to 62 feet.|Global Positioning System (GPS), Standard Positioning Service (SPS) or Precise Positioning Service (PPS)|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0593|39.28333333|-76.00483056|Kent|Maryland|KE Bd 183|Betterton||sediment core|1.5|Core in fair to good condition||https://pubs.er.usgs.gov/publication/70188285|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=391700076001701&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1496|KE Bd 185|25.0|||RSY10|KE Bd 185|0.0|5 boxes of nearly continuous core from depths of 0 to 36 feet.|Global Positioning System (GPS), Standard Positioning Service (SPS) or Precise Positioning Service (PPS)|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0594|39.28407222|-76.00876111|Kent|Maryland|KE Bd 185|Betterton||sediment core|1.5|Core in fair to good condition||https://pubs.er.usgs.gov/publication/70188285|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=391703076003201&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1497|KE Bd 186|25.0|||RSY10|KE Bd 186|0.0|4 boxes of nearly continuous core from depths of 0 to 36 feet.|Global Positioning System (GPS), Standard Positioning Service (SPS) or Precise Positioning Service (PPS)|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0595|39.28150833|-76.01040556|Kent|Maryland|KE Bd 186|Betterton||sediment core|1.5|Core in fair condition||https://pubs.er.usgs.gov/publication/70188285|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=391653076003701&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1498|KE Bd 34|25.0|||RSY10|KE Bd 34|0.0|approx. 6 feet of core in 2-foot segments from 3 intervals from depths of 10 to 37 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0596|39.27149863|-76.03827874|Kent|Maryland|KE Bd 34|Betterton||sediment core||Core in fair condition, wrapped in plastic sheets|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=391618076021601&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1499|KE Be 183|25.0|||RSY10|KE Be 183|0.0|9 boxes of core (variable recovery of continuous coring) from depths of 1 to 85 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0597|39.3084444|-75.96938731|Kent|Maryland|KE Be 183|Galena||sediment core|2.5|Core in good condition||https://pubs.er.usgs.gov/publication/70188285|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=391830075581101&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1500|KE Be 184|25.0|||RSY10|KE Be 184|0.0|11 boxes of core (variable recovery of continuous coring) from depths of 0 to 92 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0598|39.30399984|-75.9649426|Kent|Maryland|KE Be 184|Galena||sediment core|2.5|Core in fair to good condition||https://pubs.er.usgs.gov/publication/70188285|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=391814075575502&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1501|KE Be 185|25.0|||RSY10|KE Be 185|0.0|9 boxes of core (variable recovery of continuous coring) from depths of 0 to 95 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0599|39.32788933|-75.94994222|Kent|Maryland|KE Be 185|Galena||sediment core|2.5|Core in good condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=391940075570102&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1502|KE Be 186|25.0|||RSY10|KE Be 186|0.0|16 boxes of core (variable recovery of continuous coring) from depths of 0 to 130 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0600|39.30261093|-75.93105213|Kent|Maryland|KE Be 186|Galena||sediment core|2.5|Core in fair to good condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=391809075555301&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1503|KE Be 221|25.0|||RSY10|KE Be 221|0.0|15 boxes of core (variable recovery of continuous coring) from depths of 0 to 210 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:43:21|DAS03|WP0601|39.30261093|-75.93105213|Kent|Maryland|KE Be 221|Galena||sediment core|1.5|Core in poor to good condition|||||||||||||||||||||||||||||||||||||||||
1504|KE Bf 180|25.0|||RSY10|KE Bf 180|0.0|51 boxes of nearly continuous core from depths of 13 to 480 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0602|39.28455499|-75.9143845|Kent|Maryland|KE Bf 180|Galena||sediment core|2|Core in fair to good condition||http://www.mgs.md.gov/publications/report_pages/OFR_93-02-7.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=391706075545201&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1505|KE Bg 107|25.0|||RSY10|KE Bg 107|0.0|6 boxes of core from select intervals from depths of 5 to 330 feet.|Interpolated from digital map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0603|39.30413333|-75.797425|Kent|Maryland|KE Bg 107|Millington||sediment core|1.5|Core in poor to good condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=391814075475001&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1506|KE Cb 103|25.0|||RSY10|KE Cb 103|0.0|3 boxes of core from select intervals from depths of 110 to 391.2 feet.|Global Positioning System (GPS), Standard Positioning Service (SPS) or Precise Positioning Service (PPS)|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0604|39.18986111|-76.16836111|Kent|Maryland|KE Cb 103|Rock Hall||sediment core|1.5|Core in fair condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=391124076101005&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1507|KE Cc 132|25.0|||RSY10|KE Cc 132|0.0|approx. 14 feet of core in 2-foot segments from select intervals from depths of 10 to 142 feet.|Interpolated from digital map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:43:21|DAS03|WP0605|39.21058056|-76.09993611|Kent|Maryland|KE Cc 132|Chestertown||sediment core|1.5|Core in good condition|||||||||||||||||||||||||||||||||||||||||
1508|KE Cd 140|25.0|||RSY10|KE Cd 140|0.0|approx. 22 feet of core from select intervals from depths of 10 to 142 feet.|Interpolated from digital map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:43:21|DAS03|WP0606|39.23348333|-76.04004444|Kent|Maryland|KE Cd 140|Chestertown||sediment core|1.5|Core in good condition|||||||||||||||||||||||||||||||||||||||||
1509|KE Db 40|25.0|||RSY10|KE Db 40|0.0|4 boxes of core from 28 select intervals from depths of 60 to 1776.5 feet.|Global Positioning System (GPS), Standard Positioning Service (SPS) or Precise Positioning Service (PPS)|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0607|39.14377778|-76.23416667|Kent|Maryland|KE Db 40|Rock Hall||sediment core||Core in good condition, wrapped in plastic sheets|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=390837076140401&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1510|PG Cf 29|25.0|||RSY11|PG Cf 29|0.0|3 boxes of core from select intervals from depths of 752 to 1171 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:43:21|DAS03|WP0608|38.96286667|-76.74721389|Prince George's|Maryland|PG Cf 29|Bowie||sediment core;rock core|1.25|Core in good condition||http://www.mgs.md.gov/output/reports/BDR/BDR_13.pdf|||||||||||||||||||||||||||||||||||||||
1511|PG Df 35|25.0|||RSY10|PG Df 35|0.0|8 boxes of core from numerous intervals from depths of 15 to 200 feet.|Reported|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0609|38.88305556|-76.72416667|Prince George's|Maryland|PG Df 35|Bowie||sediment core|2.75|Core in fair condition||http://www.mgs.md.gov/publications/report_pages/OFR_77-02-1.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=385259076432701&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1512|PG Ed 48|25.0|||RSY10|PG Ed 48|0.0|13 boxes of approx. 54 feet of nearly continuous core from depths of 1385 to 1453 feet.|Reported|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:43:21|DAS03|WP0610|38.7559482|-76.85441583|Prince George's|Maryland|PG Ed 48|Upper Marlboro||sediment core|3|Core in good condition|||||||||||||||||||||||||||||||||||||||||
1513|PG Fc 34|25.0|||RSY10|PG Fc 34|0.0|approx. 19 feet of core from select intervals from depths of 1342 to 1399 feet.|Reported|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:43:21|DAS03|WP0611|38.70456054|-76.91691719|Prince George's|Maryland|PG Fc 34|Piscataway||sediment core|3|Core in fair to good condition|||||||||||||||||||||||||||||||||||||||||
1514|PG Fc 37|25.0|||RSY10|PG Fc 37|0.0|10 boxes of core from select intervals (some intervals poor condition) from depths of 1267 to 1345 feet.|Reported|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:43:21|DAS03|WP0612|38.69511636|-76.91858384|Prince George's|Maryland|PG Fc 37|Piscataway||sediment core|3|Core in poor to good condition|||||||||||||||||||||||||||||||||||||||||
1515|QA Be 15|25.0|||RSY10|QA Be 15|0.0|7 boxes of core from select intervals from depths of 60 to 1883 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0613|39.20094315|-76.04494493|Queen Anne|Maryland|QA Be 15|Chestertown||sediment core|1.5|Core in fair to good condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=391203076024301&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1516|QA Bg 53|25.0|||RSY10|QA Bg 53|0.0|a few feet of core (incl. some in Shelby tube) from select intervals from depths of 42 to 47 feet.|Reported|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:43:21|DAS03|WP0614|39.23622148|-75.85299244|Queen Anne|Maryland|QA Bg 53|Sudlersville||sediment core|3|Core in fair to poor condition (in shelby tube)||http://www.mgs.md.gov/publications/report_pages/OFR_77-02-1.html|||||||||||||||||||||||||||||||||||||||
1517|QA Bg 54|25.0|||RSY10|QA Bg 54|0.0|7 boxes of core plus a couple steel Shelby tube/Denison cores from select intervals from depths of 51 to 293 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0615|39.23622148|-75.85299244|Queen Anne|Maryland|QA Bg 54|Sudlersville||sediment core|3.5|Core in fair to poor condition||http://www.mgs.md.gov/publications/report_pages/OFR_77-02-1.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=391410075511201&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1518|QA Bg 55|25.0|||RSY10|QA Bg 55|0.0|2 feet of core from depths of 40 to 42 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0616|39.18983326|-75.83910263|Queen Anne|Maryland|QA Bg 55|Sudlersville||sediment core||Core in fair condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=391123075502201&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1519|QA Bg 56|25.0|||RSY10|QA Bg 56|0.0|2 feet of core from depths of 30 to 32 feet.|Interpolated from digital map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0617|39.18444444|-75.89277778|Queen Anne|Maryland|QA Bg 56|Church Hill||sediment core||Core in fair condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=391104075530601&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1520|QA Bg 57|25.0|||RSY10|QA Bg 57|0.0|2 feet of core from depths of 15 to 17 feet.|Interpolated from digital map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0618|39.20027778|-75.90166667|Queen Anne|Maryland|QA Bg 57|Church Hill||sediment core||Core in fair condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=391201075540401&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1521|QA Bh 44|25.0|||RSY10|QA Bh 44|0.0|4 feet of core (2-foot segments from 2 intervals) from depths of 30 to 45 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0619|39.17900028|-75.80437889|Queen Anne|Maryland|QA Bh 44|Sudlersville||sediment core||Core in fair condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=391044075481701&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1522|QA Bh 45|25.0|||RSY10|QA Bh 45|0.0|4 feet of core (2-foot segments from 2 intervals) from depths of 25 to 42 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0620|39.17427837|-75.76382163|Queen Anne|Maryland|QA Bh 45|Sudlersville||sediment core||Core in fair condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=391027075455101&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1523|QA Ce 39|25.0|||RSY10|QA Ce 39|0.0|2 boxes of core from select intervals from depths of 10 to 152 feet.|Interpolated from digital map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:43:21|DAS03|WP0621|39.13478333|-76.06876944|Queen Anne|Maryland|QA Ce 39|Chestertown||sediment core|1.5|Core in fair to good condition|||||||||||||||||||||||||||||||||||||||||
1524|QA Cf 63|25.0|||RSY10|QA Cf 63|0.0|8 feet of core (2-foot segments from 4 intervals) from depths of 35 to 72 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:52|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0622|39.0984448|-75.96160679|Queen Anne|Maryland|QA Cf 63|Price||sediment core||Core in fair condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=390554075574301&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1525|QA Cf 64|25.0|||RSY10|QA Cf 64|0.0|2 feet of core from depths of 35 to 37 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0623|39.14094448|-75.92493908|Queen Anne|Maryland|QA Cf 64|Church Hill||sediment core||Core in fair condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=390827075553101&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1526|QA Cg 59|25.0|||RSY10|QA Cg 59|0.0|8 feet of core (2-foot segments from 4 intervals) from depths of 35 to 67 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0624|39.13761135|-75.89827131|Queen Anne|Maryland|QA Cg 59|Church Hill||sediment core||Core in fair condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=390815075535501&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1527|QA Cg 60|25.0|||RSY10|QA Cg 60|0.0|2 feet of core from depths of 70 to 72 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0625|39.14455591|-75.86326995|Queen Anne|Maryland|QA Cg 60|Sudlersville||sediment core||Core in fair condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=390840075514901&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1528|QA Db 30|25.0|||RSY10|QA Db 30|0.0|4 feet of core from depths of 359 to 371 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0626|39.03372249|-76.30717813|Queen Anne|Maryland|QA Db 30|Love Point||sediment core|1.5|Core condition unknown||http://www.mgs.md.gov/publications/report_pages/RI_51.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=390201076182701&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1529|QA Db 31|25.0|||RSY10|QA Db 31|0.0|8.9 feet of core from depths of 170.6 to 317 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0627|39.03372249|-76.30717813|Queen Anne|Maryland|QA Db 31|Love Point||sediment core|1.5|Core condition unknown||http://www.mgs.md.gov/publications/report_pages/RI_51.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=390201076182702&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1530|QA Db 32|25.0|||RSY10|QA Db 32|0.0|2 feet of core from depths of 124 to 126 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0628|39.03372249|-76.30717813|Queen Anne|Maryland|QA Db 32|Love Point||sediment core|1.5|Core condition unknown||http://www.mgs.md.gov/publications/report_pages/RI_51.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=390201076182703&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1531|QA Db 33|25.0|||RSY10|QA Db 33|0.0|2 feet of core from depths of 309 to 311 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0629|39.00650065|-76.29495549|Queen Anne|Maryland|QA Db 33|Love Point||sediment core|1.5|Core condition unknown||http://www.mgs.md.gov/publications/report_pages/RI_51.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=390023076174303&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1532|QA Db 34|25.0|||RSY10|QA Db 34|0.0|4.7 feet of core from depths of 89 to 186 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0630|39.00650065|-76.29495549|Queen Anne|Maryland|QA Db 34|Love Point||sediment core|1.5, 3|Core condition unknown||http://www.mgs.md.gov/publications/report_pages/RI_51.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=390023076174301&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1533|QA Db 35|25.0|||RSY10|QA Db 35|0.0|4 feet of core from depths of 53 to 231 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0631|39.02205595|-76.3191229|Queen Anne|Maryland|QA Db 35|Love Point||sediment core|1.5|Core condition unknown||http://www.mgs.md.gov/publications/report_pages/RI_51.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=390119076191001&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1534|QA Dd 4H-1|25.0|||RSY10|QA Dd 4H-1|0.0|14 plastic tubes of nearly continuous core from depths of 0 to 80 feet.|Interpolated from digital map|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS03|WP0632|39.03068333|-76.11095278|Queen Anne|Maryland|QA Dd 4H-1|Centreville||sediment core|1.5||||||||||||||||||||||||||||||||||||||||||
1535|QA Dd WN-1|25.0|||RSY10|QA Dd WN-1|0.0|16 plastic tubes of nearly continuous core from depths of 0 to 80 feet.|Interpolated from digital map|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS03|WP0633|39.07292222|-76.11655833|Queen Anne|Maryland|QA Dd WN-1|Centreville||sediment core|1.5||||||||||||||||||||||||||||||||||||||||||
1536|QA De BFP-1|25.0|||RSY10|QA De BFP-1|0.0|16 plastic tubes of nearly continuous core from depths of 0 to 80 feet.|Interpolated from digital map|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS03|WP0634|39.06723333|-76.042675|Queen Anne|Maryland|QA De BFP-1|Centreville||sediment core|1.5||||||||||||||||||||||||||||||||||||||||||
1537|QA Df 53|25.0|||RSY10|QA Df 53|0.0|2 feet of core from depths of 40 to 42 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0635|39.07955605|-75.9782739|Queen Anne|Maryland|QA Df 53|Price||sediment core||Core in fair condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=390446075584301&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1538|QA Ea 77|25.0|||RSY10|QA Ea 77|0.0|6 feet of core from depths of 289 to 397 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0636|38.9551129|-76.35384487|Queen Anne|Maryland|QA Ea 77|Kent Island||sediment core|1.5|Core condition unknown||http://www.mgs.md.gov/publications/report_pages/RI_51.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=385718076211501&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1539|QA Ea 78|25.0|||RSY10|QA Ea 78|0.0|1.9 feet of core from depths of 90 to 135.3 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0637|38.9551129|-76.35384487|Queen Anne|Maryland|QA Ea 78|Kent Island||sediment core|1.5, 3|Core condition unknown||http://www.mgs.md.gov/publications/report_pages/RI_51.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=385718076211502&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1540|QA Ea 79|25.0|||RSY10|QA Ea 79|0.0|3.3 feet of core from depths of 60 to 281.3 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0638|38.96594599|-76.33328901|Queen Anne|Maryland|QA Ea 79|Kent Island||sediment core|1.5|Core condition unknown||http://www.mgs.md.gov/publications/report_pages/RI_51.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=385757076200101&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1541|QA Ea 80|25.0|||RSY10|QA Ea 80|0.0|1.4 feet of core from depths of 130 to 131.4 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0639|38.96594599|-76.33328901|Queen Anne|Maryland|QA Ea 80|Kent Island||sediment core|1.5|Core condition unknown||http://www.mgs.md.gov/publications/report_pages/RI_51.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=385757076200102&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1542|QA Ea 81|25.0|||RSY10|QA Ea 81|0.0|2 feet of core from depths of 267 to 269 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0640|38.9551129|-76.35384487|Queen Anne|Maryland|QA Ea 81|Kent Island||sediment core|1.5|Core condition unknown||http://www.mgs.md.gov/publications/report_pages/RI_51.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=385718076211503&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1543|QA Eb 110|25.0|||RSY10|QA Eb 110|0.0|2 boxes of core (limited core from 31 select intervals) from depths of 100 to 2530 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0641|38.96427946|-76.2874543|Queen Anne|Maryland|QA Eb 110|Kent Island||sediment core||Core in good condition, wrapped in plastic sheets|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=385751076171603&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1544|QA Eb 115|25.0|||RSY10|QA Eb 115|0.0|2 feet of core from depths of 40 to 42 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0642|38.97261265|-76.24995343|Queen Anne|Maryland|QA Eb 115|Queenstown||sediment core||Core in fair condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=385821076150101&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1545|QA Eb 153|25.0|||RSY10|QA Eb 153|0.0|3.5 feet of core from depths of 70.4 to 162 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0643|38.97872357|-76.26439846|Queen Anne|Maryland|QA Eb 153|Kent Island||sediment core|1.5, 3|Core condition unknown||http://www.mgs.md.gov/publications/report_pages/RI_51.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=385843076155301&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1546|QA Eb 156|25.0|||RSY10|QA Eb 156|0.0|2 feet of core from depths of 219 to 221 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0644|38.98122338|-76.33078935|Queen Anne|Maryland|QA Eb 156|Kent Island||sediment core|1.5|Core condition unknown||http://www.mgs.md.gov/publications/report_pages/RI_51.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=385852076195201&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1547|QA Eb 157|25.0|||RSY10|QA Eb 157|0.0|2 feet of core from depths of 45 to 47 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0645|38.98122338|-76.33078935|Queen Anne|Maryland|QA Eb 157|Kent Island||sediment core|1.5|Core condition unknown||http://www.mgs.md.gov/publications/report_pages/RI_51.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=385852076195202&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1548|QA Ec 84|25.0|||RSY10|QA Ec 84|0.0|1 foot of core from depths of 19.5 to 20.5 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0646|38.96733502|-76.22022952|Queen Anne|Maryland|QA Ec 84|Queenstown||sediment core||Core in fair condition, wrapped in plastic sheets|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=385802076131401&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1549|QA Ee 25|25.0|||RSY10|QA Ee 25|0.0|2 feet of core from depths of 40 to 42 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0647|38.93011329|-76.01105158|Queen Anne|Maryland|QA Ee 25|Wye Mills||sediment core||Core in fair condition, wrapped in plastic sheets|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=385548076004101&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1550|QA Ee 26|25.0|||RSY10|QA Ee 26|0.0|2 feet of core from depths of 30 to 32 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0648|38.93344661|-76.02521898|Queen Anne|Maryland|QA Ee 26|Wye Mills||sediment core||Core in fair condition, wrapped in plastic sheets|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=385600076013201&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1551|QA Ee 27|25.0|||RSY10|QA Ee 27|0.0|6 feet of core (2-foot segments from 3 intervals) from depths of 30 to 47 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0649|38.93789104|-76.05327599|Queen Anne|Maryland|QA Ee 27|Wye Mills||sediment core||Core in fair condition, wrapped in plastic sheets|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=385616076031301&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1552|QA Ef 28|25.0|||RSY10|QA Ef 28|0.0|2 feet of core from depths of 40 to 42 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0650|38.92428009|-75.95604952|Queen Anne|Maryland|QA Ef 28|Ridgely||sediment core||Core in fair condition, wrapped in plastic sheets|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=385527075572301&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1553|QA Ef 29|25.0|||RSY10|QA Ef 29|0.0|1 box of very limited core from 14 intervals from depths of 750 to 1685 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0651|38.9273356|-75.96077192|Queen Anne|Maryland|QA Ef 29|Ridgely||sediment core|1.5|Core in fair condition||http://www.mgs.md.gov/publications/report_pages/OFR_87-02-3.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=385534075573601&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1554|QA Ef 40|25.0|||RSY10|QA Ef 40|0.0|9 plastic tubes of nearly continuous core from depths of 0 to 64.5 feet.|Global Positioning System (GPS), Standard Positioning Service (SPS) or Precise Positioning Service (PPS)|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0652|38.96394444|-75.94644444|Queen Anne|Maryland|QA Ef 40|Ridgely||sediment core|1.5|Core in good condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=385750075564701&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1555|SM Df 84|25.0|||RSY10|SM Df 84|0.0|5 boxes of core from select intervals from depths of 115 to 2619 feet.|Global Positioning System (GPS), Standard Positioning Service (SPS) or Precise Positioning Service (PPS)|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0653|38.26311111|-76.45605556|St. Marys|Maryland|SM Df 84|Solomons Island||sediment core|1.5|Core in fair to poor condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=381548076272102&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1556|SO Af 16|25.0|||RSY10|SO Af 16|0.0|approx. 2 feet of core from depths of 11.5 to 13.5 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0654|38.28095325|-75.65075896|Sommerset|Maryland|SO Af 16|Eden||sediment core||Core in fair condition, wrapped in plastic sheets|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=381651075390401&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1557|SO Ce 95|25.0|||RSY10|SO Ce 95|0.0|3 boxes of core from limited intervals from depths of 120 to 1352 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0655|38.15789992|-75.70965019|Sommerset|Maryland|SO Ce 95|Princess Anne||sediment core||||http://www.mgs.md.gov/publications/report_pages/OFR_91-02-5.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=380921075423201&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1558|SO Dd 47|25.0|||RSY10|SO Dd 47|0.0|33 variable-length cores in half PVC tubes (plus some bagged samples) from select intervals from depths of 1109.1 to 4199 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0656|38.0159572|-75.82520937|Sommerset|Maryland|SO Dd 47|Marion||sediment core|3.5|Core in poor condition||http://www.mgs.md.gov/publications/report_pages/OFR_82-02-1.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=380057075493201&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1559|TA Ae WM 09-07|25.0|||RSY10|TA Ae WM 09-07|0.0|approx. 11.5 feet of core (poor to fair condition) from limited intervals from depths of 16 to 132 feet.|Interpolated from digital map|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS03|WP0657|38.935|-76.06277778|Talbot|Maryland|TA Ae WM 09-07|Wye Mills||sediment core|1.5|Core in fair to poor condition|||||||||||||||||||||||||||||||||||||||||
1560|TA Af 11|25.0|||RSY10|TA Af 11|0.0|2 feet of core from depths of 20 to 22 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0658|38.92344674|-75.96827214|Talbot|Maryland|TA Af 11|Ridgely||sediment core||Core in fair condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=385524075580701&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1561|TA Be 82|25.0|||RSY10|TA Be 82|0.0|2 feet of core from depths of 40 to 42 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0659|38.86094741|-76.00799527|Talbot|Maryland|TA Be 82|Easton||sediment core||Core in fair condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=385139076003001&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1562|TA Bf 81|25.0|||RSY10|TA Bf 81|0.0|4 feet of core (2-foot segments from 2 intervals) from depths of 50 to 62 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0660|38.88789151|-75.98577246|Talbot|Maryland|TA Bf 81|Ridgely||sediment core||Core in fair condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=385316075591001&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1563|TA Bf 82|25.0|||RSY10|TA Bf 82|0.0|2 feet of core from depths of 40 to 42 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0661|38.88011381|-75.99160591|Talbot|Maryland|TA Bf 82|Ridgely||sediment core||Core in fair condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=385248075593101&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1564|TA Bf 83|25.0|||RSY10|TA Bf 83|0.0|2 feet of core from depths of 35 to 37 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0662|38.8715028|-75.9985505|Talbot|Maryland|TA Bf 83|Fowling Creek||sediment core||Core in fair condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=385217075595602&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1565|TA Bf 99|25.0|||RSY10|TA Bf 99|0.0|approx. 2.5 feet of core from limited intervals from depths of 50 to 241 feet.|Global Positioning System (GPS), Standard Positioning Service (SPS) or Precise Positioning Service (PPS)|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0663|38.87305556|-75.99722222|Talbot|Maryland|TA Bf 99|Fowling Creek||sediment core|1.5|Core in good condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=385223075595001&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1566|VA 53T 58|25.0|||RSY10|VA 53T 58|0.0|limited core material in bags from 9 intervals from depths of 151 to 647 feet.|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS03|WP0664|38.63703802|-77.15386908|Fairfax|Virginia|VA 53T 58|Fort Belvoir||sediment core||Core in fair condition||http://www.mgs.md.gov/publications/report_pages/OFR_12-02-20.html|||||||||||||||||||||||||||||||||||||||
1567|VA 58H 4|25.0|||RSY10|VA 58H 4|0.0|limited core material in steel tubes from 9 intervals from depths of 248 to 1720 feet.|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:51:44|DAS03|WP0665|37.39194|-76.52389|Gloucester|Virginia|VA 58H 4|Gloucester||sediment core|2.25|Core in steel tubes||https://pubs.usgs.gov/pp/2006/1731/pp1731_download.htm|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=372331076312601&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1568|WI Bf 68|25.0|||RSY10|WI Bf 68|0.0|approx. 6 feet of core (2-foot segments from 3 intervals) from depths of 50 to 152 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0666|38.44456074|-75.51853338|Wicomico|Maryland|WI Bf 68|Delmar||sediment core||Core in fair condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=382640075310801&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1569|WI Bf 69|25.0|||RSY10|WI Bf 69|0.0|approx. 8 feet of core (2-foot segments from 4 intervals) from depths of 50 to 132 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0667|38.42150573|-75.56325729|Wicomico|Maryland|WI Bf 69|Delmar||sediment core||Core in fair condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=382517075334901&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1570|WI Bf 72|25.0|||RSY10|WI Bf 72|0.0|4 feet of core (2-foot segments from 2 intervals) from depths of 120 to 137 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0668|38.45483851|-75.55825736|Wicomico|Maryland|WI Bf 72|Delmar||sediment core||Core in fair condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=382717075333101&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1571|WI Cf 182|25.0|||RSY10|WI Cf 182|0.0|approx. 2 feet of core from depths of 150 to 152 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS03|WP0669|38.410125|-75.56681111|Wicomico|Maryland|WI Cf 182|Delmar||sediment core|1.25|Core in fair to poor condition||http://www.mgs.md.gov/publications/report_pages/BULL_31.html|||||||||||||||||||||||||||||||||||||||
1572|WI Cf 184|25.0|||RSY10|WI Cf 184|0.0|2 boxes of core containing core samples from approx. 34 intervals from depths of 10 to 282 feet.|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS03|WP0670|38.40428465|-75.55270137|Wicomico|Maryland|WI Cf 184|Delmar||sediment core|1.25|Core in fair to poor condition||http://www.mgs.md.gov/publications/report_pages/OFR_12-02-20.html|||||||||||||||||||||||||||||||||||||||
1573|WI De 73|25.0|||RSY10|WI De 73|0.0|approx. 5 feet of core from 3 intervals from depths of 50 to 95 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0671|38.30511928|-75.6307586|Wicomico|Maryland|WI De 73|Eden||sediment core||Core in fair condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=381818075375201&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1574|WI De 74|25.0|||RSY10|WI De 74|0.0|approx. 5 feet of core from 5 intervals from depths of 45.5 to 110 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0672|38.29206407|-75.64214771|Wicomico|Maryland|WI De 74|Eden||sediment core||Core in fair condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=381731075383301&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1575|WI De 75|25.0|||RSY10|WI De 75|0.0|approx. 6 feet of core from 3 intervals from depths of 20 to 97 feet.|Interpolated from map|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:41:08.000001|DAS03|WP0673|38.31539681|-75.62409183|Wicomico|Maryland|WI De 75|Salisbury||sediment core||Core in fair condition, wrapped in plastic sheets||http://www.mgs.md.gov/publications/report_pages/RI_40.html|||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=381855075372801&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1576|WI Df 59|25.0|||RSY10|WI Df 59|0.0|approx. 10 feet of core from depths of 771.8 and 782 feet remaining; originally more core from depths of 765 to 788 feet.|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS03|WP0674|38.33178437|-75.51047859|Wicomico|Maryland|WI Df 59|Salisbury||sediment core|3.5|Core in poor condition||http://www.mgs.md.gov/publications/report_pages/OFR_12-02-20.html|||||||||||||||||||||||||||||||||||||||
1577|WO Ae 23|25.0|||RSY10|WO Ae 23|0.0|approx. 3 feet of core from depths of 251 to 254 feet plus bags of core from a few limited intervals from depths of 0 to 254 feet.|Global Positioning System (GPS), Standard Positioning Service (SPS) or Precise Positioning Service (PPS)|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0675|38.43925|-75.29480556|Worchester|Maryland|WO Ae 23|Whaleysville||sediment core|3.5|Core in poor to unknown condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=382621075174201&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1578|WO Ae 24|25.0|||RSY10|WO Ae 24|0.0|approx. 3.5 feet of core from 2 depth intervals (11 to 13 feet and 177 to 179 feet) and bags of core from a few limited intervals from depths of 11 to 179 feet.|Global Positioning System (GPS), Standard Positioning Service (SPS) or Precise Positioning Service (PPS)|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0676|38.43922222|-75.29483333|Worchester|Maryland|WO Ae 24|Whaleysville||sediment core|3.5|Core in poor to unknown condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=382621075174202&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1579|WO Ae 25|25.0|||RSY10|WO Ae 25|0.0|approx. 2 feet of core from depths of 11.5 to 13.5 feet.|Global Positioning System (GPS), Standard Positioning Service (SPS) or Precise Positioning Service (PPS)|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0677|38.43922222|-75.29480556|Worchester|Maryland|WO Ae 25|Whaleysville||sediment core|3.5|Core in poor to unknown condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=382621075174203&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1580|WO Ah 37|25.0|||RSY10|WO Ah 37|0.0|approx. 9 feet of core in steel tubes of various lengths from limited intervals from depths of 53 to 489 feet.|Global Positioning System (GPS), Standard Positioning Service (SPS) or Precise Positioning Service (PPS)|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0678|38.44241667|-75.05111111|Worchester|Maryland|WO Ah 37|Assawoman Bay||sediment core|3.5|unknown|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=382635075030603&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1581|WO Cg OC Arprt 30-A geothermal|25.0|||RSY10|WO Cg OC Arprt 30-A geothermal|0.0|approx. 37 feet of core in half PVC tubes (poor condition) from limited intervals from depths of 535 to 1033 feet.|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS03|WP0679|38.30983723|-75.11851846|Worchester|Maryland|WO Cg OC Arprt 30-A geothermal|Ocean City||sediment core|3.5|Core in poor condition||https://www.osti.gov/scitech/servlets/purl/6031469-9tFH3s/native/|||||||||||||||||||||||||||||||||||||||
1582|WO De 36|25.0|||RSY10|WO De 36|0.0|approx. 2.5 feet of core (in steel tubes) from 3 intervals from depths of 90 to 208 feet.|Global Positioning System (GPS), Standard Positioning Service (SPS) or Precise Positioning Service (PPS)|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0680|38.24961111|-75.29288889|Worchester|Maryland|WO De 36|Public Landing||sediment core|3.5|unknown|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=381457075174101&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1583|WO Dg 21|25.0|||RSY10|WO Dg 21|0.0|approx. 6 feet of core (in steel tubes) from 5 intervals plus bags of core from a few limited intervals from depths of 31 to 331.67 feet.|Global Positioning System (GPS), Standard Positioning Service (SPS) or Precise Positioning Service (PPS)|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:00|DAS03|WP0681|38.24119444|-75.13633333|Worchester|Maryland|WO Dg 21|Tingles Island||sediment core|3.5|Core in poor to unknown condition|||||https://nwis.waterdata.usgs.gov/nwis/inventory/?site_no=381427075081102&agency_cd=USGS&amp||||||||||||||||||||||||||||||||||||
1584|BDR5-001|25.0|||RSY01|BDR5-001|0.0|Gas producer, shut in. Open file|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0682|39.70944444|-78.45944444|Allegany|Maryland|Phillips Petroleum Co. #1 Ridge "A"|Artemas|1966|lithologic log||||||||Jennings |at surface|Purcell lime |3901|Onondaga |4109|Oriskany |4238|Helderberg |4452|||||||||||||||||||||||||4650|981
1585|BDR5-002|25.0|||RSY02|BDR5-002|0.0|Gas test, dry hole. Open file|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0683|39.69972222|-78.46416667|Allegany|Maryland|Phillips Petroleum Co. #2 Ridge "A"|Artemas|1968|lithologic log||||||||Jennings |at surface|Onondaga |4279|Oriskany |4348|Helderberg |4560|Helderberg |4560|||||||||||||||||||||||||4605|825
1586|BDR5-003|25.0|||RSY02|BDR5-003|0.0|Gas test, dry hole. Open file|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0684|39.71722222|-78.45444444|Allegany|Maryland|Consolidated Gas Supply Corp. #1 Oscar Foor WN-1090      (Double Pine Unit)|Artemas|1968|lithologic log||||||||Jennings |at surface|Onondaga |4200|Lime |4230|Oriskany |4387|Mandata |4600|||||||||||||||||||||||||4650|866
1587|BDR5-004|25.0|||RSY02|BDR5-004|0.0|Gas test, dry hole. Open file|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0685|39.70472222|-78.49805556|Allegany|Maryland|Consolidated Gas Supply Corp. #1 William B. Yowell WN-1098      (Ridge Road Unit)|Artemas|1968|lithologic log||||||||Jennings |at surface|Onondaga |4980|Oriskany |5118|Helderberg |5250|||||||||||||||||||||||||||5380|1177
1588|BDR5-005|25.0|||RSY08|BDR5-005|0.0|Water well, abandoned. Slaughter (1962)|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0686|39.60888889|-78.81583333|Allegany|Maryland|Celanese Corporation of America|Cresaptown|1931|lithologic log||||||||Quaternary |at surface|Rose Hill |40|Tuscarora |498|Juniata |880|||||||||||||||||||||||||||952|655
1589|BDR5-006|25.0|||RSY02|BDR5-006|0.0|Gas test, dry hole. Open file|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0687|39.595|-78.76194444|Allegany|Maryland|Joyce Pipe Line Co. #1 Pittsburgh Plate Glass Co.      Works #7|Cresaptown|1964|lithologic log||||||||Jennings (Brallier) |at surface|Genessee-Harrell-Portage |808|Romney |919|Marcellus |1959|Onondaga |2056|Oriskany |2224|Helderberg |2425|||||||||||||||||||||2463|638
1590|BDR5-007|25.0|||RSY02|BDR5-007|0.0|Oil or gas test, dry hole. Amsden (1954) Reger (1924) Tucker (1936)|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0688|39.66555556|-78.78166667|Allegany|Maryland|Operator and lease names unknown. well referred to as "Narrows Test Well" or "Cumberland Well"|Cumberland|1905-1910|lithologic log||||||||Juniata (257 ft below base of Tuscarora)|at surface|Bottomed in Martinsburg||||||||||||||||||||||||||||||||2240|625
1591|BDR5-008|25.0|||RSY05|BDR5-008|0.0|Water well, not used. Clark, and others (1918)|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0689|39.67527778|-78.94388889|Allegany|Maryland|Town of Frostburg|Frostburg|?|lithologic log||||||||No log available.||||||||||||||||||||||||||||||||||1200|2460
1592|BDR5-009|25.0|||RSY05|BDR5-009|0.0|Stratigraphic test and water well, not used. Slaughter (1962) Toenges, and others (1949)|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0690|39.67361111|-78.9425|Allegany|Maryland|U.S. Bureau of Mines Drill hole GC-21|Frostburg|1946|lithologic log||||||||Conemaugh |at surface|Allegheny-Pottsville |621|Mauch Chunk |998|||||||||||||||||||||||||||||1030|2415
1593|BDR5-010|25.0|||RSY06|BDR5-010|0.0|Stratigraphic test. Slaughter (1962) Toenges, and others (1949)|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0691|39.6475|-78.95833333|Allegany|Maryland|U.S. Bureau of Mines Drill hole GC-10|Frostburg|1946|lithologic log||||||||Conemaugh |at surface|Allegheny-Pottsville |784|||||||||||||||||||||||||||||||1081|2165
1594|BDR5-011|25.0|||RSY06|BDR5-011|0.0|Stratigraphic test. Slaughter (1962) Toenges, and others (1949)|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0692|39.60222222|-78.90472222|Allegany|Maryland|U.S. Bureau of Mines Drill hole GC-11|Lonaconing|1946|lithologic log||||||||Conemaugh |at surface|Allegheny-Pottsville |687|||||||||||||||||||||||||||||||1011|2420
1595|BDR5-012|25.0|||RSY08|BDR5-012|0.0|Stratigraphic test and water well, abandoned. Slaughter (1962)|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0693|39.57055556|-78.92111111|Allegany|Maryland|Lonaconing Water Co.|Lonaconing|deepened in 1954|lithologic log||||||||Allegheny and/or Pottsville |at surface|Mauch Chunk |648|||||||||||||||||||||||||||||||1354|2100
1596|BDR5-013|25.0|||RSY06|BDR5-013|0.0|Stratigraphic test. Slaughter (1962) roenges, and others (1949)|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0694|39.55194444|-78.97388889|Allegany|Maryland|U.S. Bureau of Mines Drill hole GC-6|Lonaconing|1946|lithologic log||||||||Conemaugh |at surface|Allegheny-Pottsville |670|Mauch Chunk |1172|||||||||||||||||||||||||||||1215|1770
1597|BDR5-014|25.0|||RSY06|BDR5-014|0.0|Stratigraphic test. Slaughter (1962) roenges, and others (1949)|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0695|39.58027778|-78.96833333|Allegany|Maryland|U.S. Bureau of Mines Drill hole GC-26|Lonaconing|1946|lithologic log||||||||Conemaugh |at surface|Allegheny-Pottsville |754|||||||||||||||||||||||||||||||1050|1586
1598|BDR5-015|25.0|||RSY05|BDR5-015|0.0|Stratigraphic test and water well. Slaughter (1962)|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0696|39.47333333|-79.0575|Allegany|Maryland|West Virginia Pulp and Paper Co.|Westernport|1945|lithologic log||||||||Recent fill |at surface|Quaternary alluvium |10|Allegheny-Pottsville |24|Mauch Chunk |271|Greenbrier |927|Pocono |1293|||||||||||||||||||||||2379|941
1599|BDR5-016|25.0|||RSY06|BDR5-016|0.0|Stratigraphic test. Brookhart (1949) Otton (1955)|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0697|38.98472222|-76.4725|Anne Arundel|Maryland|U.S. Navy Ship Research and Development Center (U.S. Navy Experiment Station)|Annapolis|1948|lithologic log||||||||Not reported |0-116 feet|Aquia, Monmouth, and Matawan |116|Magothy |210|Raritan and Patapsco |254|||||||||||||||||||||||||||1000|36
1600|BDR5-017|25.0|||RSY06|BDR5-017|0.0|Stratigraphic test. Hansen (1968) Mack (1962)|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0698|39.05722222|-76.49722222|Anne Arundel|Maryland|Anne Arundel County Department of Public Works|Gibson Island|1954|lithologic log||||||||Monmouth-Matawan |at surface|Magothy |80|Potomac |160?|||||||||||||||||||||||||||||1008|58
1601|BDR5-018|25.0|||RSY05|BDR5-018|0.0|Stratigraphic test and water well. Hansen (19.68) Mack (1962)|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0699|39.04638889|-76.75027778|Anne Arundel|Maryland|U.S. Army, Fort George G. Meade|Laurel|1959|lithologic log||||||||Patapsco |at surface|Arundel |385|Patuxent |565|Basement |655?|||||||||||||||||||||||||||659|170
1602|BDR5-019|25.0|||RSY05|BDR5-019|0.0|Water well. Hansen (1968) Mack (1962)|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0700|39.07305556|-76.69666667|Anne Arundel|Maryland|Anne Arundel County Department of Public Works|Odenton|1962|lithologic log||||||||Patapsco |at surface|Arundel |510|Patuxent |670|Basement |910|||||||||||||||||||||||||||915|178
1603|BDR5-020|25.0|||RSY06|BDR5-020|0.0|Stratigraphic test.      Located 25 feet from production      well (no. 21). Open file|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0701|39.00277778|-76.69916667|Anne Arundel|Maryland|Crofton Corporation|Odenton|1963|lithologic log||||||||See log for well no. |21|||||||||||||||||||||||||||||||||1069|53
1604|BDR5-021|25.0|||RSY05|BDR5-021|0.0|Water well. Hansen (1968) Mack (1966)|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0702|39.00277778|-76.69916667|Anne Arundel|Maryland|Crofton Corporation Production well #1|Odenton|1964|lithologic log||||||||Magothy |at surface|Patapsco|90|Arundel|610|Patuxent|820|||||||||||||||||||||||||||1058|53
1605|BDR5-022|25.0|||RSY08|BDR5-022|0.0|Two water wells, now covered. Clark, and others (1918)|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0703|39.14277778|-76.77777778|Anne Arundel|Maryland|State of Maryland House of Correction (two wells, side by side)|Savage|1907|lithologic log||||||||Basement encountered in both wells||||||||||||||||||||||||||||||||||675|225
1606|BDR5-023|25.0|||RSY06|BDR5-023|0.0|Stratigraphic test. Hansen (1968)|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0704|38.98777778|-76.56305556|Anne Arundel|Maryland|City of Annapolis Annapolis Water Works|South River|1965|lithologic log||||||||Aquia-Brightseat |at surface|Monmouth-Matawan|120|Magothy|225|Potomac|380|||||||||||||||||||||||||||1054|80
1607|BDR5-024|25.0|||RSY06|BDR5-024|0.0|Stratigraphic test. Open file|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0705|39.25666667|-76.41555556|Baltimore|Maryland|Baltimore County Department of Recreation and Parks|Middle River|1970|lithologic log||||||||Pleistocene |at surface|Potomac Group |60|Bottomed in basement||||||||||||||||||||||||||||||792|20
1608|BDR5-025|25.0|||RSY08|BDR5-025|0.0|Water well, abandoned. Bennett and Meyer (1952) Hansen (1968)|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0706|39.23222222|-76.49305556|Baltimore|Maryland|Bethlehem Steel Co.|Sparrows Point|1940|lithologic log||||||||Pleistocene |at surface|Patapsco |73|Arundel |261|Patuxent |418|Basement |658|||||||||||||||||||||||||711|10
1609|BDR5-026|25.0|||RSY05|BDR5-026|0.0|Water well, never used. Dingman and Ferguson (1956) Laughlin (1966)|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0707|39.42777778|-76.62416667|Baltimore|Maryland|Walter Weisbrod (Lutherville Municipal Water Supply)|Towson|1910|lithologic log||||||||Cockeysville Marble, surface to bottom||||||||||||||||||||||||||||||||||1800|350
1610|BDR5-027|25.0|||RSY08|BDR5-027|0.0|Water well, abandoned. Clark, and others (1918)|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0708|39.27805556|-76.57777778|Baltimore City|Maryland|J.S. Young Co.|Baltimore East|1907|lithologic log||||||||Bottomed in basement.||No log available.||||||||||||||||||||||||||||||||1000|5
1611|BDR5-028|25.0|||RSY08|BDR5-028|0.0|Water well, now covered. Clark, and others (1918)|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0709|39.28916667|-76.635|Baltimore City|Maryland|American Ice Co.|Baltimore West|?|lithologic log||||||||Patuxent |at surface|Basement - hard granite |60|softer granite |600|soft granite |750|||||||||||||||||||||||||||1017|75
1612|BDR5-029|25.0|||RSY05|BDR5-029|0.0|Water well, Bennett and Meyer (1952)|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0710|39.28083333|-76.59805556|Baltimore City|Maryland|Mutual Chemical Co.|Baltimore East|1898|lithologic log||||||||Bottomed in basement.||No log available.||||||||||||||||||||||||||||||||1000|8
1613|BDR5-030|25.0|||RSY08|BDR5-030|0.0|Water well, abandoned. Bennett and Meyer (1952)|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0711|39.30277778|-76.61583333|Baltimore City|Maryland|Belvedere Hotel|Baltimore East|?|lithologic log||||||||Hard rock at 40 feet (Basement ?)||No log available.||||||||||||||||||||||||||||||||1105|100
1614|BDR5-031|25.0|||RSY08|BDR5-031|0.0|Water well, now covered. Exact location unknown. Bennett and Meyer (1952) Clark, and others (1918)|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0712|39.30944444|-76.58722222|Baltimore City|Maryland|American Brewery, Inc. (Weissner's Brewery)|Baltimore East|1907|lithologic log||||||||Bottomed in basement.||No log available.||||||||||||||||||||||||||||||||1500|140
1615|BDR5-032|25.0|||RSY08|BDR5-032|0.0|Water well, now covered. Exact location unknown. Bennett and Meyer (1952) Clark, and others (1918)|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0713|39.30944444|-76.58722222|Baltimore City|Maryland|American Brewery, Inc. (Weissner's Brewery)|Baltimore East|1907|lithologic log||||||||Bottomed in basement||No log available.||||||||||||||||||||||||||||||||3000|140
1616|BDR5-033|25.0|||RSY08|BDR5-033|0.0|Water well, abandoned as a failure. Exact location unknown. Open file|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0714|39.30944444|-76.58722222|Baltimore City|Maryland|J.F. Wessner and Sons Brewery|Baltimore East|1908|lithologic log||||||||No log available.||||||||||||||||||||||||||||||||||2379|140
1617|BDR5-034|25.0|||RSY08|BDR5-034|0.0|Water well, abandoned as a failure. Exact location unknown. Open file|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0715|39.30944444|-76.58722222|Baltimore City|Maryland|J.F. Wessner and Sons Brewery|Baltimore East|1909|lithologic log||||||||No log available.||||||||||||||||||||||||||||||||||1000|140
1618|BDR5-035|25.0|||RSY05|BDR5-035|0.0|Water well, now filled. Bennett and Meyer (1952)|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0716|39.31972222|-76.60472222|Baltimore City|Maryland|Fairfield Western Maryland Dairy|Baltimore East|1940|lithologic log||||||||Fill, Pleistocene, and weathered basement |at surface|Basement - granite |44|mica rock |200|granite |360|mica rock |385|white flint rock |435|white limestone |485|hard black rock |770|||||||||||||||||||790|140
1619|BDR5-036|25.0|||RSY08|BDR5-036|0.0|Water well, now covered. Exact location unknown. Bennett and Meyer (1952)|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0717|39.32027778|-76.60416667|Baltimore City|Maryland|Fairfield Western Maryland Dairy|Baltimore East|1940|lithologic log||||||||Pleistocene and weathered basement |at surface|Basement - granite |55|mica rock |187|granite |340|mica rock |360|white flint |420|granite |460|white limestone |510|||||||||||||||||||864|160
1620|BDR5-037|25.0|||RSY05|BDR5-037|0.0|Water well, plugged to 800 feet. Exact location unknown . Bennett and Meyer (1952) Clark, and others (1918)|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0718|39.32027778|-76.56944444|Baltimore City|Maryland|Brehm Brewery|Baltimore East|Before 1896|lithologic log||||||||Bottomed in basement||No log available.||||||||||||||||||||||||||||||||1500|140
1621|BDR5-038|25.0|||RSY08|BDR5-038|0.0|Water well, abandoned. Exact location unknown. Bennett and Meyer (1952) Darton (1896), (1902), (1905)|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0719|39.32027778|-76.56944444|Baltimore City|Maryland|Brehm Brewery|Baltimore East|Before 1896|lithologic log||||||||Yellow clay |at surface|Rock (basement?) |55|No log available.||||||||||||||||||||||||||||||1300|140
1622|BDR5-039|25.0|||RSY06|BDR5-039|0.0|Stratigraphic test. Weigle and Webb (1970) Weigle, and others (1970)|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0720|38.55472222|-76.58527778|Calvert|Maryland|U.S. Geological Survey Prince Frederick Test Well|Prince Frederick|1966|lithologic log||||||||Pleistocene |at surface|Chesapeake Group |20|Nanjemoy |225|Aquia-Brightseat |470|Monmouth-Matawan |690|Magothy |795|Potomac Group |885|||||||||||||||||||||1515|130
1623|BDR5-040|25.0|||RSY05|BDR5-040|0.0|Water well. Rasmussen and Slaughter (1957)|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0721|38.88611111|-75.84166667|Caroline|Maryland|Caroline Poultry Farms, Inc.|Denton|1953|lithologic log||||||||Pleistocene |at surface|St. Marys |40|Choptank |82|Calvert |192|Piney Point |331|Nanjemoy |488|Aquia |522|Brightseat |609|Monmouth -Matawan |853|||||||||||||||||980|18
1624|BDR5-041|25.0|||RSY08|BDR5-041|0.0|Water well, abandoned. Clark, and others (1918) Meyer (1958)|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0722|39.3775|-76.95916667|Carroll|Maryland|Springfield State Hospital|Finksburg|1911|lithologic log||||||||Wissahickon Schist, surface to bottom||||||||||||||||||||||||||||||||||500-505|490
1625|BDR5-042|25.0|||RSY08|BDR5-042|0.0|Water well, abandoned. Clark, and others (1918) Meyer (1958)|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0723|39.3775|-76.95916667|Carroll|Maryland|Springfield State Hospital|Finksburg|1915|lithologic log||||||||Wissahickon Schist, surface to bottom||||||||||||||||||||||||||||||||||550|490
1626|BDR5-043|25.0|||RSY05|BDR5-043|0.0|Water well. Meyer (1958)|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0724|39.665|-76.87138889|Carroll|Maryland|Town of Manchester Well #3|Lineboro|1930's|lithologic log||||||||Wissahickon Schist, surface to bottom||||||||||||||||||||||||||||||||||645|960
1627|BDR5-044|25.0|||RSY08|BDR5-044|0.0|Water well, abandoned. Meyer (1958)|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0725|39.53472222|-77.10111111|Carroll|Maryland|Edward Derr|New Windsor|1939|lithologic log||||||||Sams Creek Metabasalt, surface to bottom||||||||||||||||||||||||||||||||||1033|585
1628|BDR5-045|25.0|||RSY04|BDR5-045|0.0|Oil or gas test. Log from samples in MGS storage library. Open file|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0726|39.60555556|-77.23472222|Carroll|Maryland|R. H, Sheppard - Donelson Co. #1 Roser, et al.|Union Bridge|1962|lithologic log||||||||Triassic New Oxford |at surface|Basal limestone cgl. |950|Green phyllite (weathered near top) (Harpers?) |1000|Black quartzite (Antietam?) |4500|Argillaceous limestone (Frederick?) |5200|||||||||||||||||||||||||6230|472
1629|BDR5-046|25.0|||RSY08|BDR5-046|0.0|Water well, abandoned. Meyer (1958)|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0727|39.57638889|-77.17666667|Carroll|Maryland|Carroll County Board of Education Elmer A. Wolfe School|Union Bridge|1953|lithologic log||||||||Wakefield Marble, surface to bottom||||||||||||||||||||||||||||||||||575|440
1630|BDR5-047|25.0|||RSY08|BDR5-047|0.0|Water well, abandoned. Meyer (1958)|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0728|39.57888889|-76.99305556|Carroll|Maryland|Koontz Creamery|Westminister|1947 deepened in 1955|lithologic log||||||||Wakefield Marble |at surface|Sams Creek Metabasalt (Blue and green schist and interbedded white marble) |160|||||||||||||||||||||||||||||||850|695
1631|BDR5-048|25.0|||RSY05|BDR5-048|0.0|Water well Meyer (1958)|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0729|39.57888889|-76.99305556|Carroll|Maryland|Shriver Packing Co.|Westminister|1938|lithologic log||||||||Encountered Sams Creek Metabasalt, Wakefield Marble, and possibly Wissahickon Schist.||||||||||||||||||||||||||||||||||885|695
1632|BDR5-049|25.0|||RSY08|BDR5-049|0.0|Water well, abandoned Meyer (1958)|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0730|39.57944444|-76.99333333|Carroll|Maryland|Koontz Creamery|Westminister|Before 1939|lithologic log||||||||Encountered Sams Creek Metabasalt and Wakefield Marble.||||||||||||||||||||||||||||||||||822|695
1633|BDR5-050|25.0|||RSY05|BDR5-050|0.0|Water well. Open file|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0731|39.47277778|-75.98277778|Cecil|Maryland|Maryland Department of Forests and Parks Elk Neck State Park|Earleville|1968|lithologic log||||||||Pleistocene |at surface|Potomac Group |12|(Believed to have bottomed very close to basement)||||||||||||||||||||||||||||||528|82
1634|BDR5-051|25.0|||RSY06|BDR5-051|0.0|Stratigraphic test Sundstrum, and others (1967)|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0732|39.53861111|-75.79833333|Cecil|Maryland|B. F. Goodrich Co.|Elkton|1966|lithologic log||||||||Pleistocene |at surface|Potomac Group |65|Basement |655|||||||||||||||||||||||||||||695|65
1635|BDR5-052|25.0|||RSY08|BDR5-052|0.0|Water well, now covered. Otton (1955) Overbeck (1948) Slaughter and Laughlin (1966)|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0733|38.585|-77.16944444|Charles|Maryland|U. S. Naval Propellant Plant|Indian Head|1920|lithologic log||||||||Pleistocene |at surface|Potomac Group |15|Basement |709|||||||||||||||||||||||||||||1200|26
1636|BDR5-053|25.0|||RSY02|BDR5-053|0.0|Oil or gas test, dry hole Open file|Reported|WJUNKIN|2021-08-19 16:38:53|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0734|38.62|-76.98833333|Charles|Maryland|Coastal Petroleum Co., Inc. #1 Osborn|La Plata|1954|lithologic log||||||||Pleistocene |at surface|Calvert and Nanjemoy |24|Marlboro |204|Aquia-Brightseat |240|Monmouth-Matawan |345|Magothy |372|Potomac |412|||||||||||||||||||||492|215
1637|BDR5-054|25.0|||RSY06|BDR5-054|0.0|Stratigraphic test. Hansen (1968) Slaughter and Laughlin (1966) Slaughter and Otton (1968)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0735|38.61166667|-76.91027778|Charles|Maryland|St. Charles Utility Co.|La Plata|1965|lithologic log||||||||Pleistocene |at surface|Calvert |34|Nanjemoy |167|Aquia |269|Monmouth |384|Magothy |433|Raritan |505|Raritan-Patapsco |635|Patuxent |902|||||||||||||||||935|210
1638|BDR5-055|25.0|||RSY05|BDR5-055|0.0|Water well. Dryden and Overbeck (1948) Otton (1955) Overbeck (1948) Slaughter and Laughlin (1966) Slaughter and Otton (1968)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0736|38.5325|-76.96916667|Charles|Maryland|Town of La Plata|La Plata|1947|lithologic log||||||||Pleistocene |at surface|Calvert |19|Nanjemoy |75|Marlboro clay |190|Aquia |210|Cretaceous |380|||||||||||||||||||||||1094|149
1639|BDR5-056|25.0|||RSY05|BDR5-056|0.0|Water well. Slaughter and Laughlin (1966) Slaughter and Otton (1968)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0737|38.54361111|-76.94944444|Charles|Maryland|U. S. Army Radio Receiving Station Well #3|La Plata|1959|lithologic log||||||||Pleistocene |at surface|Chesapeake Group |50|Nanjemoy|?|Aquia-Brightseat |290|Potomac Group |455|||||||||||||||||||||||||1219|197
1640|BDR5-057|25.0|||RSY05|BDR5-057|0.0|Water well. Hansen (1968) Slaughter and Laughlin (1966) Slaughter and Otton (1968)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0738|38.53166667|-76.98027778|Charles|Maryland|Town of La Plata|La Plata|1964|lithologic log||||||||Pleistocene |at surface|Calvert |19|Nanjemoy |96|Aquia |260|Raritan |394|Patapsco-Arundel |480|Patuxent |1003|||||||||||||||||||||1252|165
1641|BDR5-058|25.0|||RSY05|BDR5-058|0.0|Water well. Slaughter and Laughlin (1966) Slaughter and Otton (1968)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0739|38.41833333|-77.00083333|Charles|Maryland|Loyola Retreat House|Mathias Point|1959|lithologic log||||||||Chesapeake Group |at surface|Nanjemoy|?|Aquia-Brightseat |205|Potomac Group |350|||||||||||||||||||||||||||990|97
1642|BDR5-059|25.0|||RSY06|BDR5-059|0.0|Stratigraphic test. Glaser (1968)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0740|38.36416667|-76.97277778|Charles|Maryland|Potomac Electric Power Co.|Colonial Beach North|1967|lithologic log||||||||Pleistocene |at surface|Nanjemoy |30|Aquia-Brightseat |205|Potomac Group |315|||||||||||||||||||||||||||1152|21
1643|BDR5-060|25.0|||RSY02|BDR5-060|0.0|Oil or gas test, dry hole. Kept open as artesian water well. Open file|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0741|38.58916667|-77.02777778|Charles|Maryland|Coastal Petroleum Co., Inc. #1 Willett|Port Tobacco|1954|lithologic log||||||||Pleistocene |at surface|Calvert-Nanjemoy |30|Aquia |210|Raritan-Patapsco |335|Patuxent |824|||||||||||||||||||||||||1117|194
1644|BDR5-061|25.0|||RSY05|BDR5-061|0.0|Water well. Hansen (1968) Slaughter and Laughlin (1966) Slaughter and Otton (1968)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0742|38.57694444|-77.03222222|Charles|Maryland|U. S. Army Military Reservation|Port Tobacco|1955|lithologic log||||||||Pleistocene |at surface|Calvert |14|Nanjemoy |82|Aquia |195|Upper Cretaceous (undiff.) |305|Raritan and Patapsco |375|Patuxent |727|||||||||||||||||||||1003|175
1645|BDR5-062|25.0|||RSY05|BDR5-062|0.0|Water well Open file|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0743|38.55805556|-77.05777778|Charles|Maryland|Pennco, Inc.|Port Tobacco|1968|lithologic log||||||||Pleistocene |at surface|Chesapeake Group |15|Nanjemoy |70|Aquia-Brightseat |195|Potomac Group |320|||||||||||||||||||||||||1334|190
1646|BDR5-063|25.0|||RSY05|BDR5-063|0.0|Water well. Rasmussen and Slaughter (1957)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0744|38.58861111|-76.09833333|Dorchester|Maryland|Mrs. P. P. Payne|Cambridge|1938|lithologic log||||||||No log available.||||||||||||||||||||||||||||||||||978|20
1647|BDR5-064|25.0|||RSY05|BDR5-064|0.0|Water well. Rasmussen and Slaughter (1957)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0745|38.5625|-76.075|Dorchester|Maryland|Crystal Ice and Cold Storage Co.|Cambridge|1945|lithologic log||||||||Pleistocene |at surface|Choptank |31|Calvert |145|Piney Point |359|Nanjemoy |515|Paleocene |580|Monmouth |754|Matawan |796|Magothy |926|||||||||||||||||966|18
1648|BDR5-065|25.0|||RSY05|BDR5-065|0.0|Water well. Rasmussen and Slaughter (1957)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0746|38.565|-76.06833333|Dorchester|Maryland|City of Cambridge|Cambridge|1946|lithologic log||||||||Pleistocene |at surface|Choptank |26|Calvert |112|Piney Point |366|Nanjemoy |485|Paleocene |590|Monmouth |760|Matawan |809|Magothy |908|Raritan |971|||||||||||||||977|15
1649|BDR5-066|25.0|||RSY05|BDR5-066|0.0|Water well, now used as observation well. Rasmussen and Slaughter (1957)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0747|38.56916667|-76.07305556|Dorchester|Maryland|Crystal Ice and Cold Storage Co.|Cambridge|1947|lithologic log||||||||Recent fill (?) |at surface|Pleistocene |5|Choptank |21|Calvert |74|Piney Point |351|Nanjemoy |494|Paleocene |600|Monmouth |724|Matawan |795|Magothy |935|||||||||||||||973|6
1650|BDR5-067|25.0|||RSY06|BDR5-067|0.0|Stratigraphic test. Hansen (1968) Mack and Otton (1969)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0748|38.56138889|-76.04277778|Dorchester|Maryland|U. S. Geological Survey Eastern Shore State Hospital Test Well|Cambridge|1965|lithologic log||||||||Pleistocene |at surface|Chesapeake Group |20|Piney Point-Nanjemoy |360|Aquia-Brightseat |700|Monmouth-Matawan |840|Magothy |915|Potomac Group |970|||||||||||||||||||||1488|20
1651|BDR5-068|25.0|||RSY05|BDR5-068|0.0|Water well. Rasmussen and Slaughter (1957)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0749|38.60444444|-76.14138889|Dorchester|Maryland|Dr. Eugene F. Traub|Church Creek|1946|lithologic log||||||||Pleistocene |at surface|Choptank-Calvert |30|Piney Point |320|Nanjemoy |390|Paleocene |540|Monmouth |714|Matawan |748|Magothy |924|Raritan-Patapsco |997|||||||||||||||||1041|15
1652|BDR5-069|25.0|||RSY05|BDR5-069|0.0|Water well. Rasmussen and Slaughter (1957)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0750|38.50222222|-76.15388889|Dorchester|Maryland|E. B. Jones|Church Creek|1935|lithologic log||||||||No log available.||||||||||||||||||||||||||||||||||934|5
1653|BDR5-070|25.0|||RSY06|BDR5-070|0.0|Stratigraphic test. Open file|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0751|39.65444444|-77.46361111|Frederick|Maryland|U. S. Army Catoctin Mountain Recreation Area core test|Blue Ridge Summit|?|lithologic log||||||||Catoctin Metabasalt cored surface to bottom||||||||||||||||||||||||||||||||||600|1785
1654|BDR5-071|25.0|||RSY05|BDR5-071|0.0|Drilled originally to 1000 feet as an oil test well, known as the "Annie Laurie well." Redrilled to 400 feet by town of Thurmont and used as a water well. Meyer (1958) Open file|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0752|39.625|-77.41722222|Frederick|Maryland|Town of Thurmont|Catoctin Furnace|1921|lithologic log||||||||No log available.||||||||||||||||||||||||||||||||||1000 plugged to 400|540
1655|BDR5-072|25.0|||RSY08|BDR5-072|0.0|Water well, abandoned. Meyer (1958)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0753|39.31222222|-77.47361111|Frederick|Maryland|Thomas and Co.|Buckeystown|1947|lithologic log||||||||Frederick Limestone, surface to bottom||||||||||||||||||||||||||||||||||1209|305
1656|BDR5-073|25.0|||RSY08|BDR5-073|0.0|Water well, abandoned. Meyer (1958)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0754|39.60861111|-77.43361111|Frederick|Maryland|Town of Thurmont|Catoctin Furnace|1929-30|lithologic log||||||||Weverton Quartzite, surface to bottom||||||||||||||||||||||||||||||||||1000|700
1657|BDR5-074|25.0|||RSY05|BDR5-074|0.0|Water well. Meyer (1958)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0755|39.6825|-77.35361111|Frederick|Maryland|Mount St. Mary's College|Emmitsburg|?|lithologic log||||||||Weverton Quartzite, surface to bottom||||||||||||||||||||||||||||||||||850|650
1658|BDR5-075|25.0|||RSY08|BDR5-075|0.0|Water well, abandoned. Clark, and others (1918) Darton (1902), (1905) Meyer (1958)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0756|39.44777778|-77.47|Frederick|Maryland|City of Frederick|Frederick|1844(?)|lithologic log||||||||Harpers Phyllite, surface to bottom||||||||||||||||||||||||||||||||||1140|560
1659|BDR5-076|25.0|||RSY05|BDR5-076|0.0|Water well. Meyer (1958)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0757|39.405|-77.43944444|Frederick|Maryland|Joseph Himes|Frederick|1930|lithologic log||||||||Triassic New Oxford |at surface|(Drilled through contact of New Oxford and Frederick)||||||||||||||||||||||||||||||||615|420
1660|BDR5-077 (A)|25.0|||RSY02|BDR5-077 (A)|0.0|Gas test, dry hole. Amsden (1954) Tucker (1943)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0758|39.63861111|-79.32861111|Garrett|Maryland|New Penn Development Co. William Snee, et al. #1 George Georg|Accident|1942|lithologic log||||||||Pocono(?) |at surface|(Did not reach Corniferous lime)||||||||||||||||||||||||||||||||6735|2535
1661|BDR5-078 (A)|25.0|||RSY02|BDR5-078 (A)|0.0|Gas test, dry hole. Amsden (1954) Martens (1945) Tucker (1943)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0759|39.63583333|-79.32361111|Garrett|Maryland|New Penn Development Co. William Snee, et al. #1 Katherine Schartzer      (Humbertson #1679)|Accident|1942|lithologic log||||||||Pocono |at surface|Chemung, Portage, Genessee, Hamilton, Marcellus |163|Onondaga |789|Huntersville |790|Needmore |800|Oriskany |808|||||||||||||||||||||||8163|2615
1662|BDR5-079 (A)|25.0|||RSY02|BDR5-079 (A)|0.0|Oil or gas test, dry hole . Deepened in 1943. Amsden (1954) Tucker (1936), (1943)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0760|39.62527778|-79.32444444|Garrett|Maryland|Norwood Johnson, et al. #1 Speicher|Accident|1922|lithologic log||||||||Pocono |at surface|Chemung (?) |618|Portage (?) |3700|||||||||||||||||||||||||||||5160 deepened to 7183|2385
1663|BDR5-080 (A)|25.0|||RSY02|BDR5-080 (A)|0.0|Gas test, dry hole. Amsden (1954) Tucker (1943)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0761|39.63333333|-79.32944444|Garrett|Maryland|William Snee, et al. #1 DeLeon J. Rush|Accident|1944|lithologic log||||||||Pocono |at surface|(No subsurface data)||||||||||||||||||||||||||||||||6539|2480
1664|BDR5-081 (A)|25.0|||RSY01|BDR5-081 (A)|0.0|Gas producer, converted to gas storage by Texas Eastern. Repeated section due to probable fault at 6971 feet . Open file|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0762|39.66027778|-79.31222222|Garrett|Maryland|Snee and Eberly #1 McCullough|Accident|1953|lithologic log||||||||Hampshire |at surface|Tully |6131|Brown break |6952|Onondaga |6954|Huntersville |6971|Brown break |7018|Onondaga |7020|Huntersville |7040|Oriskany |7186|||||||||||||||||7191 deepened to 7238|2010
1665|BDR5-082 (A)|25.0|||RSY01|BDR5-082 (A)|0.0|Gas producer. Deepened in 1964 and converted to gas storage well by Texas Eastern. Open file|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0763|39.63277778|-79.3475|Garrett|Maryland|Snee and Eberly #1 John Miller      John Miller Unit|Accident|1954|lithologic log||||||||Pocono |at surface|Onondaga |7048|Huntersville |7084|60' fault|7143|Huntersville |7144|90' fault|7234|Needmore |7380|Oriskany |7426|Helderberg |7556|||||||||||||||||7451 deepened to 7720|2411
1666|BDR5-083 (A)|25.0|||RSY02|BDR5-083 (A)|0.0|Gas test, dry hole. Open file|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0764|39.6375|-79.30611111|Garrett|Maryland|Snee and Eberly #1 Harold Georg      Harold Georg Unit|Accident|1956|lithologic log||||||||Hampshire |at surface|Brown break |7870|Onondaga |7872|||||||||||||||||||||||||||||7880|2335
1667|BDR5-084 (A)|25.0|||RSY01|BDR5-084 (A)|0.0|Gas producer. Reworked in 1963 by Texas Eastern and converted to gas storage. Open file|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0765|39.63027778|-79.3|Garrett|Maryland|Snee and Eberly #1 Charles Bowser      Charles Bowser Unit|Accident|1956|lithologic log||||||||Pocono |at surface|180' fault|3240|Benson |3590|Tully |6732|60' fault|7136|Onondaga |7483|Huntersville |7511|Needmore |7610|Oriskany |7664|Helderberg |7788|||||||||||||||7812|2659
1668|BDR5-085 (A)|25.0|||RSY01|BDR5-085 (A)|0.0|Gas producer. Deepened in 1963 and converted to gas storage by Texas Eastern. Open file|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0766|39.63972222|-79.35|Garrett|Maryland|Snee and Eberly #1 Herman - Hanlin      Herman and Hanlin Unit|Accident|1956|lithologic log||||||||Hampshire |at surface|Tully |6405|Brown break |7024|Onondaga |7026|Huntersville |7046|Oriskany |7186|Helderberg |7330|||||||||||||||||||||7175 deepened to 7350|2353
1669|BDR5-086 (A)|25.0|||RSY01|BDR5-086 (A)|0.0|Gas producer. Deepened in 1964 and converted to gas storage by Texas Eastern. Open file|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0767|39.64166667|-79.34055556|Garrett|Maryland|Snee and Eberly #1 Roy Turney      John Miller Unit|Accident|1957|lithologic log||||||||Hampshire |at surface|100' fault|6723|1st Onondaga|6972|1st Huntersville|7014|55' fault|7032|2nd Onondaga|7040|2nd Huntersville|7060|1st Oriskany|7247|155' fault|7290|3rd Huntersville|7290|2nd Oriskany|7410|Helderberg|7536|||||||||||7260 deepened to 7563|2391
1670|BDR5-087 (A)|25.0|||RSY01|BDR5-087 (A)|0.0|Gas producer. Deepened in 1963 and converted to gas storage by Texas Eastern. Open file|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0768|39.65388889|-79.32833333|Garrett|Maryland|Snee and Eberly #1 Black and Frazee      Black and Frazee Unit|Accident|1958|lithologic log||||||||Hampshire |at surface|Brown break |6534|Onondaga |6536|Huntersville |6555|Needmore |6655|Oriskany |6685|Helderberg |6819|||||||||||||||||||||6707 deepened to 6850|1959
1671|BDR5-088 (A)|25.0|||RSY01|BDR5-088 (A)|0.0|Gas producer . Reworked in 1964 and converted to gas storage by Texas Eastern. Open file|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0769|39.65027778|-79.34583333|Garrett|Maryland|Snee and Eberly #1 Brobst      Carrie Brobst Unit|Accident|1959|lithologic log||||||||Hampshire |at surface|Tully lime |6350|Brown break |7169|Onondaga |7171|Huntersville |7190|Needmore |7276|Oriskany |7372|Shale |7397|Oriskany |7434|||||||||||||||||7584|2199
1672|BDR5-089 (A)|25.0|||RSY01|BDR5-089 (A)|0.0|Gas producer, converted to gas storage by Texas Eastern. Open file|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0770|39.67944444|-79.29583333|Garrett|Maryland|Snee and Eberly #1 J. W. Margroff      J. W. Margroff Unit|Accident|1960|lithologic log||||||||Hampshire |at surface|Brown break |7503|Onondaga |7505|Huntersville |7529|||||||||||||||||||||||||||7639|2387
1673|BDR5-090 (A)|25.0|||RSY01|BDR5-090 (A)|0.0|Gas producer. Open file|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0771|39.66166667|-79.27916667|Garrett|Maryland|Snee and Eberly #1 U.S.A. - Henry Bach      U.S.A. - Henry Bach Unit|Accident|1960|lithologic log||||||||Hampshire |at surface|Brown break |7560|Onondaga |7562|Huntersville |7585|Needmore |7735|Oriskany |7773|||||||||||||||||||||||7936|2342
1674|BDR5-091 (A)|25.0|||RSY03|BDR5-091 (A)|0.0|Observation gas storage well. Open file|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0772|39.63416667|-79.3575|Garrett|Maryland|Texas Eastern Transmission Corp. #2 Herman and Hanlin Unit|Accident|1964|lithologic log||||||||Hampshire |at surface|65' fault|7012|100' fault|7173|45' fault|7328|Onondaga |7374|Huntersville |7408|Oriskany |7538|Helderberg |7667|||||||||||||||||||7800|2400
1675|BDR5-092 (A)|25.0|||RSY07|BDR5-092 (A)|0.0|Gas test, temporarily abandoned. Later converted to gas storage well. Open file|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0773|39.63694444|-79.34166667|Garrett|Maryland|Texas Eastern Transmission Corp. #1 Mark Lokotos      John Miller Unit|Accident|1964|lithologic log||||||||Pocono |at surface|Tully |6280|25' normal fault|6995|Onondaga |6997|Huntersville |7030|Needmore |7203|Oriskany |7263|Helderberg |7407|||||||||||||||||||7605|2441
1676|BDR5-093 (A)|25.0|||RSY03|BDR5-093 (A)|0.0|Gas storage well. Repeated section probably due to fault at 6689 feet. Open file|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0774|39.65722222|-79.325|Garrett|Maryland|Texas Eastern Transmission Corp. #1 Woodrow Friend (amended loc.)      Black and Frazee Unit|Accident|1966|lithologic log||||||||Hampshire |at surface|Tully |5193|1st Onondaga|6563|1st Huntersville|6595|2nd Onondaga|6689|2nd Huntersville|6732|3rd Huntersville|6821|Needmore|6942|Oriskany|6983|Helderberg|7106|||||||||||||||7160|1979
1677|BDR5-094 (A)|25.0|||RSY01|BDR5-094 (A)|0.0|Gas producer. Converted to gas storage well. Open file|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0775|39.64944444|-79.33472222|Garrett|Maryland|Texas Eastern Transmission Corp. #1 Harold Jenkins      Black and Frazee Unit|Accident|1964|lithologic log||||||||Hampshire at surface||1st Onondaga||30' fault||2nd Onondaga||1st Huntersville||90' fault||3rd Onondaga||2nd Huntersville||Needmore||Oriskany||45' fault||Helderberg||||||||||||7303|2310
1678|BDR5-095 (A)|25.0|||RSY03|BDR5-095 (A)|0.0|Gas storage well. Open file|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0776|39.64472222|-79.3475|Garrett|Maryland|Texas Eastern Transmission Corp. #3 Herman and Hanlin      Carrie Brobst Unit|Accident|1965|lithologic log||||||||Hampshire at surface||Onondaga||Huntersville||Needmore||Oriskany||Helder berg||||||||||||||||||||||||7323|2245
1679|BDR5-096 (A)|25.0|||RSY02|BDR5-096 (A)|0.0|Gas test, dry hole. Open file|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0777|39.67194444|-79.26611111|Garrett|Maryland|Snee and Eberly #1 U. S. A. - Harry P. Collier|Accident|1965|lithologic log||||||||Pocono at surface||1st Onondaga||1st Huntersville||2nd Onondaga||2nd Huntersville||Needmore||Oriskany||||||||||||||||||||||8809|2847
1680|BDR5-097 (A)|25.0|||RSY03|BDR5-097 (A)|0.0|Gas storage well. Open file|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0778|39.62611111|-79.35166667|Garrett|Maryland|Texas Eastern Transmission Corp. #1 John H. Bowman      John Miller Unit|Accident|1965|lithologic log||||||||Pocono |at surface|Tully |6228|50' fault |6900|50' fault |7028|1st Onondaga |7100|20' fault |7119|2nd Onondaga |7120|1st Huntersville |7156|80' fault |7233|2nd Huntersville |7233|130' fault |7362|3rd Huntersville |7364|Needmore |7503|1st Oriskany |7557|18' fault |7574|2nd Oriskany |7575|Helderberg |7690|7780|2380
1681|BDR5-098 (A)|25.0|||RSY03|BDR5-098 (A)|0.0|Gas storage well. Open file|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0779|39.66388889|-79.31888889|Garrett|Maryland|Texas Eastern Transmission Corp. #2 Ford C. McCullough      Ford C. McCullough Unit|Accident|1965|lithologic log||||||||Hampshire |at surface|Tully |6387|Onondaga |7085|Huntersville |7110|Needmore |7216|Oriskany |7250|Helderberg |7355|||||||||||||||||||||7369|2234
1682|BDR5-099 (A)|25.0|||RSY03|BDR5-099 (A)|0.0|Gas storage well. Open file|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0780|39.65027778|-79.33055556|Garrett|Maryland|Texas Eastern Transmission Corp. #2 Black and Frazee      Black and Frazee Unit|Accident|1965|lithologic log||||||||Hampshire |at surface|Tully |5975|Onondaga |6742|Huntersville |6770|Needmore |6965|Oriskany |7016|Helderberg |7115|||||||||||||||||||||7120|2270
1683|BDR5-100 (A)|25.0|||RSY03|BDR5-100 (A)|0.0|Gas storage well. Open file|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0781|39.62944444|-79.35638889|Garrett|Maryland|Texas Eastern Transmission Corp. #1 Bowman - Seibert      Herman and Hanlin Unit|Accident|1966|lithologic log||||||||Pocono |at surface|Tully |6342|Onondaga |7043|Huntersville |7064|Needmore |7172|Oriskany |7216|||||||||||||||||||||||7355?|2418
1684|BDR5-101 (A)|25.0|||RSY03|BDR5-101 (A)|0.0|Gas storage well. Open file|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0782|39.63666667|-79.34583333|Garrett|Maryland|Texas Eastern Transmission Corp. #2 Mark Lokotos      John Miller Unit|Accident|1966|lithologic log||||||||Hampshire (?) |at surface|Tully |6294|Onondaga |7178|Huntersville |7203|Needmore |7306|1st Oriskany |7338|30' fault |7365|2nd Oriskany |7369|||||||||||||||||||7485|2398
1685|BDR5-102 (A)|25.0|||RSY03|BDR5-102 (A)|0.0|Gas storage well. Open file|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0783|39.64027778|-79.34611111|Garrett|Maryland|Texas Eastern Transmission Corp. #4 Herman and Hanlin      Carrie Brobst Unit|Accident|1966|lithologic log||||||||Hampshire |at surface|Tully |6240|Onondaga |7079|Huntersville |7103|Needmore |7320|Oriskany |7381|||||||||||||||||||||||7568|2373
1686|BDR5-103 (A)|25.0|||RSY03|BDR5-103 (A)|0.0|Gas storage well. Open file|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0784|39.62916667|-79.35055556|Garrett|Maryland|Texas Eastern Transmission Corp. #1 Snee and Eberly      John Miller Unit|Accident|1966|lithologic log||||||||Pocono |at surface|Tully |6254|Onondaga |7038|1st Huntersville |7058|75' fault |7131|2nd Huntersville |7134|Needmore |7259|Oriskany |7326|||||||||||||||||||7430?|2445
1687|BDR5-104 (A)|25.0|||RSY03|BDR5-104 (A)|0.0|Gas storage well. Open file|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0785|39.64555556|-79.33944444|Garrett|Maryland|Texas Eastern Transmission Corp. #2 Roy Turney      John Miller Unit|Accident|1966|lithologic log||||||||Hampshire |at surface|Tully |6313|Onondaga |6834|1st Huntersville|6859|1st Needmore|6980|fault |6996|2nd Huntersville|6996|2nd Needmore|7062|1st Oriskany|7084|fault?||3rd Needmore|7091|2nd Oriskany|7108|Helderberg |7220|||||||||7270|2250
1688|BDR5-105 (A)|25.0|||RSY03|BDR5-105 (A)|0.0|Gas storage well. Open file|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0786|39.65361111|-79.3325|Garrett|Maryland|Texas Eastern Transmission Corp. #3 Ford C. McCullough      Black and Frazee Unit|Accident|1966|lithologic log||||||||Hampshire |at surface|Tully |5799|Onondaga |6868|Huntersville |6890|Needmore |7031|Oriskany |7062|Helderberg |7184|||||||||||||||||||||7185 (7191 by logger)|1958
1689|BDR5-106|25.0|||RSY02|BDR5-106|0.0|Gas test, dry hole. Open file|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0787|39.71666667|-79.28527778|Garrett|Maryland|Consolidated Gas Supply Corp. #WN- 1104 Edward C. Brougher      Negro Mountain Unit|Accident|1969|lithologic log||||||||Pocono |at surface|Brown break |7770|Onondaga |7780|Huntersville |7795|Oriskany |7964|Helder berg |7998|||||||||||||||||||||||8019|2507
1690|BDR5-107 (A)|25.0|||RSY03|BDR5-107 (A)|0.0|Gas storage well. Open file|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0788|39.62972222|-79.29166667|Garrett|Maryland|Texas Eastern Transmission Corp. #2 U. S. A. - Savage River State Forest      Charles Bowser Unit|Accident|1969|lithologic log||||||||Pocono |at surface|Tully |6836|Onondaga |7536|Huntersville |7568|Needmore |7799|Oriskany |7906|Helderberg |8074|||||||||||||||||||||8172|2772
1691|BDR5-108 (A)|25.0|||RSY03|BDR5-108 (A)|0.0|Gas storage well. Open file|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0789|39.66194444|-79.32388889|Garrett|Maryland|Texas Eastern Transmission Corp. #1 Elizabeth Everly|Accident|1969|lithologic log||||||||Hampshire |at surface|Tully |6286|Onondaga |6979|Huntersville |7004|1st Needmore|7222|fault?||2nd Needmore|7259|fault?||3rd Needmore|7300|Oriskany |7370|Helderberg |7504|||||||||||||7505|2346
1692|BDR5-109 (A)|25.0|||RSY03|BDR5-109 (A)|0.0|Gas storage well. Open file|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0790|39.63277778|-79.29694444|Garrett|Maryland|Texas Eastern Transmission Corp. #2 Charles E. Bowser      Charles Bowser Unit|Accident|1969|lithologic log||||||||Pocono |at surface|Tully |6594|Onondaga |7314|Huntersville |7338|Needmore |7458|Oriskany |7503|Helderberg |7643|||||||||||||||||||||7631|2513
1693|BDR5-110|25.0|||RSY02|BDR5-110|0.0|Gas test, dry hole. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0791|39.67916667|-79.01666667|Garrett|Maryland|Snee and Eberly #1 G. H. Blocher|Avilton|1950|lithologic log||||||||Jennings |at surface|Tully |4105|Onondaga |5025|Huntersville |5081|Needmore |5099|Oriskany |5133|||||||||||||||||||||||5136|2630
1694|BDR5-111|25.0|||RSY02|BDR5-111|0.0|Gas test, dry hole. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0792|39.6375|-79.05|Garrett|Maryland|Superior Oil Development Co. #1 William A, Robeson|Avilton|1951|lithologic log||||||||Jennings |at surface|Tully |3920|Onondaga |4862|Huntersville |4918|Needmore |4936|Oriskany |4960|||||||||||||||||||||||5004|2530
1695|BDR5-112|25.0|||RSY02|BDR5-112|0.0|Gas test, dry hole. (Completion report lost) Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0793|39.64083333|-79.05416667|Garrett|Maryland|Seaboard Oil and Gas Co. #1 Wilt - Jacobs|Avilton|1952|lithologic log||||||||Jennings |at surface|Tully |3736|Huntersville |4819|Oriskany |4880|||||||||||||||||||||||||||4884|2559
1696|BDR5-113|25.0|||RSY02|BDR5-113|0.0|Gas test, dry hole. Open file|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0794|39.71333333|-79.00166667|Garrett|Maryland|Consolidated Gas Supply Corp. #1 Naomi Berry|Avilton|1967|lithologic log||||||||Jennings |at surface|Huntersville |5170|Needmore |5210|Oriskany |5252|||||||||||||||||||||||||||5340|2439
1697|BDR5-114|25.0|||RSY05|BDR5-114|0.0|Stratigraphic test and water well. Slaughter (1962)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0795|39.54111111|-79.03111111|Garrett|Maryland|Barton Water Co.|Barton|1950|lithologic log||||||||Conemaugh |at surface|Allegheny~Pottsville|?|Mauch Chunk |1000|||||||||||||||||||||||||||||1014|1580
1698|BDR5-115|25.0|||RSY02|BDR5-115|0.0|Gas test, dry hole. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0796|39.50472222|-79.21388889|Garrett|Maryland|Oil Ventures, Inc. #1 Kenneth Beckman|Bittinger|1952|lithologic log||||||||Jennings |at surface|Marcellus |5572|Brown break |5790|Onondaga |5792|Huntersville |5837|Needmore |5871|Oriskany |5992|||||||||||||||||||||6010|2630
1699|BDR5-116|25.0|||RSY08|BDR5-116|0.0|Water well, now abandoned. Clark, and others (1918) Darton (1902), (1905)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0797|39.41888889|-79.32916667|Garrett|Maryland|Deer Park Hotel Baltimore and Ohio Railroad|Deer Park|1890|lithologic log||||||||No log available.||||||||||||||||||||||||||||||||||2010|2460
1700|BDR5-117 (B)|25.0|||RSY07|BDR5-117 (B)|0.0|Gas producer, plugged and abandoned 1961 . Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0798|39.40972222|-79.35638889|Garrett|Maryland|Snee and Eberly #1 Gordon|Deer Park|1951|lithologic log||||||||Jennings |at surface|Tully |3132|Brown break |3695|Onondaga |3698|Huntersville |3725|Needmore |3798|Oriskany |3848|Helderberg |3952|||||||||||||||||||4145|2450
1701|BDR5-118 (B)|25.0|||RSY07|BDR5-118 (B)|0.0|Gas producer, plugged and abandoned 1967 . Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0799|39.41388889|-79.35777778|Garrett|Maryland|Columbian Carbon Co. #1 D. E. Offutt, et al.      GW- 1505      (#1 William R. Offutt)|Deer Park|1951|lithologic log||||||||Jennings |at surface|Onondaga |3891|Huntersville |3943|Needmore |3981|Oriskany |4035|Helderberg |4144|Chert |4423|||||||||||||||||||||4511|2530
1702|BDR5-119 (B)|25.0|||RSY07|BDR5-119 (B)|0.0|Gas producer, abandoned . Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0800|39.40055556|-79.36944444|Garrett|Maryland|Blaho Oil and Gas Co. Thomas J. Blaho, Jr. #1 Kight (Mountain Lake Park Association)|Deer Park|1951|lithologic log||||||||Jennings |at surface|Brown break |357 5|Onondaga |3528|Huntersville |3606|||||||||||||||||||||||||||3675|2415
1703|BDR5-120 (B)|25.0|||RSY07|BDR5-120 (B)|0.0|Gas producer, plugged and abandoned 1952. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0801|39.39972222|-79.36805556|Garrett|Maryland|O. M. Fox, et al . (Fox, Trimble, et al.) #1 McKee|Deer Park|1951|lithologic log||||||||Jennings |at surface|Tully |2940|Marcellus |3653|Huntersville |3798|||||||||||||||||||||||||||3834|2430
1704|BDR5-121|25.0|||RSY02|BDR5-121|0.0|Gas test, dry hole. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0802|39.44694444|-79.32|Garrett|Maryland|Charles E. Young Columbian Carbon Co . #1 F. Perry Smith, Jr.|Deer Park|1951|lithologic log||||||||Jennings |at surface|Tully |4345|Onondaga |4875|Huntersville |4934|Oriskany |5055|||||||||||||||||||||||||5212|2570
1705|BDR5-122|25.0|||RSY02|BDR5-122|0.0|Gas test, dry hole. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0803|39.47055556|-79.33638889|Garrett|Maryland|Eagle Gas Co. #1 Dorothea Ashby|Deer Park|1951|lithologic log||||||||Hampshire |at surface|No log available.||||||||||||||||||||||||||||||||1427|2540
1706|BDR5-123 (B)|25.0|||RSY02|BDR5-123 (B)|0.0|Gas test, dry hole. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0804|39.39333333|-79.37222222|Garrett|Maryland|Mid-Atlantic Oil and Gas Co. #1 J.B. Simmons      (W. B. Symonds)|Deer Park|1952|lithologic log||||||||Jennings |at surface|Brown break |3921|Onondaga |3923|Huntersville |3956|Needmore |4034|Oriskany |4079|||||||||||||||||||||||4186|2460
1707|BDR5-124|25.0|||RSY02|BDR5-124|0.0|Gas test, dry hole. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0805|39.43|-79.32944444|Garrett|Maryland|Mid-Atlantic Oil and Gas Co. #1 J. Clarence Lashorn      (C. J, Lashorn)|Deer Park|1951|lithologic log||||||||Jennings |at surface|Tully |4493|Brown break |5042|Onondaga |5045|Huntersville |5068|Needmore |5127|Oriskany |5180|||||||||||||||||||||5195|2540
1708|BDR5-125 (B)|25.0|||RSY02|BDR5-125 (B)|0.0|Gas test, dry hole. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0806|39.40861111|-79.36722222|Garrett|Maryland|New York State Natural Gas Corp #1 John K. Shaw estate, Mercantile Trust Co. of Baltimore, trustees.      #N-241|Deer Park|1952|lithologic log||||||||Jennings |at surface|Onondaga |3668|Huntersville |3705|Oriskany |3829|Helderberg |3925|||||||||||||||||||||||||3963|2440
1709|BDR5-126|25.0|||RSY02|BDR5-126|0.0|Gas test, dry hole. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0807|39.4425|-79.37138889|Garrett|Maryland|Harry Goodman Goodman Brothers, Inc. #1 Holtschneider|Deer Park|1952|lithologic log||||||||Hampshire |at surface|No log available.||||||||||||||||||||||||||||||||2600|2640
1710|BDR5-127 (B)|25.0|||RSY02|BDR5-127 (B)|0.0|Gas test, dry hole. Amsden (19 54)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0808|39.41083333|-79.36805556|Garrett|Maryland|Columbian Carbon Co. #1 Emily F. Moon      GW-1506|Deer Park|1951|lithologic log||||||||Jennings |at surface|Brown break |4011|Onondaga |4014|Huntersville |4043|Needmore |4090|Oriskany |4154|Helder berg |4265|||||||||||||||||||||4267|2457
1711|BDR5-128|25.0|||RSY02|BDR5-128|0.0|Gas test, dry hole. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0809|39.38888889|-79.35333333|Garrett|Maryland|Union Drilling Co. #1 Roy B. Lichty|Deer Park|1951|lithologic log||||||||Jennings |at surface|No log available.||||||||||||||||||||||||||||||||3800|2510
1712|BDR5-129 (B)|25.0|||RSY02|BDR5-129 (B)|0.0|Gas test, dry hole. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0810|39.40472222|-79.37472222|Garrett|Maryland|Richard Downing Moran and Co. #1 McClain|Deer Park|1951|lithologic log||||||||Jennings |at surface|Brown break |3703|Onondaga |3706|Huntersville |3733|Needmore |3823|Oriskany |3860|Helderberg |3975|||||||||||||||||||||3986|2505
1713|BDR5-130 (B)|25.0|||RSY07|BDR5-130 (B)|0.0|Gas producer, plugged and abandoned 1953. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0811|39.39666667|-79.37083333|Garrett|Maryland|Snee and Eberly #1 Simmons|Deer Park|1951|lithologic log||||||||Jennings |at surface|Tully |3170|Marcellus |3660|Brown break |3718|Onondaga |3719|Huntersville |3747|||||||||||||||||||||||3786|2410
1714|BDR5-131 (B)|25.0|||RSY07|BDR5-131 (B)|0.0|Gas producer, plugged and abandoned 1952. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0812|39.39083333|-79.37472222|Garrett|Maryland|Delaware Gas Co. #1 George T. Perrine, et al.|Deer Park|1951|lithologic log||||||||Jennings |at surface|Tully |3032|Brown break |3674|Onondaga |3677|Huntersville |3711|Oriskany |3824|||||||||||||||||||||||3835|2420
1715|BDR5-132|25.0|||RSY02|BDR5-132|0.0|Gas test, dry hole. No completion report. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0813|39.4|-79.34444444|Garrett|Maryland|Penn-Maryland Gas Co. #1 Murphy|Deer Park|1951|lithologic log||||||||Hampshire |at surface|No log available.||||||||||||||||||||||||||||||||?|2480
1716|BDR5-133 (B)|25.0|||RSY02|BDR5-133 (B)|0.0|Gas test, dry hole. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0814|39.40027778|-79.36666667|Garrett|Maryland|New York State Natural Gas Corp. #2 John K. Shaw estate, Mercantile Trust Co. of Baltimore, trustees.      #N-247|Deer Park|1952|lithologic log||||||||Jennings |at surface|Tully |3240|Onondaga |3765|Huntersville |3790|Oriskany |3904|Helderberg |4007|Tonoloway |4380|Wills Creek |5085|Williamsport |5740|McKenzie |5790|Rose Hill |6450|Tuscarora |7120|||||||||||7162|2450
1717|BDR5-134 (B)|25.0|||RSY07|BDR5-134 (B)|0.0|Gas producer, plugged and abandoned 1954. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0815|39.39694444|-79.37444444|Garrett|Maryland|Cumberland and Allegheny Gas Corp. #1 H. M. Weeks      A-461|Deer Park|1951|lithologic log||||||||Jennings |at surface|Tully |2928|Marcellus |3428|Brown break |3465|Onondaga |3467|Huntersville |3490|Oriskany |3608|Helder berg |3716|||||||||||||||||||3719|2390
1718|BDR5-135 (B)|25.0|||RSY02|BDR5-135 (B)|0.0|Gas test, dry hole. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0816|39.41222222|-79.36277778|Garrett|Maryland|Snee and Eberly #2 Gordon|Deer Park|1951|lithologic log||||||||Jennings |at surface|Tully |3204|Brown break |3775|Onondaga |3778|Huntersville |3811|Oriskany |3931|Helderberg |4007|||||||||||||||||||||4042|2480
1719|BDR5-136 (B)|25.0|||RSY07|BDR5-136 (B)|0.0|Gas producer, abandoned. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0817|39.39527778|-79.37444444|Garrett|Maryland|Thomas Lafferty and Columbus Whetzel #1 Ashby      (#1 Mountain Lake Park Motors)|Deer Park|1951|lithologic log||||||||Jennings |at surface|Huntersville |3530|Oriskany |3641|||||||||||||||||||||||||||||3719?|2390
1720|BDR5-137 (B)|25.0|||RSY07|BDR5-137 (B)|0.0|Gas producer, plugged and abandoned 1952. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0818|39.39944444|-79.36888889|Garrett|Maryland|Cumberland and Allegheny Gas Corp. #1 C. C. Mason      A-465|Deer Park|1951|lithologic log||||||||Jennings |at surface|Brown break |3692|Onondaga |3696|Huntersville |3729|Oriskany |3848|Helderberg |3972|||||||||||||||||||||||3980|2418
1721|BDR5-138 (B)|25.0|||RSY07|BDR5-138 (B)|0.0|Gas producer, abandoned 1952. No completion report. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0819|39.395|-79.37472222|Garrett|Maryland|Antietam Natural Gas Co., Inc. #1 Killius - Sisler|Deer Park|1951|lithologic log||||||||Jennings |at surface|Huntersville |3850|Oriskany |3979|||||||||||||||||||||||||||||4077|2440
1722|BDR5-139 (B)|25.0|||RSY02|BDR5-139 (B)|0.0|Gas test, dry hole. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0820|39.39777778|-79.37|Garrett|Maryland|Fox and Trimble #2 McKee|Deer Park|1952|lithologic log||||||||Jennings |at surface|Brown break |3817|Onondaga |3823|Huntersville |3852|Oriskany |3964|||||||||||||||||||||||||4038|2400
1723|BDR5-140 (B)|25.0|||RSY07|BDR5-140 (B)|0.0|Gas producer, plugged and abandoned 1952. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0821|39.39333333|-79.37416667|Garrett|Maryland|W. H. and J. A. Roeder      (Roeder and Roeder) #1 United Brethren Church|Deer Park|1951|lithologic log||||||||Jennings |at surface|Tully |3100|Marcellus |3570|Onondaga |3642|Huntersville |3672|||||||||||||||||||||||||3721|2420
1724|BDR5-141 (B)|25.0|||RSY07|BDR5-141 (B)|0.0|Gas producer, plugged and abandoned 1952. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0822|39.39444444|-79.37083333|Garrett|Maryland|Mid-Atlantic Oil and Gas Co. #1 Joseph Callis, et al.|Deer Park|1951|lithologic log||||||||Jennings |at surface|Brown break |3875|Onondaga |3877|Huntersville |3912|Oriskany |4022|||||||||||||||||||||||||4040|2480
1725|BDR5-142 (B)|25.0|||RSY07|BDR5-142 (B)|0.0|Gas producer, plugged and abandoned 1952, Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0823|39.39388889|-79.37361111|Garrett|Maryland|Mid-Atlantic Oil and Gas Co. #1 I.O.O.F. Oak Lodge #8|Deer Park|1951|lithologic log||||||||Jennings |at surface|Onondaga |3699|Huntersville |3729|Oriskany |3842|||||||||||||||||||||||||||3975|2425
1726|BDR5-143 (B)|25.0|||RSY02|BDR5-143 (B)|0.0|Gas test, dry hole. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0824|39.39583333|-79.37305556|Garrett|Maryland|Mid-Atlantic Oil and Gas Co.      (Union Drilling Co.) #1 Baltimore and Ohio Railroad|Deer Park|1952|lithologic log||||||||Jennings |at surface|Tully |3070|Brown break |3627|Onondaga |3628|Huntersville |3655|||||||||||||||||||||||||3712|2400
1727|BDR5-144 (B)|25.0|||RSY02|BDR5-144 (B)|0.0|Gas test, dry hole. No completion report. Amsden (1954) (data from Oil and Gas Journal, Apr. 28, 1952)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0825|39.39388889|-79.36944444|Garrett|Maryland|Penn-Maryland Gas Co. #1 Smith|Deer Park|?|lithologic log||||||||Jennings |at surface|Huntersville |4102|Oriskany |4231|||||||||||||||||||||||||||||?|2490
1728|BDR5-145 (B)|25.0|||RSY02|BDR5-145 (B)|0.0|Gas test, dry hole . Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0826|39.39416667|-79.37444444|Garrett|Maryland|S. and M. Oil and Gas, Inc. #1 H. Z, Gibson|Deer Park|1952|lithologic log||||||||Jennings |at surface|Onondaga |3555|Huntersville |3585|Oriskany |3660|Helderberg |3750|||||||||||||||||||||||||4044|2410
1729|BDR5-146 (B)|25.0|||RSY02|BDR5-146 (B)|0.0|Gas test, dry hole. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0827|39.40861111|-79.36138889|Garrett|Maryland|Snee and Eberly #3 Gordon|Deer Park|1952|lithologic log||||||||Jennings |at surface|Tully |3221|Brown break |3775|Onondaga |3778|Huntersville |3800|Oriskany |3922|Helderberg |4023|||||||||||||||||||||4091|2510
1730|BDR5-147 (B)|25.0|||RSY02|BDR5-147 (B)|0.0|Gas test, dry hole. No completion report. Amsden (1954) (data from Oil and Gas Journal, May 12, 1952)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0828|39.39194444|-79.375|Garrett|Maryland|Thomas Blaho Blaho Oil and Gas Co. #1 Joseph Gower      (#1 Garrett)|Oakland|1952|lithologic log||||||||Jennings |at surface|Huntersville |3540|||||||||||||||||||||||||||||||?|2400
1731|BDR5-148 (B)|25.0|||RSY07|BDR5-148 (B)|0.0|Gas producer, abandoned 1953 . Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0829|39.40333333|-79.36805556|Garrett|Maryland|Ray Kight #1 Friend|Deer Park|1952|lithologic log||||||||Jennings |at surface|Onondaga |3733|Huntersville |3735|Oriskany |3848|||||||||||||||||||||||||||3924|2440
1732|BDR5-149|25.0|||RSY02|BDR5-149|0.0|Oil or gas test, dry hole . Amsden (1954) Reger (1924) Tucker (1936)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0830|39.30527778|-79.31472222|Garrett|Maryland|Potomac Oil and Gas Corp. #1 Bayard Coal Co.|Gorman|1920|lithologic log||||||||Allegheny |at surface|Homewood Sandstone |115|Maxton Sandstone |866|Greenbrier |874|Berea |1488|Gordon Sandstone |2166|||||||||||||||||||||||2240|2350
1733|BDR5-150|25.0|||RSY02|BDR5-150|0.0|Oil or gas test, dry hole. Amsden (1954) Reger (1924) Tucker (1936)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0831|39.29|-79.35305556|Garrett|Maryland|Potomac Oil and Gas Corp. #1 John Nydegger|Gorman|1921|lithologic log||||||||Conemaugh |at surface|Homewood Sandstone |425|Greenbrier |1440|Berea(?) |1798|Gordon Sandstone |2552|Elizabeth Sandstone |3445|||||||||||||||||||||||3500|2360
1734|BDR5-151|25.0|||RSY02|BDR5-151|0.0|Gas test, dry hole. Open file|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0832|39.3525|-79.34583333|Garrett|Maryland|Furman L. Nuss #1 W. H. Steyer|Gorman|1957|lithologic log||||||||Allegheny |at surface|Greenbrier |1118|Bottomed in Jennings||||||||||||||||||||||||||||||4116|2669
1735|BDR5-152|25.0|||RSY06|BDR5-152|0.0|Stratigraphic test. Toenges, and others (1952)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0833|39.67|-79.155|Garrett|Maryland|U. S. Bureau of Mines Drill Hole CB-2|Grantsville|1947 (?)|lithologic log||||||||Conemaugh |at surface|Allegheny-Pottsville |568|Mauch Chunk |1012|||||||||||||||||||||||||||||1045|2474
1736|BDR5-153|25.0|||RSY01|BDR5-153|0.0|Gas producer. Open file|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0834|39.665|-79.23611111|Garrett|Maryland|Cumberland and Allegheny Gas Co. #1 Negro Mountain Unit      A-602      (Farm 186-A, U. S. A.)|Grantsville|1965|lithologic log||||||||Pottsville |at surface|Mauch Chunk |314 |Greenbrier |775 |Pocono |785 |Hampshire |1800 |Jennings |3205 |Tully |7531 |Hamilton |7605 |Marcellus |7840 |Onondaga |8358 |Huntersville |8374 |Needmore |8461 |Oriskany |8491 |Helderberg |8634 |||||||8640|2929
1737|BDR5-154|25.0|||RSY01|BDR5-154|0.0|Gas producer. Open file|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0835|39.67833333|-79.22222222|Garrett|Maryland|Cumberland and Allegheny Gas Co. #1 Sincell and Howell      Negro Mountain Unit      A-603|Grantsville|1966|lithologic log||||||||Pottsville |at surface|Benson Sandstone |4675 |Tully |7416 |Brown break |8277 |Onondaga |8279 |Huntersville |8295 |Needmore |8378 |Oriskany |8398 |Helderberg |8548 |||||||||||||||||8607|2766
1738|BDR5-155|25.0|||RSY01|BDR5-155|0.0|Gas producer. Open file|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0836|39.69|-79.21388889|Garrett|Maryland|Cumberland and Allegheny Gas Co. #1 Smith - Kerr      A-604|Grantsville|1966|lithologic log||||||||Pottsville |at surface|Benson |4745|Tully |7545|Brown break |8354|Onondaga |8356|Huntersville |8373|Needmore |8460|Oriskany |8478|Helderberg |8658|||||||||||||||||8700 (8675 by logger)|2882
1739|BDR5-156|25.0|||RSY06|BDR5-156|0.0|Stratigraphic test. Toenges, and others (1949)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0837|39.58972222|-78.99805556|Garrett|Maryland|U. S. Bureau of Mines Drill Hole GC-5|Lonaconing|1946|lithologic log||||||||Conemaugh |at surface|Allegheny |586|Pottsville |863|Mauch Chunk |1063|||||||||||||||||||||||||||1127|2000
1740|BDR5-157|25.0|||RSY05|BDR5-157|0.0|Stratigraphic test and water we 11. Slaughter (1962)|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0838|39.59083333|-78.99944444|Garrett|Maryland|Lonaconing Water Co.|Lonaconing|1951 deepened in 1953|lithologic log||||||||Conemaugh |at surface|Allegheny-Pottsville |540|Mauch Chunk |1142|||||||||||||||||||||||||||||1276|2000
1741|BDR5-158 (B)|25.0|||RSY01|BDR5-158 (B)|0.0|Gas producer. Deepened by Snee and Eberly in 1960 under permit G-34. Converted to gas storage by Texas Eastern. Open file|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0839|39.62222222|-79.31111111|Garrett|Maryland|Snee and Eberly #1 Ella Collier      Ella Collier Unit|McHenry|1955|lithologic log||||||||Hampshire |at surface|1st Benson Sandstone |3126|80' fault |3202|2nd Benson Sandstone |3203|Tully |6052|175' fault |6460|Brown break |6978|Onondaga |6980|Huntersville |7003|35' fault |7032|Needmore |7132|Oriskany |7171|Helderberg |7284|||||||||7255 deepened to 7355|2399
1742|BDR5-159 (A)|25.0|||RSY01|BDR5-159 (A)|0.0|Gas producer, converted to gas storage by Texas Eastern. Open file|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0840|39.59194444|-79.33416667|Garrett|Maryland|Snee and Eberly #1 Ford Fike      Ford Fike Unit|McHenry|1956|lithologic log||||||||Hampshire |at surface|Brown break |7358|Onondaga |7360|Huntersville |7384|Needmore |7498|Oriskany |7544|Helderberg |7650|||||||||||||||||||||7790|2479
1743|BDR5-160 (A)|25.0|||RSY01|BDR5-160 (A)|0.0|Gas producer. Redrilled from 6626 to 7205 by Texas Eastern in 1964 and converted to gas storage. Open file|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0841|39.60722222|-79.31666667|Garrett|Maryland|Snee and Eberly #1 Barbara Miller      Barbara Miller Unit|McHenry|1955|lithologic log||||||||Hampshire |at surface|Benson |3145|Brown break |6860|Onondaga |6863|Huntersville |6881|Needmore |6980|Oriskany |7025|Helderberg |7164|||||||||||||||||||7042 deepened to 7205|2415
1744|BDR5-161 (A)|25.0|||RSY01|BDR5-161 (A)|0.0|Gas producer. Deepened by Texas Eastern and converted to gas storage. Open file|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0842|39.59444444|-79.31861111|Garrett|Maryland|Snee and Eberly #1 Earl Knox      Earl Knox Unit|McHenry|1955|lithologic log||||||||Pocono |at surface|Benson |3738|Onondaga |7457|Huntersville |7482|Needmore |7575|Oriskany |7612|Helderberg |7703|||||||||||||||||||||7728 deepened to 7769|2858
1745|BDR5-162 (A)|25.0|||RSY01|BDR5-162 (A)|0.0|Gas producer. Redrilled from 6542 to 7283 by Texas Eastern in 1964 and converted to gas storage. Open file|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0843|39.62194444|-79.35722222|Garrett|Maryland|Snee and Eberly #1 Mitchell Rush      Mitchell Rush Unit|McHenry|1956|lithologic log||||||||Pocono |at surface|Tully |6330|45' fault|6867|Brown break |6946|Onondaga |6948|Huntersville |6972|Needmore |7088|Oriskany |7109|Helderberg |7230|||||||||||||||||7237 deepened to 7283|2332
1746|BDR5-163 (A)|25.0|||RSY01|BDR5-163 (A)|0.0|Gas producer. Deepened by Texas Eastern in 1964 and converted to gas storage. Open file|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0844|39.57972222|-79.33333333|Garrett|Maryland|Snee and Eberly #1 Whiteface      Whiteface Unit|McHenry|1957|lithologic log||||||||Pocono |at surface|Onondaga |7616|Huntersville |7646|Needmore |7770|Oriskany |7810|Helderberg |7937|||||||||||||||||||||||8183 deepened to 8194|2850
1747|BDR5-164 (A)|25.0|||RSY01|BDR5-164 (A)|0.0|Gas producer. Deepened by Texas Eastern in 1964 and converted to gas storage. Open file|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0845|39.61027778|-79.30277778|Garrett|Maryland|Snee and Eberly #1 Arnold Georg      Arnold Georg Unit|McHenry|1957|lithologic log||||||||Pocono |at surface|Tully |7048|Onondaga |7790|Huntersville |7819|Needmore |7906|Oriskany |7949|Helderberg |8100|||||||||||||||||||||7909 deepened to 8200|2861
1748|BDR5-165 (A)|25.0|||RSY01|BDR5-165 (A)|0.0|Gas producer, converted to gas storage by Texas Eastern. Open file|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0846|39.61194444|-79.37111111|Garrett|Maryland|Snee and Eberly #1 Frazee      Frazee Bros. Unit|McHenry|1959|lithologic log||||||||Pocono |at surface|Brown break |7408|Onondaga |7410|Huntersville |7434|Needmore |7566|Oriskany |7590|||||||||||||||||||||||7762|2547
1749|BDR5-166 (A)|25.0|||RSY01|BDR5-166 (A)|0.0|Gas producer, converted to gas storage by Texas Eastern. Repeated section probably due to fault between 7353 and 7465. Open file|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0847|39.60638889|-79.36|Garrett|Maryland|Snee and Eberly #1 Doerr      Doerr Unit|McHenry|1959|lithologic log||||||||Pocono |at surface|Tully |6345|Onondaga |7317|Huntersville |7353|Shale |7420|Onondaga |7465|Huntersville |7493|Needmore |7657|Oriskany |7706|||||||||||||||||7810|2383
1750|BDR5-167 (A)|25.0|||RSY01|BDR5-167 (A)|0.0|Gas producer. Reworked by Texas Eastern and converted to gas storage. Open file|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0848|39.6025|-79.30472222|Garrett|Maryland|Snee and Eberly #1 Walter Harman      Walter Harman Unit|McHenry|1959|lithologic log||||||||Pocono |at surface|Benson |3660|Tully |6845|Brown break |7639|Onondaga |7642|Huntersville |7661|Needmore |7697|70' fault|7714|Onondaga |7714|Huntersville |7732|Needmore |7836|Oriskany |7884|Helderberg |8020|||||||||8166|2788
1751|BDR5-168 (A)|25.0|||RSY03|BDR5-168 (A)|0.0|Gas storage well. Open file|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0849|39.60222222|-79.31166667|Garrett|Maryland|Texas Eastern Transmission Corp. #1 Helen Enlow (relocated)      Walter Harman Unit|McHenry|1965|lithologic log||||||||Hampshire |at surface|Benson |3577|Onondaga |7313|Huntersville |7345|Needmore |7477|Oriskany |7528|Helderberg |7787|||||||||||||||||||||7850|2572
1752|BDR5-169 (A)|25.0|||RSY03|BDR5-169 (A)|0.0|Gas storage well. Open file|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0850|39.61638889|-79.30277778|Garrett|Maryland|Texas Eastern Transmission Corp. #1 J. J . Schlossnagle      Ella B. Collier Unit|McHenry|1964|lithologic log||||||||Hampshire |at surface|Benson |3208|Tully |6030|230' fault|6110|55' fault|6877|35' fault|7000|Onondaga |7062|1st Huntersville|7093|2nd Huntersville|1735|50' fault|7152|Needmore |7232|Oriskany |7280|Helderberg |7464|||||||||7507|2476
1753|BDR5-170 (A)|25.0|||RSY03|BDR5-170 (A)|0.0|Gas storage well. Open file|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0851|39.60083333|-79.32027778|Garrett|Maryland|Texas Eastern Transmission Corp. #1 Playford Smith      Earl Knox Unit|McHenry|1964|lithologic log||||||||Hampshire |at surface|Benson |3308|Tully |6353|Onondaga |7156|Huntersville |7184|Needmore |7274|55' fault |7295|2nd Huntersville |7296|2nd Needmore |7332|25' fault |7340|3rd Huntersville |7341|3rd Needmore |7349|Oriskany |7391|Helderberg |7510|||||||7546|2505
1754|BDR5-171 (A)|25.0|||RSY03|BDR5-171 (A)|0.0|Gas storage well. Open file|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0852|39.61027778|-79.31666667|Garrett|Maryland|Texas Eastern Transmission Corp. #2 Barbara Miller      Barbara Miller Unit|McHenry|1964|lithologic log||||||||Hampshire |at surface|90' fault |3070|Benson |3268|Tully |6163|1st Onondaga |6878|35' fault |6915|2nd Onondaga |6916|Huntersville |6952|Needmore |7047|Oriskany |7091|Helderberg |7225|||||||||||||7251|2459
1755|BDR5-172 (A)|25.0|||RSY03|BDR5-172 (A)|0.0|Gas storage well. Open file|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0853|39.61277778|-79.31027778|Garrett|Maryland|Texas Eastern Transmission Corp. #2 Arnold Georg      Arnold Georg Unit|McHenry|1965|lithologic log||||||||Pocono |at surface|Benson |3546|1st Onondaga |7258|fault?||2nd Onondaga |7345|1st Huntersville |7374|fault||2nd Huntersville |7409|Needrnore |7500|Oriskany |7546|Helderberg |7695|||||||||||||7801|2785
1756|BDR5-173 (A)|25.0|||RSY03|BDR5-173 (A)|0.0|Gas storage well. Open file|Reported|WJUNKIN|2021-08-19 16:38:54|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0854|39.60194444|-79.325|Garrett|Maryland|Texas Eastern Transmission Corp. #1 Period B. Spear      Ford Fike Unit|McHenry|1965|lithologic log||||||||Hampshire |at surface|Benson |3300|Onondaga |7178|Huntersville |72 09|Needrnore |7329|Oriskany |7365|Helderberg |7496|||||||||||||||||||||7615|2464
1757|BDR5-174 (A)|25.0|||RSY03|BDR5-174 (A)|0.0|Gas storage well . Open file|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0855|39.5875|-79.325|Garrett|Maryland|Texas Eastern Transmission Corp. 1/1 Roy E. Kahl      Earl Knox Unit|McHenry|1965|lithologic log||||||||Pocono |at surface|Benson |3622|Tully |6527|Onondaga |7510|Huntersville |7543|Needrnore |7629|Oriskany |7670|Helder berg |7843|||||||||||||||||||7882|2718
1758|BDR5-175 (A)|25.0|||RSY03|BDR5-175 (A)|0.0|Gas storage well. Open file|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0856|39.60888889|-79.31111111|Garrett|Maryland|Texas Eastern Transmission Corp. #1 Walter Burkhard      Arnold Georg Unit|McHenry|1965|lithologic log||||||||Hampshire |at surface|Tully |6389|75' fault |6970|Onondaga |7236|Huntersville |7268|45' fault |7346|25' fault |7411|Oriskany |7485|||||||||||||||||||7630|2630
1759|BDR5-176 (A)|25.0|||RSY03|BDR5-176 (A)|0.0|Gas storage well. Open file|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0857|39.62333333|-79.32138889|Garrett|Maryland|Texas Eastern Transmission Corp. #1 Walter H. Fratz (alternate location)      Ella Collier Unit|McHenry|1966|lithologic log||||||||Hampshire |at surface|Benson |3313|Tully |6313|Onondaga |6997|Huntersville |7022|Needmore |7113|Oriskany |7151|Helderberg |7297|||||||||||||||||||7310 (7301 by logger)|2484
1760|BDR5-177 (A)|25.0|||RSY03|BDR5-177 (A)|0.0|Gas storage well. Open file|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0858|39.59638889|-79.32638889|Garrett|Maryland|Texas Eastern Transmission Corp. #1 Charles A. Rexrode      Ford Fike Unit|McHenry|1966|lithologic log||||||||Hampshire |at surface|Benson |3532|Tully |6674|Onondaga |7364|Huntersville |7390|Needmore |7485|Oriskany |7521|Helderberg |7640|||||||||||||||||||7650 (7642 by logger)|2623
1761|BDR5-178 (A)|25.0|||RSY03|BDR5-178 (A)|0.0|Gas storage well. Open file|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0859|39.62138889|-79.28722222|Garrett|Maryland|Texas Eastern Transmission Corp. #1 U. S. A. - Savage River State Forest      Charles Bowser Unit|McHenry|1966|lithologic log||||||||Pocono |at surface|Benson |3951|Tully |7102|Onondaga |7830|Huntersville |7859|Needmore |7948|Oriskany |7981|Helderberg |8138|||||||||||||||||||8140|2684
1762|BDR5-179 (A)|25.0|||RSY03|BDR5-179 (A)|0.0|Gas storage well. Open file|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0860|39.61388889|-79.31444444|Garrett|Maryland|Texas Eastern Transmission Corp. #3 Barbara Miller      Ella Collier Unit|McHenry|1966|lithologic log||||||||Hampshire |at surface|Benson |3291|Tully |6216|Onondaga |6937|Huntersville |6963|Needmore |7063|Oriskany |7106|Helderberg |7279|||||||||||||||||||7279+|2370
1763|BDR5-180 (A)|25.0|||RSY03|BDR5-180 (A)|0.0|Gas storage well. Open file|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0861|39.60388889|-79.31972222|Garrett|Maryland|Texas Eastern Transmission Corp. #2 Helen Enlow|McHenry|1966|lithologic log||||||||Hampshire |at surface|Benson |3193|Tully |6207|Onondaga |7000|1st Hunterville |7036|fault |7055|2nd Huntersville |7058|1st Needmore |7153|1st Oriskany |7196|fault |7220|2nd Needmore |7223|2nd Oriskany |7264|Helderberg |7397|||||||||7402?|2413
1764|BDR5-181 (A)|25.0|||RSY03|BDR5-181 (A)|0.0|Gas storage well. Open file|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0862|39.59277778|-79.32972222|Garrett|Maryland|Texas Eastern Transmission Corp. #2 Charles A. Rexrode      Ford Fike Unit|McHenry|1966|lithologic log||||||||Hampshire |at surface|Benson |3371|Tully |6602|Onondaga |7255|1st Huntersville |7282|40' fault |7318|2nd Huntersville |7323|Needmore |7422|Oriskany |7456|||||||||||||||||7619|2521
1765|BDR5-182 (A)|25.0|||RSY03|BDR5-182 (A)|0.0|Gas storage well. Open file|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0863|39.61944444|-79.30833333|Garrett|Maryland|Texas Eastern Transmission Corp. #2 Ella B. Collier|McHenry|1966|lithologic log||||||||Helderberg |7592|Hampshire |at surface|Benson |3129|Onondaga |6947|1st Huntersville |6973|40' fault |7013|2nd Huntersville |7015|Needmore |7110|Oriskany |7150|Helderberg |7275|||||||||||||||7288|2397
1766|BDR5-183 (A)|25.0|||RSY03|BDR5-183 (A)|0.0|Gas storage well. Open file|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0864|39.60527778|-79.30916667|Garrett|Maryland|Texas Eastern Transmission Corp. #2 Burkhard - Knox      Walter Harman Unit|McHenry|1966|lithologic log||||||||Hampshire |at surface|Tully |6435|Onondaga |7178|Huntersville |7209|Needmore |7308|Oriskany |7356|Helderberg |7496|||||||||||||||||||||7499|2582
1767|BDR5-184 (A)|25.0|||RSY03|BDR5-184 (A)|0.0|Gas storage well. Open file|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0865|39.59166667|-79.32388889|Garrett|Maryland|Texas Eastern Transmission Corp. #3 Charles A. Rexrode      Earl Knox Unit|McHenry|1966|lithologic log||||||||Hampshire |at surface|Benson |3488|Tully |6393|1st Onondaga |7337|1st Huntersville |7359|2nd Onondaga |7403|2nd Huntersville |7420|Needmore |7513|Oriskany |7544|Helderberg |7666|||||||||||||||7669 (7665 by logger)|2633
1768|BDR5-185 (A)|25.0|||RSY03|BDR5-185 (A)|0.0|Gas storage well. Open file|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0866|39.60861111|-79.31972222|Garrett|Maryland|Texas Eastern Transmission Corp. #4 Barbara Miller      Barbara Miller Unit|McHenry|1966|lithologic log||||||||Hampshire |at surface|Benson |3188|Tully |6296|Onondaga |7078|Huntersville |7104|Needmore |7235|Oriskany |7277|Helderberg |7412|||||||||||||||||||7415 (7419 by logger)|2376
1769|BDR5-186 (A)|25.0|||RSY03|BDR5-186 (A)|0.0|Gas storage well. Open file|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0867|39.59861111|-79.31555556|Garrett|Maryland|Texas Eastern Transmission Corp. #3 Helen L. Enlow      Earl Knox Unit|McHenry|1966|lithologic log||||||||Pocono |at surface|Benson |3603|Tully |6517|Onondaga |7225|Huntersville |7254|Needmore |7360|Oriskany |7408|Helderberg |7628|||||||||||||||||||7631 (7626 by logger)|2662
1770|BDR5-187 (A)|25.0|||RSY03|BDR5-187 (A)|0.0|Gas storage well. Open file|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0868|39.6225|-79.3075|Garrett|Maryland|Texas Eastern Transmission Corp. #2 J. J. Schlossnagle      Ella Collier Unit|McHenry|1966|lithologic log||||||||Hampshire |at surface|Benson |3452|Tully |6306|1st Onondaga |7115|1st Huntersville |7147|fault |7194|2nd Onondaga |7194|2nd Huntersville |7215|1st Needmore |7327|1st Oriskany |7371|fault |7381|2nd Needmore |7381|2nd Oriskany |7444|Helderberg |7640|||||||7690|2539
1771|BDR5-188 (A)|25.0|||RSY03|BDR5-188 (A)|0.0|Gas storage well. Open file|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0869|39.62166667|-79.36472222|Garrett|Maryland|Texas Eastern Transmission Corp. #2 Mitchell J. Rush      Mitchell Rush Unit|McHenry|1966|lithologic log||||||||Pocono |at surface|Tully |6417|Onondaga |7235|Huntersville |7260|Needmore |7384|Oriskany |7414|Helderberg |7545|||||||||||||||||||||7536 (7549 by logger)|2357
1772|BDR5-189 (A)|25.0|||RSY03|BDR5-189 (A)|0.0|Gas storage well. Open file|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0870|39.58777778|-79.31611111|Garrett|Maryland|Texas Eastern Transmission Corp. #1 William H. Kelso      Earl Knox Unit|McHenry|1969|lithologic log||||||||Pocono |at surface|Tully |6738|Onondaga |7572|1st Huntersville |7606|fault||2nd Huntersville |7652|Needmore |7746|Oriskany |7794|Helderberg |7934|||||||||||||||||7940|2760
1773|BDR5-190 (A)|25.0|||RSY03|BDR5-190 (A)|0.0|Gas storage well. Open file|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0871|39.62194444|-79.29611111|Garrett|Maryland|Texas Eastern Transmission Corp. #3 U. S. A, - Savage River State Forest      Charles Bowser Unit|McHenry|1969|lithologic log||||||||Pocono |at surface|Tully |6957|Onondaga |7756|Huntersville |7784|Needmore |7881|Oriskany |7921|Helderberg |8068|||||||||||||||||||||8070|2838
1774|BDR5-191 (A)|25.0|||RSY03|BDR5-191 (A)|0.0|Gas storage well. Open file|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0872|39.61972222|-79.36|Garrett|Maryland|Texas Eastern Transmission Corp. #3 Mitchell Rush      Mitchell Rush Unit|McHenry|1969|lithologic log||||||||Pocono |at surface|Tully |6256|1st Onondaga |6892|1st Huntersville |6910|fault||2nd Onondaga |6942|2nd Huntersville |6940|Needmore |7113|Oriskany |7178|Helderberg |7308|||||||||||||||7307|2312
1775|BDR5-192|25.0|||RSY02|BDR5-192|0.0|Oil or gas test, dry hole. Amsden (1954) Hennen and Reger (1914) Tucker (1936)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0873|39.43333333|-79.45833333|Garrett|Maryland|Oakland Oil and Gas Co. #1 Harned Heirs|Oakland|Before 1914|lithologic log||||||||Conemaugh |at surface|Allegheny |180|Pottsville |430|Mauch Chunk |745|Greenbrier |1410|Pocono |1680|Catskill and Chemung |2100|||||||||||||||||||||3200|2500
1776|BDR5-193 (B)|25.0|||RSY01|BDR5-193 (B)|0.0|Gas producer. Deepened in 1951. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0874|39.38666667|-79.39083333|Garrett|Maryland|Columbian Carbon Co. #1 Norris K. Welch, et al.      GW-1502|Oakland|1950|lithologic log||||||||Jennings |at surface|Tully |2262|Huntersville |2834|Needmore |2895|Oriskany |2953|||||||||||||||||||||||||2869 deepened to 2977|2415
1777|BDR5-194 (B)|25.0|||RSY07|BDR5-194 (B)|0.0|Gas producer, plugged and abandoned 1955. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0875|39.39277778|-79.37916667|Garrett|Maryland|Snee and Eberly #1 O'Donnell|Oakland|1951|lithologic log||||||||Jennings |at surface|Marcellus |3217|Onondaga |3247|Brown break (fault ?) |3254|Onondaga |3257|Huntersville |3280|Oriskany |3414|Helderberg |3500|||||||||||||||||||3522|2390
1778|BDR5-195 (B)|25.0|||RSY07|BDR5-195 (B)|0.0|; Gas producer, plugged and abandoned 1961. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0876|39.39861111|-79.38277778|Garrett|Maryland|Nollem Oil and Gas Corp. Snee and Eberly #1 Camp Meeting Association Grounds      (#1 Mountain Lake Park Camp Meeting Association)|Oakland|1950|lithologic log||||||||Jennings |at surface|Tully |2877|Brown break |3608|Onondaga |3611|Huntersville |3645|Oriskany(?) |3670|||||||||||||||||||||||3672|2460
1779|BDR5-196 (B)|25.0|||RSY07|BDR5-196 (B)|0.0|Gas producer, plugged and abandoned 1967. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0877|39.38972222|-79.3875|Garrett|Maryland|Columbian Carbon Co. #1 Oren T. Graser, et al.      GW- 1503|Oakland|1951|lithologic log||||||||Jennings |at surface|Huntersville |2969|Needmore |3055|Oriskany |3093|Helderberg-Tonoloway |3200|||||||||||||||||||||||||3601|2385
1780|BDR5-197 (B)|25.0|||RSY07|BDR5-197 (B)|0.0|Gas producer, plugged and abandoned 1956. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0878|39.39277778|-79.38444444|Garrett|Maryland|Snee and Eberly #1 Mountain Lake Park      (#1 Baker)|Oakland|1951|lithologic log||||||||Jennings |at surface|Tully |2450|Marcellus |3019|Brown break |3069|Onondaga |3072|Huntersville |3099|Needmore |3151|Oriskany |3222|Helderberg |3309|||||||||||||||||3905|2410
1781|BDR5-198 (B)|25.0|||RSY07|BDR5-198 (B)|0.0|Gas producer, plugged and abandoned 1954. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0879|39.39722222|-79.37777778|Garrett|Maryland|James I. Shearer      (Petroleum Drilling Corp.) #1 Grimes|Oakland|1951|lithologic log||||||||Jennings |at surface|Brown break |3351|Onondaga |3354|Huntersville |3387|Needmore |3486|Oriskany |3510|Helderberg |3641|||||||||||||||||||||3651|2420
1782|BDR5-199 (C)|25.0|||RSY02|BDR5-199 (C)|0.0|Gas test, dry hole. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0880|39.37305556|-79.42361111|Garrett|Maryland|Nollem Oil and Gas Corp. #1 Ralph Gilbert|Table Rock|1951|lithologic log||||||||Jennings |at surface|Bottomed near Marcellus||||||||||||||||||||||||||||||||4854|2470
1783|BDR5-200 (B)|25.0|||RSY07|BDR5-200 (B)|0.0|Gas producer, plugged and abandoned 1954. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0881|39.39527778|-79.37805556|Garrett|Maryland|Nollem Oil and Gas Corp. #1 A. D. Naylor|Oakland|1951|lithologic log||||||||Jennings |at surface|Tully |2696|Brown break |3264|Onondaga |3267|Huntersville |3300?|Needmore |3400|Oriskany |3423|Helderberg |3527|||||||||||||||||||3543|2395
1784|BDR5-201 (B)|25.0|||RSY01|BDR5-201 (B)|0.0|Gas producer. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0882|39.39666667|-79.38166667|Garrett|Maryland|O. M. Fox Drilling      (Western Maryland Gas Co .) #1 Dawson      (Lelia and George Dawson)|Oakland|1951|lithologic log||||||||Jennings |at surface|Tully (?) |2910|Huntersville |3372|Needmore |3463|Oriskany |3490|||||||||||||||||||||||||3500|2445
1785|BDR5-202 (B)|25.0|||RSY02|BDR5-202 (B)|0.0|Gas test, dry hole. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0883|39.39833333|-79.39361111|Garrett|Maryland|Petroleum Drilling Corp. #1 Earl J. Hirshman|Oakland|1951|lithologic log||||||||Jennings |at surface|No log available.||||||||||||||||||||||||||||||||4323|2445
1786|BDR5-203 (B)|25.0|||RSY07|BDR5-203 (B)|0.0|Gas producer, plugged and abandoned 1959. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0884|39.39444444|-79.385|Garrett|Maryland|Snee and Eberly #1 Artis|Oakland|1951|lithologic log||||||||Jennings |at surface|Tully |2765|Marcellus |3273|Brown break |3328|Onondaga |3331|Huntersville |3366|Needmore |3424|Oriskany |3520|Helder berg |3630|||||||||||||||||3861|2415
1787|BDR5-204|25.0|||RSY02|BDR5-204|0.0|Gas test, dry hole. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0885|39.39527778|-79.40194444|Garrett|Maryland|Union Drilling, Inc., et al. #1 Ray E. Cogley|Oakland|1951|lithologic log||||||||Jennings |at surface|No log available.||||||||||||||||||||||||||||||||5531|2410
1788|BDR5-205 (B)|25.0|||RSY02|BDR5-205 (B)|0.0|Gas test, dry hole. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0886|39.39861111|-79.38638889|Garrett|Maryland|Eagle Gas Co. #1 Mary K. Germaine|Oakland|1951|lithologic log||||||||Jennings |at surface|Tully |3510|Marcellus |4445|Brown break |4511|Onondaga |4512|Huntersville |4556|||||||||||||||||||||||4621|2430
1789|BDR5-206 (B)|25.0|||RSY02|BDR5-206 (B)|0.0|Gas test, dry hole. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0887|39.39527778|-79.38555556|Garrett|Maryland|New York State Natural Gas Corp. #1 Orval Kitzmiller      N-225|Oakland|1951|lithologic log||||||||Jennings |at surface|Tully |2853|Brown break |3897|Onondaga |3898|Huntersville |3938|Needmore |4059|Oriskany |4104|Helderberg |4205|||||||||||||||||||4532|2411
1790|BDR5-207 (B)|25.0|||RSY07|BDR5-207 (B)|0.0|Gas producer, -plugged and abandoned 1955. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0888|39.39361111|-79.38138889|Garrett|Maryland|Delaware Gas Co. #1 Elizabeth S. Holloway, et al.|Oakland|1951|lithologic log||||||||Jennings |at surface|Tully |2575|Brown break |3165|Onondaga |3168|Huntersville |3198|Needmore |3262|||||||||||||||||||||||3268|2400
1791|BDR5-208 (B)|25.0|||RSY01|BDR5-208 (B)|0.0|Gas producer. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0889|39.40138889|-79.37194444|Garrett|Maryland|Shaw and Smith #1 Harvey|Deer Park|1951|lithologic log||||||||Jennings |at surface|Tully |3199|Onondaga |3804|Huntersville |3838|||||||||||||||||||||||||||3896 (3907 ?)|2490
1792|BDR5-209 (B)|25.0|||RSY02|BDR5-209 (B)|0.0|Gas test, dry hole. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0890|39.40277778|-79.37694444|Garrett|Maryland|Snee and Eberly #1 Fee|Oakland|1951|lithologic log||||||||Jennings |at surface|Tully |3108|Marcellus |3626|Brown break |3665|Onondaga |3668|Huntersville |3689|Needmore |3757|Oriskany |3817|Shriver |3910|||||||||||||||||3932|2440
1793|BDR5-210 (B)|25.0|||RSY02|BDR5-210 (B)|0.0|Gas test, dry hole. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0891|39.40166667|-79.37583333|Garrett|Maryland|New York State Natural Gas Corp. #1 C. P. Martin, et al.      N-230|Oakland|1952|lithologic log||||||||Jennings |at surface|Brown break |3502|Onondaga |3503|Huntersville |3532|Needmore |3630|Oriskany |3665|Helderberg |4048|||||||||||||||||||||4089|2435
1794|BDR5-211 (B)|25.0|||RSY07|BDR5-211 (B)|0.0|Gas producer, plugged and abandoned 1954. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0892|39.39277778|-79.37638889|Garrett|Maryland|Johnston Bros. Snee and Eberly #1 William White|Oakland|1951|lithologic log||||||||Jennings |at surface|Tully |3026|Brown break |3587|Onondaga |3590|Huntersville |3627|Needmore |3674|Oriskany |3748|Helder berg |3838|||||||||||||||||||3866|2410
1795|BDR5-212 (B)|25.0|||RSY02|BDR5-212 (B)|0.0|Gas test, dry hole. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0893|39.40305556|-79.39361111|Garrett|Maryland|Mid-Atlantic Oil and Gas Co. #1 Stewart F. Hamill|Oakland|1951|lithologic log||||||||Jennings |at surface|No log available.||||||||||||||||||||||||||||||||4004|2500
1796|BDR5-213 (B)|25.0|||RSY02|BDR5-213 (B)|0.0|Gas test, dry hole. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0894|39.4075|-79.37833333|Garrett|Maryland|New York State Natural Gas Corp. #1 Jay Ward Bolyard      N-229|Oakland|1951|lithologic log||||||||Jennings |at surface|No log available.||||||||||||||||||||||||||||||||5015|2454
1797|BDR5-214 (B)|25.0|||RSY02|BDR5-214 (B)|0.0|Gas test, dry hole. Amsden (19 54)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0895|39.40138889|-79.38388889|Garrett|Maryland|Blaho Oil and Gas Co. #1 Richards (?)|Oakland|1951|lithologic log||||||||Jennings |at surface|No log available.||||||||||||||||||||||||||||||||4552|2490
1798|BDR5-215 (B)|25.0|||RSY07|BDR5-215 (B)|0.0|Gas producer, plugged and abandoned 1961. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0896|39.39666667|-79.38277778|Garrett|Maryland|Snee and Eberly #4 Fee|Oakland|1951|lithologic log||||||||Jennings |at surface|Tully |2668|Marcellus |3278|Brown break |3330|Onondaga |3333|Huntersville |3360|Oriskany |3487|||||||||||||||||||||3600|2440
1799|BDR5-216 (B)|25.0|||RSY02|BDR5-216 (B)|0.0|Gas test, dry hole. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0897|39.4025|-79.39194444|Garrett|Maryland|Eagle Gas Co. #1 Mussard|Oakland|1951|lithologic log||||||||Jennings |at surface|No log available.||||||||||||||||||||||||||||||||118|2475
1800|BDR5-217 (B)|25.0|||RSY02|BDR5-217 (B)|0.0|Gas test, dry hole. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0898|39.39944444|-79.38638889|Garrett|Maryland|Guesman, Mathews, and Harper #1 Calhoun|Oakland|1951|lithologic log||||||||Jennings |at surface|Tully |3540|Bottomed near to Marcellus||||||||||||||||||||||||||||||4390|2425
1801|BDR5-218 (B)|25.0|||RSY07|BDR5-218 (B)|0.0|Gas producer, plugged and abandoned 1958 . Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0899|39.39777778|-79.38194444|Garrett|Maryland|Nollem Oil and Gas Corp. #1 Otis W. Shahan|Oakland|1951|lithologic log||||||||Jennings |at surface|Tully |2788|Brown break |3372|Onondaga |3375|Huntersville |3410|Oriskany |3531|Helderberg |3641|||||||||||||||||||||3664|2435
1802|BDR5-219 (B)|25.0|||RSY02|BDR5-219 (B)|0.0|Gas test, dry hole . Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0900|39.3975|-79.37916667|Garrett|Maryland|Mid-Atlantic Oil and Gas Co. #1 Grimes (?)|Oakland|1952|lithologic log||||||||Jennings |at surface|Tully |2806|Brown break |3352|Onondaga |3355|Huntersville |3386|Oriskany |3515|||||||||||||||||||||||3602?|2435
1803|BDR5-220 (B)|25.0|||RSY07|BDR5-220 (B)|0.0|Gas producer, plugged and abandoned 1952. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0901|39.39277778|-79.38694444|Garrett|Maryland|George Jackson #1 A. M. Calhoun      (#78)|Oakland|1951|lithologic log||||||||Jennings |at surface|Brown break |3211|Onondaga |3214|Huntersville |3263|Needrnore |3388|Oriskany |3436|Helderberg |3568|||||||||||||||||||||3571|2395
1804|BDR5-221 (B)|25.0|||RSY07|BDR5-221 (B)|0.0|Gas producer, abandoned. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0902|39.40277778|-79.37944444|Garrett|Maryland|Blaho Oil and Gas Co. #1 Rumer|Oakland|1951|lithologic log||||||||Jennings |at surface|Tully |3202|Brown break |3771|Onondaga |3774|Huntersville |3810|Oriskany |3940|Helderberg |4051|||||||||||||||||||||4051?|2460
1805|BDR5-222 (B)|25.0|||RSY02|BDR5-222 (B)|0.0|Gas test, dry hole. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0903|39.4125|-79.37583333|Garrett|Maryland|E. T. Lowstuter      (Union Drilling Co.) #1 A. D. Naylor|Oakland|1952|lithologic log||||||||Jennings |at surface|No log available.||||||||||||||||||||||||||||||||4671|2460
1806|BDR5-223 (B)|25.0|||RSY07|BDR5-223 (B)|0.0|Gas producer, plugged and abandoned 1953. No completion report. Data from letter in MGS open file. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0904|39.39388889|-79.37638889|Garrett|Maryland|Loch Lynn Gas Corp.      (Lexa Oil Corp.) #1 White|Oakland|1952|lithologic log||||||||Jennings |at surface|Huntersville |3415|Oriskany |3430|||||||||||||||||||||||||||||3520|2390
1807|BDR5-224 (B)|25.0|||RSY07|BDR5-224 (B)|0.0|Gas producer, plugged and abandoned 1953. Amsden (19 54)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0905|39.38972222|-79.3775|Garrett|Maryland|Columbian Carbon Co. #1 George A. Kight|Oakland|1952|lithologic log||||||||Jennings |at surface|Brown break |3388|Onondaga |3391|Huntersville |3432|Oriskany |3542|||||||||||||||||||||||||3548|2400
1808|BDR5-225 (C)|25.0|||RSY02|BDR5-225 (C)|0.0|Gas test, dry hole. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0906|39.3775|-79.39583333|Garrett|Maryland|Cumberland and Allegheny Gas Co 4H Jasper Riley      A-474|Oakland|1952|lithologic log||||||||Jennings |at surface|Brown break |2834|Onondaga |2837|Huntersville |2863|Oriskany |2990|Helderberg |3051|||||||||||||||||||||||3109|2400
1809|BDR5-226 (B)|25.0|||RSY02|BDR5-226 (B)|0.0|Gas test, dry hole. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0907|39.38944444|-79.38111111|Garrett|Maryland|Mid-Atlantic Oil and Gas Co. #1 Oren T. Graser|Oakland|1952|lithologic log||||||||Jennings |at surface|Tully |2668|Brown break |3234|Onondaga |3236|Huntersville |3270|Oriskany |3387|||||||||||||||||||||||3511|2390
1810|BDR5-227 (C)|25.0|||RSY01|BDR5-227 (C)|0.0|Gas producer. No completion report. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0908|39.37472222|-79.40083333|Garrett|Maryland|Eagle Gas Co., Inc. #1 Arthur E. Lohr|Table Rock|1952|lithologic log||||||||Jennings |at surface|Huntersville |3166|Oriskany |3267|||||||||||||||||||||||||||||3558|2420
1811|BDR5-228 (C)|25.0|||RSY01|BDR5-228 (C)|0.0|Gas producer. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0909|39.38|-79.39416667|Garrett|Maryland|Columbian Carbon Co. #2 N. K. Welch      GW-1509|Oakland|1952|lithologic log||||||||Jennings |at surface|Oriskany |2879|Helderberg |3018|||||||||||||||||||||||||||||3047|2395
1812|BDR5-229 (B)|25.0|||RSY07|BDR5-229 (B)|0.0|Gas producer, plugged and abandoned 1953. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0910|39.3975|-79.37666667|Garrett|Maryland|Lexa Oil Corp.      (Loch Lynn Gas Corp.) #1 Nellie Lee|Oakland|1952|lithologic log||||||||Jennings |at surface|Brown break |3382|Huntersville (?) |3404|||||||||||||||||||||||||||||3445?|2410
1813|BDR5-230 (C)|25.0|||RSY02|BDR5-230 (C)|0.0|Oil or gas test, dry hole. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0911|39.29416667|-79.47138889|Garrett|Maryland|Preston Lumber Co.      #1 (Benjamin F. Knapp)|Table Rock|1930|lithologic log||||||||Jennings |at surface|No log available.||||||||||||||||||||||||||||||||1540|2425
1814|BDR5-231 (C)|25.0|||RSY02|BDR5-231 (C)|0.0|Oil or gas test, dry hole. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0912|39.34111111|-79.45|Garrett|Maryland|Fox and Trimble #1 Kite      (Kight)|Table Rock|?|lithologic log||||||||Jennings |at surface|Huntersville |4700|Oriskany |4828|||||||||||||||||||||||||||||5019|2480
1815|BDR5-232 (C)|25.0|||RSY02|BDR5-232 (C)|0.0|Gas test, dry hole. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0913|39.3|-79.47861111|Garrett|Maryland|Columbian Carbon Co . #1 W. J. Durr, et al.      GW- 1501|Table Rock|1947|lithologic log||||||||Jennings |at surface|Corniferous lime |4558|Huntersville |4582|Oriskany |4747|Helderberg |4897|||||||||||||||||||||||||5259|2460
1816|BDR5-233 (C)|25.0|||RSY07|BDR5-233 (C)|0.0|Gas producer, plugged and abandoned 1956. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0914|39.3325|-79.43666667|Garrett|Maryland|Cumberland and Allegheny Gas Co. #1 E. N. Beachy      A-424|Table Rock|1949|lithologic log||||||||Jennings |at surface|Tully |3915|Onondaga |4367|Huntersville |4403|Needmore |4505|Oriskany |4520|Helderberg |4659|||||||||||||||||||||4910|2475
1817|BDR5-234 (C)|25.0|||RSY07|BDR5-234 (C)|0.0|Gas producer, plugged and abandoned 1967. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0915|39.35944444|-79.40527778|Garrett|Maryland|Columbian Carbon Co . #1 Joni J. Miller      GW- 1504|Table Rock|1951|lithologic log||||||||Jennings |at surface|Tully |3305|Marcellus |3750|Onondaga |3822|Huntersville |3848|Needmore |3908|Oriskany |3943|Lime |4044|Oriskany |4054|Helderberg |4106|||||||||||||||4398|2460
1818|BDR5-235 (C)|25.0|||RSY07|BDR5-235 (C)|0.0|Gas producer, plugged and abandoned 1958. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0916|39.34527778|-79.42416667|Garrett|Maryland|Gnee and Eberly #1 Eli D. Beachey|Table Rock|1951|lithologic log||||||||Jennings |at surface|Tully |3452|Marcellus |3951|Brown break |3963|Onondaga |3966|Huntersville |4007|Needmore |4099|Oriskany |4121|Helderberg |4215|||||||||||||||||4365|2445
1819|BDR5-236 (C)|25.0|||RSY07|BDR5-236 (C)|0.0|Gas producer, plugged and abandoned 1958. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0917|39.33388889|-79.44194444|Garrett|Maryland|Columbian Carbon Co. #1 Artie E. Dodge      GW- 1508|Table Rock|1951|lithologic log||||||||Jennings |at surface|Tully |3600|Brown break |4048|Onondaga |4051|Huntersville |4108|Needmore |4207|Oriskany |4227|Helderberg |4388|||||||||||||||||||4395|2475
1820|BDR5-237 (C)|25.0|||RSY02|BDR5-237 (C)|0.0|Gas test, dry hole, Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0918|39.33777778|-79.42638889|Garrett|Maryland|Columbian Carbon Co. #1 Noah Lichty      GW-1507|Table Rock|1951|lithologic log||||||||Jennings |at surface|Tully |4195|Brown break |4583|Onondaga |4586|Huntersville |4596|||||||||||||||||||||||||4623|2425
1821|BDR5-238 (C)|25.0|||RSY07|BDR5-238 (C)|0.0|Gas producer, plugged and abandoned 1958. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0919|39.35333333|-79.415|Garrett|Maryland|Snee and Eberly #2 Eli D. Beachey|Table Rock|1951|lithologic log||||||||Jennings |at surface|Tully |3515|Marcellus |3965|Brown break |4020|Onondaga |4023|Huntersville |4052|Oriskany |4174|Helderberg |4295|||||||||||||||||||4395|2460
1822|BDR5-239 (C)|25.0|||RSY07|BDR5-239 (C)|0.0|Gas test, dry hole, plugged and abandoned 1953. No completion report and no production record. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0920|39.37166667|-79.39027778|Garrett|Maryland|Roeder and Roeder      (W. H. and J. A. Roeder) #1 Pleasant Valley Church|Table Rock|1951|lithologic log||||||||Jennings |at surface|Oriskany |4020|||||||||||||||||||||||||||||||?|2460
1823|BDR5-240 (C)|25.0|||RSY07|BDR5-240 (C)|0.0|Gas producer, plugged and abandoned 1956. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0921|39.34638889|-79.41916667|Garrett|Maryland|Snee and Eberly #3 Eli D. Beachey|Table Rock|1952|lithologic log||||||||Jennings |at surface|Tully |3495|Brown break |4041|Onondaga |4043|Huntersville |4076|Oriskany |4190|Helderberg |4309|||||||||||||||||||||4362|2430
1824|BDR5-241 (C)|25.0|||RSY01|BDR5-241 (C)|0.0|Gas producer . No completion report. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0922|39.37305556|-79.39944444|Garrett|Maryland|Cumberland and Allegheny Gas Co. #1 Harry E. Rice      A-476|Table Rock|1952|lithologic log||||||||Jennings |at surface|Huntersville |2948?|||||||||||||||||||||||||||||||3182|2440
1825|BDR5-242 (C)|25.0|||RSY07|BDR5-242 (C)|0.0|Gas producer, plugged and abandoned 1962. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0923|39.37388889|-79.39277778|Garrett|Maryland|Cumberland and Allegheny Gas Co. #2 Jasper Riley      2-475|Table Rock|1952|lithologic log||||||||Jennings |at surface|Tully |2635|Brown break |3261|Onondaga |3263|Huntersville |3293|||||||||||||||||||||||||3322|2400
1826|BDR5-243 (C)|25.0|||RSY02|BDR5-243 (C)|0.0|Gas test, dry hole. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0924|39.335|-79.43361111|Garrett|Maryland|Cumberland and Allegheny Gas Co. #1 Noah D. Shrock      A-487|Table Rock|1952|lithologic log||||||||Jennings |at surface|Tully |3955|Brown break |4405|Onondaga |4407|Huntersville |4437|Needmore |4505|Oriskany |4534|Helderberg |4670|||||||||||||||||||4714|2500
1827|BDR5-244 (C)|25.0|||RSY07|BDR5-244 (C)|0.0|Gas producer, plugged and abandoned 1962. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0925|39.36666667|-79.39944444|Garrett|Maryland|Cumberland and Allegheny Gas Co #2 Harry E. Rice      A-485|Table Rock|1952|lithologic log||||||||Jennings |at surface|Tully |3062|Brown break |3602|Onondaga |3606|Huntersville |3633|||||||||||||||||||||||||3698|2420
1828|BDR5-245 (C)|25.0|||RSY01|BDR5-245 (C)|0.0|Gas producer. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0926|39.36666667|-79.40611111|Garrett|Maryland|Cumberland and Allegheny Gas Co #1 Walter N. Beckman      A-486|Table Rock|1951|lithologic log||||||||Jennings |at surface|Tully |2980|Brown break |3086|Onondaga |3090|Huntersville |3128|Needmore |3179|Oriskany |3210|Helder berg |3345|||||||||||||||||||3351|2440
1829|BDR5-246 (C)|25.0|||RSY02|BDR5-246 (C)|0.0|Gas test, dry hole. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0927|39.34277778|-79.43083333|Garrett|Maryland|Snee and Eberly #1 Ross Lichty|Table Rock|1953|lithologic log||||||||Jennings |at surface|Tully |3400|Brown break |3893|Onondaga |3895|Huntersville |3930|Needmore |4017|Oriskany |4050|Helderberg |4145|||||||||||||||||||4177|2430
1830|BDR5-247 (C)|25.0|||RSY07|BDR5-247 (C)|0.0|Gas producer, plugged and abandoned 1963. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0928|39.37111111|-79.39444444|Garrett|Maryland|Columbian Carbon Co. #1 D. Milton Riley, et al.      GW-1510|Table Rock|1952|lithologic log||||||||Jennings |at surface|Tully |3074|Brown break |3600|Onondaga |3603|Huntersville |3620|Oriskany |3735|||||||||||||||||||||||3924|2410
1831|BDR5-248 (C)|25.0|||RSY02|BDR5-248 (C)|0.0|Gas test, dry hole. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0929|39.34833333|-79.42694444|Garrett|Maryland|Cumberland and Allegheny Gas Co #1 Simon D. Swartzentruber      A-492|Table Rock|1953|lithologic log||||||||Jennings |at surface|Tully |3282|Onondaga |3889|Huntersville |3918|Needmore |3999|Oriskany |4037|||||||||||||||||||||||4153|2435
1832|BDR5-249 (C)|25.0|||RSY01|BDR5-249 (C)|0.0|Gas producer. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0930|39.36222222|-79.41194444|Garrett|Maryland|Orville Eberly Nellem Oil and Gas Corp. #1 H. D. Swartzentruber|Table Rock|1953|lithologic log||||||||Jennings |at surface|Brown break |3206|Onondaga |3208|Huntersville |3228|Needmore |3300|Oriskany |3330|||||||||||||||||||||||3399|2460
1833|BDR5-250 (C)|25.0|||RSY02|BDR5-250 (C)|0.0|Gas test, dry hole. Amsden (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0931|39.36416667|-79.40083333|Garrett|Maryland|Orville Eberly Nellem Oil and Gas Corp. #1 Joni Miller|Table Rock|1953|lithologic log||||||||Jennings |at surface|Brown break |3700|Onondaga |3702|Huntersville |3733|Needmore |3820|Oriskany |3847|Helderberg |3952|||||||||||||||||||||4021|2440
1834|BDR5-251 (C)|25.0|||RSY02|BDR5-251 (C)|0.0|Gas test, dry hole. Open file|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0932|39.30361111|-79.45555556|Garrett|Maryland|Cumberland and Allegheny Gas Co #1 James E. Knepp|Table Rock|1954|lithologic log||||||||Jennings |at surface|No log available. ||||||||||||||||||||||||||||||||5901|2490
1835|BDR5-252 (C)|25.0|||RSY07|BDR5-252 (C)|0.0|Gas producer, plugged and abandoned 1958. Open file|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0933|39.31694444|-79.45444444|Garrett|Maryland|Columbian Carbon Co. #1 L.B. Shaffer, et al.      GW-1512|Table Rock|1954|lithologic log||||||||Jennings |at surface|Tully |3572|Brown break |4046|Onondaga |4047|Huntersville |4085|Needmore |4160|Oriskany |4208|||||||||||||||||||||4351|2486
1836|BDR5-253 (C)|25.0|||RSY01|BDR5-253 (C)|0.0|Gas producer. Now owned by Cities Service Oil Co. Open file|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0934|39.28444444|-79.48638889|Garrett|Maryland|Columbian Carbon Co. #1 Ezra B. Hamstead, et al.      GW-1511|Table Rock|1954|lithologic log||||||||Jennings |at surface|Huntersville |4001|Needmore |4090|Oriskany |4123|Helderberg |4203|||||||||||||||||||||||||4280|2506
1837|BDR5-254 (C)|25.0|||RSY01|BDR5-254 (C)|0.0|Gas producer. Now owned by Cities Service Oil Co. Open file|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0935|39.31972222|-79.45833333|Garrett|Maryland|Columbian Carbon Co. #1 Ray C. Arnold, et al.      GW-1513|Table Rock|1954|lithologic log||||||||Jennings |at surface|Huntersville |3533|Needmore |3640|Oriskany |3664|||||||||||||||||||||||||||3805|2465
1838|BDR5-255 (C)|25.0|||RSY07|BDR5-255 (C)|0.0|Gas producer, plugged and abandoned 1955. Open file (last page of completion report is missing)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0936|39.32361111|-79.44861111|Garrett|Maryland|Cumberland and Allegheny Gas Co #1 John G. Mulvey      #505|Table Rock|1954|lithologic log||||||||Jennings |at surface|Tully |3666|||||||||||||||||||||||||||||||4387|2472
1839|BDR5-256 (C)|25.0|||RSY07|BDR5-256 (C)|0.0|Gas producer, plugged and abandoned 1967. Open file|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0937|39.3075|-79.46361111|Garrett|Maryland|Columbian Carbon Co. #1 James F. Hamilton      GW-1514|Table Rock|1955|lithologic log||||||||Jennings |at surface|Brown break |3848|Onondaga |3949|Huntersville |3998|Oriskany |4080|Helderberg |4167|||||||||||||||||||||||4191|2480
1840|BDR5-257 (C)|25.0|||RSY07|BDR5-257 (C)|0.0|Gas producer, plugged and abandoned 1967 by Cities Service Oil Co. Open file|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0938|39.33111111|-79.45|Garrett|Maryland|Columbian Carbon Co. #2 Artie E. Dodge      GW-1515|Table Rock|1955|lithologic log||||||||Jennings |at surface|Onondaga |3650|Huntersville |3698|Needmore |3779|Oriskany |3829|Helderberg |3979|||||||||||||||||||||||3986|2466
1841|BDR5-258 (C)|25.0|||RSY01|BDR5-258 (C)|0.0|Gas producer. Open file|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0939|39.31611111|-79.4625|Garrett|Maryland|Cumberland and Allegheny Gas Co #1 James F. Hamilton      #1-520|Table Rock|1955|lithologic log||||||||Jennings |at surface|Tully |3152|Brown break |3639|Onondaga |3641|Huntersville |3669|Needmore |3740|Oriskany |3758|Helderberg |3802|||||||||||||||||||3820|2507
1842|BDR5-259 (C)|25.0|||RSY02|BDR5-259 (C)|0.0|Gas test, dry hole. Open file|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0940|39.32305556|-79.46972222|Garrett|Maryland|Acme Drilling Co. #1 Lester C. Moon|Table Rock|1955|lithologic log||||||||Jennings |at surface|Tully |4146|||||||||||||||||||||||||||||||4281|2584
1843|BDR5-260 (C)|25.0|||RSY02|BDR5-260 (C)|0.0|Gas test, dry hole. Open file|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0941|39.30222222|-79.46888889|Garrett|Maryland|Columbian Carbon Co. #2 James F. Hamilton      GW-1516|Table Rock|1955|lithologic log||||||||Jennings |at surface|Huntersville |3960|Needmore |4044|Oriskany |4077|Helderberg |4174|||||||||||||||||||||||||4587|2436
1844|BDR5-261 (C)|25.0|||RSY02|BDR5-261 (C)|0.0|Gas test, dry hole. Open file|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0942|39.31944444|-79.47861111|Garrett|Maryland|Johnston Bros. George H. Bortz #1 Elizabeth Martin|Table Rock|1955|lithologic log||||||||Jennings |at surface|Brown break |6141|Onondaga |6142|Huntersville |6170|Needmore |6273|Oriskany |6297|||||||||||||||||||||||6388|2474
1845|BDR5-262 (C)|25.0|||RSY01|BDR5-262 (C)|0.0|Gas producer. Production reported as C&A :/Fl Richard F. and June Marsh. Open file|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0943|39.32305556|-79.45694444|Garrett|Maryland|Cumberland and Allegheny Gas Co #1 E. F. Stahl      #536      (#1 Keith J. Stahl)|Table Rock|1955|lithologic log||||||||Jennings |at surface|Onondaga |3465|Huntersville |3493|||||||||||||||||||||||||||||3566|2467
1846|BDR5-263 (C)|25.0|||RSY02|BDR5-263 (C)|0.0|Gas test, dry hole. Open file|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0944|39.32388889|-79.45222222|Garrett|Maryland|Cumberland and Allegheny Gas Co #2 J. G. Mulvey      #2-541|Table Rock|1955|lithologic log||||||||Jennings |at surface|Tully |3415|Brown break |3933|Huntersville |3943|Needmore |4074|Oriskany |4090|Helderberg |4175|||||||||||||||||||||4220|2480
1847|BDR5-264 (C)|25.0|||RSY02|BDR5-264 (C)|0.0|Gas test, dry hole. Open file|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0945|39.37388889|-79.39861111|Garrett|Maryland|Cumberland and Allegheny Gas Co #1 William Lucas      A-601|Table Rock|1962|lithologic log||||||||Jennings |at surface|Tully |2318|Onondaga |2917|Huntersville |2940|Oriskany |3063|Helderberg |3178|Keyser |3459|Williamsport Sandstone |6301|||||||||||||||||||7197|2450
1848|BDR5-265|25.0|||RSY08|BDR5-265|0.0|Water well, abandoned. Bennett and Meyer (1952)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0946|39.39583333|-76.30833333|Harford|Maryland|U. S. Army Edgewood Arsenal|Edgewood|1941|lithologic log||||||||Pleistocene |at surface|Potomac Group |55?|Basement |400|||||||||||||||||||||||||||||402|5
1849|BDR5-266|25.0|||RSY05|BDR5-266|0.0|Water well. Dingman and Ferguson (1956)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0947|39.59805556|-76.47805556|Harford|Maryland|Curt Fuller|Jarrettsville|1948|lithologic log||||||||Wissahickon Schist, surface to bottom ||||||||||||||||||||||||||||||||||469|640
1850|BDR5-267|25.0|||RSY05|BDR5-267|0.0|Water well. Dingman and Meyer (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0948|39.26027778|-76.82555556|Howard|Maryland|J. Natwick|Ellicott City|1935|lithologic log||||||||Baltimore Gabbro, surface to bottom ||||||||||||||||||||||||||||||||||750|400
1851|BDR5-268|25.0|||RSY08|BDR5-268|0.0|Water well, abandoned. Clark, and others (1918) Overbeck and Slaughter (1958) Richards (1945a)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0949|39.21138889|-76.06555556|Kent|Maryland|Chestertown Water Board|Chestertown|1909|lithologic log||||||||Pleistocene |at surface|Aquia |60|Monmouth |129?|Matawan |200?|Magothy |268|Raritan |344|Patapsco |581?|Patuxent |955 ?|||||||||||||||||||1135|15
1852|BDR5-269|25.0|||RSY05|BDR5-269|0.0|Water well. Dingman and Meyer (1954)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0950|39.2825|-77.21055556|Montgomery|Maryland|Montgomery County Board of Education Damascus High School|Damascus|1949|lithologic log||||||||ljamsville Phyllite, surface to bottom ||||||||||||||||||||||||||||||||||572|780
1853|BDR5-270|25.0|||RSY06|BDR5-270|0.0|Stratigraphic test. Mack {1966)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0951|38.76666667|-77.01861111|Prince Georges|Maryland|Washington Suburban Sanitary Commission Fort Foote Test Well|Alexandria|1956|lithologic log||||||||Pleistocene |at surface|Basement |827|No log available. ||||||||||||||||||||||||||||||828|151
1854|BDR5-271|25.0|||RSY02|BDR5-271|0.0|Oil or gas test, dry hole. Darton (1950) Meyer (1952)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0952|38.85083333|-76.89472222|Prince Georges|Maryland|Potomac Oil and Gas Co.|Anacostia|1920|lithologic log||||||||No log available.||May have penetrated basement ||||||||||||||||||||||||||||||||1120|280
1855|BDR5-272|25.0|||RSY06|BDR5-272|0.0|Stratigraphic test. Hansen (1968) Mack (1966)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0953|38.79555556|-76.99777778|Prince Georges|Maryland|Washington Suburban Sanitary Commission South Lawn Test Well|Anacostia|1960|lithologic log||||||||Pleistocene |at surface|Monmouth-Matawan |30|Patapsco |50|Arundel |460|Patuxent |620?|Basement |870|||||||||||||||||||||||875|179
1856|BDR5-273|25.0|||RSY06|BDR5-273|0.0|Stratigraphic test. Mack (1966)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0954|38.78416667|-76.99805556|Prince Georges|Maryland|Washington Suburban Sanitary Commission Oxon Hill Junior High School Test Well|Anacostia|1960|lithologic log||||||||Pleistocene |at surface|Potomac Group |15 |Basement |843 |||||||||||||||||||||||||||||843|109
1857|BDR5-274|25.0|||RSY06|BDR5-274|0.0|Stratigraphic test. Mack (1966)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0955|38.77944444|-76.99861111|Prince Georges|Maryland|Washington Suburban Sanitary Commission Kerby Hill Test Well|Anacostia|1960|lithologic log||||||||Pleistocene |at surface|Weathered basement |794 |Basement |804 |||||||||||||||||||||||||||||804|71
1858|BDR5-275 (D)|25.0|||RSY04|BDR5-275 (D)|0.0|Stratigraphic test for gas storage. Mack (1966)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0956|38.73277778|-76.87083333|Prince Georges|Maryland|Washington Gas Light Co. #3 Mudd|Brandywine|1955|lithologic log||||||||Pleistocene |at surface|Aquia|?|Monmouth |149 |Magothy |188 |Potomac |234 |Triassic ? |1491 |||||||||||||||||||||||1725|118
1859|BDR5-276 (D)|25.0|||RSY04|BDR5-276 (D)|0.0|Stratigraphic test for gas storage. Mack (1966)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0957|38.72|-76.85388889|Prince Georges|Maryland|Washington Gas Light Co. #2 Robinson|Brandywine|1955|lithologic log||||||||Pleistocene |at surface|Nanjemoy ? ||Aquia |200 |Monmouth |320 |Magothy |395 |Potomac |510 |Triassic |1813 |||||||||||||||||||||1818|230
1860|BDR5-277 (D)|25.0|||RSY04|BDR5-277 (D)|0.0|Stratigraphic test for gas storage. No Triassic encountered. Mack (1966)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0958|38.74472222|-76.87194444|Prince Georges|Maryland|Washington Gas Light Co. #3 Dennison|Brandywine|1955|lithologic log||||||||Pleistocene |at surface|Nanjemoy ?||Aquia |196|Monmouth |320|Magothy |370|Potomac |480|Precambrian |1708|||||||||||||||||||||1743|233
1861|BDR5-278|25.0|||RSY06|BDR5-278|0.0|Stratigraphic test. Mack (1966)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0959|38.96861111|-76.73194444|Prince Georges|Maryland|Levitt and Sons of Maryland, Inc. Bowie - Belair Water Supply Probe Hole #1|Bowie/Davidsonville|1958|lithologic log||||||||Matawan-Monmouth |at surface|Magothy |70|Patapsco |200|Arundel |700|Patuxent |920|Basement |1160|||||||||||||||||||||||1178|114
1862|BDR5-279|25.0|||RSY06|BDR5-279|0.0|Stratigraphic test. Mack (1966)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0960|38.96305556|-76.74777778|Prince Georges|Maryland|Levitt and Sons of Maryland, Inc. Bowie - Belair Water Supply Probe Hole #2|Bowie/Davidsonville|1958|lithologic log||||||||Matawan-Momnouth |at surface|Magothy |80|Patapsco |155?|Arundel |705|Patuxent |900|Basement |1150|||||||||||||||||||||||1165|142
1863|BDR5-280|25.0|||RSY06|BDR5-280|0.0|Stratigraphic test. Mack (1966)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0961|38.97111111|-76.72972222|Prince Georges|Maryland|Levitt and Sons of Maryland, Inc. Bowie - Belair Water Supply Probe Hole #3|Bowie/Davidsonville|1962|lithologic log||||||||Pleistocene |at surface|Matawan-Monmouth |20|Magothy |80|Patapsco |190|Arundel |690|Patuxent |955|Basement |1162|||||||||||||||||||||1172|114
1864|BDR5-281|25.0|||RSY05|BDR5-281|0.0|Water well. Hansen (1968) Mack (1966)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0962|38.97111111|-76.72972222|Prince Georges|Maryland|Area Development Corp.      (Levitt and Sons, Inc.) Bowie - Belair Water Supply Production Well #4|Bowie/Davidsonville|1965|lithologic log||||||||Pleistocene |at surface|Monmouth-Matawan |19|Magothy |60|Patapsco |184|Arundel |687|Patuxent |976|Basement |1162|||||||||||||||||||||1172|114
1865|BDR5-282|25.0|||RSY06|BDR5-282|0.0|Stratigraphic test. Mack (1966)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0963|38.96861111|-76.73666667|Prince Georges|Maryland|Levitt and Sons of Maryland, Inc. Bowie - Belair Water Supply Probe Hole #4|Bowie/Davidsonville|1965|lithologic log||||||||Pleistocene |at surface|Monmouth-Matawan ?||Magothy ?||Patapsco |688|Patuxent |976|Basement |1176|||||||||||||||||||||||1176|130
1866|BDR5-283|25.0|||RSY05|BDR5-283|0.0|Water well. Mack (1966)|Reported|WJUNKIN|2021-08-19 16:38:55|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0964|38.96305556|-76.74777778|Prince Georges|Maryland|Area Development Corp.      (Levitt and Sons, Inc.) Bowie - Belair Water Supply Production Well #PW-5A|Bowie/Davidsonville|1965|lithologic log||||||||See log for well #277||||||||||||||||||||||||||||||||||1127|142
1867|BDR5-284|25.0|||RSY08|BDR5-284|0.0|Water well, covered. Darton (1950) Hansen (1968) Meyer (1952) Otton (1955)|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0965|38.96388889|-76.80944444|Prince Georges|Maryland|Glen Dale Sanatorium|Lanham|1938|lithologic log||||||||Patapsco |at surface|Arundel |474|Patuxent |670|Basement (weathered) |945|||||||||||||||||||||||||||946|145
1868|BDR5-285|25.0|||RSY08|BDR5-285|0.0|Water well, covered. Exact location unknown. Clark, and others (1918) Darton (1950) Meyer (1952) Otton (1955) Richards (1945a)|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0966|38.71|-77.02611111|Prince Georges|Maryland|Fort Washington|Mount Vernon|Before 1914|lithologic log||||||||No record surface to 583 feet||Potomac Group ||||||||||||||||||||||||||||||||1000|150
1869|BDR5-286 (D)|25.0|||RSY04|BDR5-286 (D)|0.0|Stratigraphic test for gas storage. Mack (1966)|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0967|38.69583333|-76.90416667|Prince Georges|Maryland|Washington Gas Light Co . #1 McMains|Piscataway|1956|lithologic log||||||||Pleistocene |at surface|Triassic(?) |1604|No log available.||||||||||||||||||||||||||||||1741|219
1870|BDR5-287 (D)|25.0|||RSY04|BDR5-287 (D)|0.0|Stratigraphic test for gas storage Mack (1966)|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0968|38.66305556|-76.92194444|Prince Georges|Maryland|Washington Gas Light Co. #2 Wedding|Piscataway|1955|lithologic log||||||||Pleistocene |at surface|Log begins at 40 feet in Nanjemoy||Marlboro |140|Aquia |165|Monmouth |290|Magothy |320|Potomac |424|Basement |1625|||||||||||||||||||1729|196
1871|BDR5-288 (D)|25.0|||RSY04|BDR5-288 (D)|0.0|Stratigraphic test for gas storage Mack (1966)|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0969|38.71361111|-76.89527778|Prince Georges|Maryland|Washington Gas Light Co. #2 P. Moore|Piscataway|1955|lithologic log||||||||Pleistocene |at surface|Log begins at 30 feet in Nanjemoy||Marlboro |50|Aquia |80|Monmouth |185|Magothy |241|Potomac |323|Triassic(?) |1490|||||||||||||||||||1523|172
1872|BDR5-289 (D)|25.0|||RSY04|BDR5-289 (D)|0.0|Stratigraphic test for gas storage. Mack (1966)|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0970|38.70138889|-76.90222222|Prince Georges|Maryland|Washington Gas Light Co . #1 Hill|Piscataway|1957|lithologic log||||||||Pleistocene |at surface|Triassic(?) |1560|No log available.||||||||||||||||||||||||||||||1611|219
1873|BDR5-290 (D)|25.0|||RSY04|BDR5-290 (D)|0.0|Stratigraphic test for gas storage. Mack (1966)|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0971|38.71388889|-76.895|Prince Georges|Maryland|Washington Gas Light Co . #3 P. Moore      (P. Moore #E0-1)|Piscataway|1957|lithologic log||||||||Pleistocene |at surface|Bottomed in Patuxent||No log available.||||||||||||||||||||||||||||||1268|173
1874|BDR5-291 (D)|25.0|||RSY04|BDR5-291 (D)|0.0|Stratigraphic test for gas storage. Mack (1966)|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0972|38.72777778|-76.9|Prince Georges|Maryland|Washington Gas Light Co. #2 Buckler      (Buckler #0-1)|Piscataway|1957|lithologic log||||||||Pleistocene |at surface|Bottomed in Potomac||No log available.||||||||||||||||||||||||||||||1547|96
1875|BDR5-292 (D)|25.0|||RSY04|BDR5-292 (D)|0.0|Stratigraphic test for gas storage. Mack (1966)|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0973|38.70833333|-76.93222222|Prince Georges|Maryland|Washington Gas Light Co. #2 Thorne|Piscataway|1955|lithologic log||||||||Pleistocene |at surface|Log begins at 30 feet in Marlboro||Aquia |45|Matawan-Monmouth |164|Magothy |171|Potomac |307|Basement |1438|Pleistocene |at surface|||||||||||||||||||1478|59
1876|BDR5-293 (D)|25.0|||RSY04|BDR5-293 (D)|0.0|Stratigraphic test for gas storage. Open file|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0974|38.695|-76.91888889|Prince Georges|Maryland|Washington Gas Light Co. #6      (Joseph S. Moore)|Piscataway|1968|lithologic log||||||||Bottomed in Potomac||No log available.||||||||||||||||||||||||||||||||1362|212
1877|BDR5-294 (D)|25.0|||RSY04|BDR5-294 (D)|0.0|Stratigraphic test for gas storage. Open file|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0975|38.70444444|-76.91722222|Prince Georges|Maryland|Washington Gas Light Co. #5      (Charles C. Marbury)|Piscataway|1968|lithologic log||||||||Pleistocene |at surface|Weathered granite |1648|Basement (granite) |1669|No log available.||||||||||||||||||||||||||||1687 by driller (1681 by logger)|206
1878|BDR5-295 (D)|25.0|||RSY04|BDR5-295 (D)|0.0|Stratigraphic test for gas storage. Open file|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0976|38.70666667|-76.92333333|Prince Georges|Maryland|Washington Gas Light Co. #15 Fee|Piscataway|1969|lithologic log||||||||Pleistocene |at surface|Weathered granite |1475|Basement (granite) |1493|No log available.||||||||||||||||||||||||||||1498|83
1879|BDR5-296 (D)|25.0|||RSY04|BDR5-296 (D)|0.0|Stratigraphic test for gas storage. Open file|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0977|38.68305556|-76.92722222|Prince Georges|Maryland|Washington Gas Light Co. #14 Fee|Piscataway|1969|lithologic log||||||||Pleistocene |at surface|Weathered granite |1729|Basement (granite) |1759|No log available.||Pleistocene |at surface|||||||||||||||||||||||||1761 by logger (1755 by driller)|225
1880|BDR5-297 (D)|25.0|||RSY04|BDR5-297 (D)|0.0|Stratigraphic test for gas storage. Open file|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0978|38.72333333|-76.89222222|Prince Georges|Maryland|Washington Gas Light Co. #1 Fee|Piscataway|1969|lithologic log||||||||Basement |1682|No log available.||||||||||||||||||||||||||||||||1695|232
1881|BDR5-298|25.0|||RSY06|BDR5-298|0.0|Oil test well, dry hole. Clark, and others (1918) Darton (1950) Meyer (1952) Miller (1911) Otton (1955) Richards (1945a) Shattuck, and others (1907)|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0979|38.80416667|-76.87194444|Prince Georges|Maryland|Maryland Oil and Development Co      (Capt. A. F. Lucas ?) Now on Andrews Air Force Base|Upper Marlboro|1906 (1902)|lithologic log||||||||Pliocene (?) |at surface|Calvert |18|Nanjemoy |108|Aquia |136|Brightseat and Monmouth |223|Brightseat, Monmouth, and Magothy |263|Magothy and Potomac |350|||||||||||||||||||||1511 (1522)|240
1882|BDR5-299|25.0|||RSY02|BDR5-299|0.0|Oil or gas test, dry hole, Darton (1950) Meyer (1952)|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0980|38.81055556|-76.85944444|Prince Georges|Maryland|Name unknown      (Champ Robinson?) Now on Andrews Air Force Base|Upper Marlboro|c. 1910|lithologic log||||||||No log available.||||||||||||||||||||||||||||||||||1728|260
1883|BDR5-300 (D)|25.0|||RSY04|BDR5-300 (D)|0.0|Stratigraphic test for gas storage, Mack (1966)|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0981|38.75361111|-76.83305556|Prince Georges|Maryland|Washington Gas Light Co. #2 Butler|Upper Marlboro|1957|lithologic log||||||||Pleistocene |at surface|Log begins at 30 feet in Nanjemoy||Marlboro |55|Aquia |100|Matawan-Monmouth |245|Magothy |275|Potomac |430|Triassic |1617|Basement |1665|Pleistocene |at surface|||||||||||||||1720|165
1884|BDR5-301 (D)|25.0|||RSY04|BDR5-301 (D)|0.0|Stratigraphic test for gas storage. Mack (1966)|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0982|38.76361111|-76.80277778|Prince Georges|Maryland|Washington Gas Light Co. #2 Roberts|Upper Marlboro|?|lithologic log||||||||Log begins at 25 feet in Nanjemoy||Marlboro ||Aquia ||Matawan-Monmouth ||Magothy ||Potomac ||Triassic(?) ||Basement ||||||||||||||||||||1752|211
1885|BDR5-302 (D)|25.0|||RSY04|BDR5-302 (D)|0.0|Stratigraphic test for gas storage. Open file|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0983|38.75583333|-76.85472222|Prince Georges|Maryland|Washington Gas Light Co. #22 U. S. Navy|Upper Marlboro|1969|lithologic log||||||||Pleistocene |at surface|Granite wash |1662|Basement (granite) |1701|No log available.||||||||||||||||||||||||||||1724|180
1886|BDR5-303|25.0|||RSY05|BDR5-303|0.0|Water well. Hansen (1968)|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0984|38.79555556|-76.80944444|Prince Georges|Maryland|Valley Development Co. Maryvale Subdivision      (Redrilling of well #PG-Ee 52, same location)|Upper Marlboro|1965|lithologic log||||||||Pleistocene |at surface|Nanjemoy |12|Aquia-Brightseat |126|Monmouth-Matawan |249|Magothy |319|Patapsco |334|||||||||||||||||||||||924|175
1887|BDR5-304|25.0|||RSY06|BDR5-304|0.0|Stratigraphic test and observation well. Open file|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0985|39.20083333|-76.045|Queen Annes|Maryland|U.S. Geological Survey Chestertown Test Well|Chestertown|1970|lithologic log||||||||Pleistocene |at surface|Aquia-Brightseat |20|Monmouth-Matawan |225|Magothy |375|Potomac Group |390|Basement |1975|||||||||||||||||||||||2009|22
1888|BDR5-305|25.0|||RSY08|BDR5-305|0.0|Water well, abandoned. Overbeck and Slaughter (1958)|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0986|38.95388889|-76.35|Queen Annes|Maryland|State of Maryland Department of Game and Fish Maryland Marine Police      (Chesapeake Ferry System)|Kent Island|1930|lithologic log||||||||Pleistocene |at surface|Eocene (undiff.) |47|Aquia |135|Monmouth |237|Matawan |345|Magothy |380|Raritan |451|||||||||||||||||||||639|16
1889|BDR5-306|25.0|||RSY05|BDR5-306|0.0|Water well. Overbeck and Slaughter (1958)|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0987|38.93388889|-76.01777778|Queen Annes|Maryland|Phillips Canning Co.|Wye Mills|1940|lithologic log||||||||Pleistocene |at surface|Bottomed in Aquia (?)||No log available.||||||||||||||||||||||||||||||647|71
1890|BDR5-307|25.0|||RSY05|BDR5-307|0.0|Water well. Ferguson (1953) Otton (1955)|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0988|38.18833333|-76.43416667|St. Marys|Maryland|St. Mary's Female Seminary|Saint Marys City|1936|lithologic log||||||||Bottomed in Raritan (?)||No log available.||||||||||||||||||||||||||||||||661|20
1891|BDR5-308|25.0|||RSY06|BDR5-308|0.0|Stratigraphic test. Weigle, and others (1970) Weigle and Webb (1970)|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0989|38.24333333|-76.48833333|St. Marys|Maryland|U. S. Geological Survey Great Mills Test Well|Saint Marys City|1966|lithologic log||||||||Pleistocene |at surface|Chesapeake Group |40|Piney Point - Nanjemoy |310|Aquia- Brightseat |515|Monmouth-Matawan |680|Magothy |780|Potomac Group |860|||||||||||||||||||||1508|108
1892|BDR5-309 (E)|25.0|||RSY08|BDR5-309 (E)|0.0|Water wells, abandoned. Old records not clear as to exact number of wells and their locations. Clark, and others (1918) Darton (1896), (1902), (1905) Hansen (1967) Hansen and Otton (1966) McLean (1950)|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0990|37.98305556|-75.84444444|Somerset|Maryland|City of Crisfield Municipal Well Field      (Contains total of 6 wells, shallowest is 250 feet, 4 wells deeper than 1000 feet, deepest is 1262 feet.)|Crisfield|1892-1900|lithologic log||||||||No log available.||||||||||||||||||||||||||||||||||4 wells over 1000; deepest is 1262|5
1893|BDR5-310 (E)|25.0|||RSY05|BDR5-310 (E)|0.0|Water well. Rasmussen and Slaughter (1955)|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0991|37.98305556|-75.84444444|Somerset|Maryland|City of Crisfield Municipal Well Field|Crisfield|1938|lithologic log||||||||No log available.||||||||||||||||||||||||||||||||||994|5
1894|BDR5-311 (E)|25.0|||RSY05|BDR5-311 (E)|0.0|Water well. Rasmussen and Slaughter (1955)|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0992|37.98305556|-75.84444444|Somerset|Maryland|City of Crisfield Municipal Well Field|Crisfield|1938|lithologic log||||||||No log available.||||||||||||||||||||||||||||||||||995|5
1895|BDR5-312 (E)|25.0|||RSY05|BDR5-312 (E)|0.0|Water well. Rasmussen and Slaughter (1955)|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0993|37.97694444|-75.86194444|Somerset|Maryland|City of Crisfield      (Jersey area)|Crisfield|1928|lithologic log||||||||No log available.||||||||||||||||||||||||||||||||||1076|5
1896|BDR5-313 (E)|25.0|||RSY05|BDR5-313 (E)|0.0|Water well. McLean (1950) Rasmussen and Slaughter (1955)|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0994|37.98194444|-75.85222222|Somerset|Maryland|City of Crisfield      (Hoptown area)|Crisfield|1948|lithologic log||||||||Pleistocene |at surface|Yorktown-Cohansey |28|St. Marys |248|Choptank |320|Calvert |392|Piney Point |760|Paleocene |860|Monmouth-Magothy |1067|Raritan |1079|||||||||||||||||1303|5
1897|BDR5-314 (E)|25.0|||RSY05|BDR5-314 (E)|0.0|Water well. Rasmussen and Slaughter (1955)|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0995|37.97527778|-75.86333333|Somerset|Maryland|George A. Christy      (Nelson R. Colburn)|Crisfield|1910|lithologic log||||||||Holocene |at surface|Pleistocene |10|Yorktown-Cohansey |35|St. Marys |249|Choptank |352|Calvert |387|Eocene |772|Paleocene |910|||||||||||||||||||1011 (1040)|2
1898|BDR5-315 (E)|25.0|||RSY05|BDR5-315 (E)|0.0|Water well. Rasmussen and Slaughter (1955)|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0996|37.97888889|-75.86416667|Somerset|Maryland|The Packers Ice and Cold Storage Co.|Crisfield|1950|lithologic log||||||||Fill |at surface|Pleistocene |13|Yorktown-Cohansey |21|St. Marys |264|Choptank |333|Calvert |400|Eocene and Paleocene |728|||||||||||||||||||||1042|2
1899|BDR5-316 (E)|25.0|||RSY08|BDR5-316 (E)|0.0|Water well, abandoned. Clark, and others (1918) Darton (1896), (1902), (1905) Darton and Fuller (1905) Rasmussen and Slaughter (1955) Woolman (1894)|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0997|37.97888889|-75.86333333|Somerset|Maryland|The Packers Ice and Cold Storage Co.|Crisfield|1895|lithologic log||||||||No log available.||||||||||||||||||||||||||||||||||1018|2
1900|BDR5-317 (E)|25.0|||RSY08|BDR5-317 (E)|0.0|Water well, abandoned. Clark, and others (1918) Darton (1896), (1902), (1905) Rasmussen and Slaughter (1955) Richards (1945a) Woolman (1894)|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0998|37.97888889|-75.86333333|Somerset|Maryland|The Packers Ice and Cold Storage Co.      (Crisfield Ice Co.)|Crisfield|1892|lithologic log||||||||No log available.||||||||||||||||||||||||||||||||||1060|2
1901|BDR5-318 (E)|25.0|||RSY05|BDR5-318 (E)|0.0|Water well. Hansen (1967)|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP0999|37.99027778|-75.84722222|Somerset|Maryland|City of Crisfield|Crisfield|1962|lithologic log||||||||Pleistocene |at surface|Chesapeake Group |40|Piney Point - Nanjemoy |715|Aquia-Brightseat |785|Monmouth-Matawan|?|Magothy |1060|Potomac Group |1095|||||||||||||||||||||1110|5
1902|BDR5-319|25.0|||RSY08|BDR5-319|0.0|Water well, abandoned. Open file|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP1000|37.97583333|-76.04222222|Somerset|Maryland|Somerset County Board of Education|Ewell|?|lithologic log||||||||No log available.||||||||||||||||||||||||||||||||||980|0
1903|BDR5-320|25.0|||RSY05|BDR5-320|0.0|Water well. Rasmussen and Slaughter (1955)|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP1001|37.96833333|-76.02388889|Somerset|Maryland|Mrs. Archie Marsh|Ewell|1948|lithologic log||||||||Holocene, Pleistocene, and Pliocene |at surface|Yorktown-Cohansey |19|St. Marys |103|Choptank |235|Calvert |292|Piney Point |575|Paleocene |630|Magothy |768|Raritan |798|||||||||||||||||915|2
1904|BDR5-321|25.0|||RSY05|BDR5-321|0.0|Water well. Open file|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP1002|37.97333333|-76.00083333|Somerset|Maryland|Mr. Fowler|Ewell|1970|lithologic log||||||||Pleistocene |at surface|Chesapeake Group |35|Piney Point - Nanjemoy |590|Aquia-Brightseat |680?|Monmouth-Matawan|?|Magothy |880?|Potomac Group (?) |935?|||||||||||||||||||||1060 plugged back to 1010|2
1905|BDR5-322|25.0|||RSY05|BDR5-322|0.0|Water well. Open file|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP1003|37.96805556|-76.02361111|Somerset|Maryland|Charlie Marsh|Ewell|1970|lithologic log||||||||Pleistocene |at surface|Chesapeake Group |38|Piney Point-Nanjemoy |570|Aquia|?|Monmouth-Matawan|?|Magothy |870|Possibly bottomed in Potomac Group ||||||||||||||||||||||940|3
1906|BDR5-323|25.0|||RSY08|BDR5-323|0.0|Water well, abandoned. Clark, and others (1918)|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP1004|37.97|-75.89027778|Somerset|Maryland|Elliott P. Dennis and Sons|Great Fox Island|1892|lithologic log||||||||Holocene |at surface|Bottomed in Calvert (?) ||No log available. ||||||||||||||||||||||||||||||1058|3
1907|BDR5-324|25.0|||RSY08|BDR5-324|0.0|Water well, abandoned. Rasmussen and Slaughter (1955)|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP1005|38.10833333|-76.01777778|Somerset|Maryland|Berwick Development Co.|Kedges Straits|1951|lithologic log||||||||Pleistocene- Pliocene |at surface|Yorktown-Cohansey |12|St. Marys |110|Choptank |220|Calvert |300|Piney Point |504|Paleocene |610|Magothy |830|||||||||||||||||||871|3
1908|BDR5-325|25.0|||RSY05|BDR5-325|0.0|Water well. Open file|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP1006|38.03944444|-76.01611111|Somerset|Maryland|U. S. Fish and Wildlife Service|Kedges Straits|1962|lithologic log||||||||No log available.||||||||||||||||||||||||||||||||||860|2
1909|BDR5-326|25.0|||RSY05|BDR5-326|0.0|Water well. Open file|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP1007|38.08388889|-75.86388889|Somerset|Maryland|Rumbley - Frenchtown Water Co.|Marion|1968|lithologic log||||||||Pleistocene |at surface|Chesapeake Group |40 |Piney Point - Nanjemoy |645 |Aquia-Brightseat |755 |Monmouth-Matawan|?|Magothy |1030 |Potomac Group |1080 |||||||||||||||||||||1175|2
1910|BDR5-327|25.0|||RSY05|BDR5-327|0.0|Water well. Open file|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP1008|38.09305556|-75.85611111|Somerset|Maryland|Rumbley - Frenchtown Water Co.|Marion|1968|lithologic log||||||||No log available.||||||||||||||||||||||||||||||||||1102|2
1911|BDR5-328|25.0|||RSY06|BDR5-328|0.0|Stratigraphic test. Open file|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP1009|38.10611111|-75.85111111|Somerset|Maryland|Robert Dykes      (Dykes #1)|Marion|1970|lithologic log||||||||Pleistocene |at surface|Chesapeake Group|?|Piney Point - Nanjemoy |645 |Aquia-Brightseat |755 |Monmouth-Matawan|?|Magothy |1035 |Potomac Group |1080 |||||||||||||||||||||1146|5
1912|BDR5-329|25.0|||RSY06|BDR5-329|0.0|Stratigraphic test. Hansen (1967)|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP1010|38.00916667|-75.84416667|Somerset|Maryland|U. s. Geological Survey Janes Island State Park Test Well|Marion|1966|lithologic log||||||||Pleistocene |at surface|Chesapeake Group |40 |Piney Point - Nanjemoy |725 |Aquia-Brightseat |800 |Monmouth-Matawan |1045 |Magothy |1110 |Potomac Group |1145 |||||||||||||||||||||1514|5
1913|BDR5-330|25.0|||RSY06|BDR5-330|0.0|Stratigraphic test. Rasmussen and Slaughter (1957)|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP1011|38.82222222|-76.29194444|Talbot|Maryland|Pan American Refining Corp.|Claiborne|1953|lithologic log||||||||Pleistocene |at surface|Calvert |44|Piney Point |139|Nanjemoy |188|Aquia |305|Brightseat |536|Monmouth |607|Matawan |700|Magothy |853|Raritan |980|||||||||||||||1520|13
1914|BDR5-331|25.0|||RSY05|BDR5-331|0.0|Water well. Clark, and others (1918) Rasmussen and Slaughter (1957) Richards (1945a)|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP1012|38.77777778|-76.0775|Talbot|Maryland|Easton Utilities Conunission      (Easton Water Works)|Easton|1901|lithologic log||||||||Fill |at surface|Pleistocene |5|Choptank |35|Calvert |99|Piney Point |280|Nanjemoy |307|Aquia |570|Paleocene |682|Monmouth |730|Matawan |960|||||||||||||||1015|15
1915|BDR5-332|25.0|||RSY05|BDR5-332|0.0|Water well. Rasmussen and Slaughter (1957)|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP1013|38.77444444|-76.07833333|Talbot|Maryland|Easton Utilities Commission|Easton|1947|lithologic log||||||||Holocene |at surface|Log begins at 21 feet in Pleistocene||Choptank |41|Calvert |71|Piney Point |283|Nanjemoy |431|Aquia |591|Paleocene |681|Monmouth |761|Matawan |956|Magothy |1102|Raritan |1145|||||||||||1188|35
1916|BDR5-333|25.0|||RSY05|BDR5-333|0.0|Water well. Rasmussen and Slaughter (1957)|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP1014|38.77777778|-76.0775|Talbot|Maryland|Easton Utilities Commission|Easton|1929|lithologic log||||||||Log not available||||||||||||||||||||||||||||||||||1025|15
1917|BDR5-334|25.0|||RSY08|BDR5-334|0.0|Water well, abandoned. Rasmussen and Slaughter (1957)|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP1015|38.87944444|-75.99055556|Talbot|Maryland|Esskay Packing Co.|Ridgely|1947|lithologic log||||||||Pleistocene |at surface|Pliocene (?) |27|Choptank |43|Calvert |77|Piney Point |294|Nanjemoy |403|Paleocene |590|Monmouth |710|Matawan |790|Magothy |908|||||||||||||||990|45
1918|BDR5-335|25.0|||RSY06|BDR5-335|0.0|Stratigraphic test. Hansen (1968) Mack (1970) Mack, and others (1970)|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP1016|38.69666667|-76.06222222|Talbot|Maryland|U. S. Geological Survey Hambleton Test Well|Trappe|1965|lithologic log||||||||Pleistocene |at surface|Chesapeake Group |45|Piney Point - Nanjemoy |345|Aquia-Brightseat |690|Monmouth-Matawan |865|Magothy |1040|Potomac Group |1140|||||||||||||||||||||1523|45
1919|BDR5-336|25.0|||RSY06|BDR5-336|0.0|Stratigraphic test. Hansen (1968) Mack, and others (1970)|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP1017|38.74194444|-76.06638889|Talbot|Maryland|U. S. Geological Survey Easton Test Well|Trappe|1965|lithologic log||||||||Pleistocene |at surface|Chesapeake Group |20 |Piney Point - Nanjemoy |310 |Aquia- Brightseat |620 |Monmouth-Matawan |830 |Magothy |1035 |Potomac Group |1155 |||||||||||||||||||||1492|37
1920|BDR5-337|25.0|||RSY05|BDR5-337|0.0|Water well. Rasmussen and Slaughter (1957)|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP1018|38.66027778|-76.06027778|Talbot|Maryland|Trappe Frozen Foods Co.|Trappe|1946|lithologic log||||||||Pleistocene |at surface|Choptank |30 |Calvert |90 |Piney Point |373 |Nanjemoy |502 |Paleocene |605 |Monmouth |830 |Matawan |911 |Magothy |1030 |Raritan |1169 |||||||||||||||1245|55
1921|BDR5-338|25.0|||RSY08|BDR5-338|0.0|Water well, abandoned, Clark, and others (1918) Slaughter (1962)|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP1019|39.63833333|-77.71583333|Washington|Maryland|Fairchild Corp.      (J. C. Roulette and Sons Knitting Co.)|Hagerstown|1911|lithologic log||||||||Stonehenge Limestone,  surface to bottom||||||||||||||||||||||||||||||||||910|540
1922|BDR5-339|25.0|||RSY08|BDR5-339|0.0|Water well, abandoned Slaughter (1962)|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP1020|39.70222222|-77.75333333|Washington|Maryland|Donald Martin|Mason and Dixon|1957|lithologic log||||||||Rockdale Run Formation,  surface to bottom||||||||||||||||||||||||||||||||||760|590
1923|BDR5-340|25.0|||RSY02|BDR5-340|0.0|Oil and/ or gas test, dry hole. Clark, and others (1918) Rasmussen and Slaughter (1955' Richards (1945a)|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP1021|38.42861111|-75.44888889|Wicomico|Maryland|F. Holloway estate      (St. Martins Oil and Gas Co.)|Pittsville|1917|lithologic log||||||||Holocene |at surface|Log begins at 315 feet in Yorktown-Cohansey||St. Marys |360 |Choptank |450 |Calvert |610 |Eocene |1130 |||||||||||||||||||||||1186|67
1924|BDR5-341|25.0|||RSY04|BDR5-341|0.0|Stratigraphic test for gas storage. Rasmussen and Slaughter (1955)|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP1022|38.36555556|-75.52777778|Wicomico|Maryland|Transcontinental Gas Pipeline Corp. Core Hole #1, Roy E. Adkins|Salisbury|1951|lithologic log||||||||Pleistocene |at surface|Pliocene |60 |Yorktown-Cohansey |102 |St. Marys |307 |Choptank |409 |Calvert |512 |||||||||||||||||||||||1025|42
1925|BDR5-342|25.0|||RSY04|BDR5-342|0.0|Stratigraphic test for gas storage. Rasmus sen and Slaughter (1955)|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP1023|38.35305556|-75.51083333|Wicomico|Maryland|Transcontinental Gas Pipeline Corp. Core Hole #2, Hearn's Farm|Salisbury|1951|lithologic log||||||||Pleistocene |at surface|Pliocene |96 |Yorktown-Cohansey |128 |St. Marys |338 |Choptank |429 |Calvert |522 |||||||||||||||||||||||1024|48
1926|BDR5-343|25.0|||RSY04|BDR5-343|0.0|Stratigraphic test for gas storage. Rasmussen and Slaughter (1955)|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP1024|38.34277778|-75.55027778|Wicomico|Maryland|Transcontinental Gas Pipeline Corp. Core Hole #3, Marshall S. Bornt|Salisbury|1951|lithologic log||||||||Pleistocene |at surface|Pliocene |82|Yorktown-Cohansey |113|St. Marys |297|Choptank |389|Calvert |503|||||||||||||||||||||||1004|38
1927|BDR5-344|25.0|||RSY02|BDR5-344|0.0|Oil and / or gas test, dry hole. Anderson (1948) Rasmussen and Slaughter (1955) Richards (1945a) Richards (1945b)|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP1025|38.34666667|-75.48694444|Wicomico|Maryland|Ohio Oil Co. #1 Larry G. Hanunond|Wango|1945|lithologic log||||||||Pleistocene |at surface|Miocene |130|Eocene |1140|Upper Cretaceous |1360|Lower Cretaceous |4424|Triassic |5563|Basement |5498|||||||||||||||||||||5568|70
1928|BDR5-345|25.0|||RSY06|BDR5-345|0.0|Oil test well, dry hole. Clark, and others (1918) Rasmussen and Slaughter (1955) Richards (1945a)|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP1026|38.39194444|-75.10888889|Worcester|Maryland|Isle of Wight Oil Co.      (Now on property of Shore Lumber Co.)|Assawoman Bay|1914|lithologic log||||||||No log available.||||||||||||||||||||||||||||||||||1706|5
1929|BDR5-346|25.0|||RSY02|BDR5-346|0.0|Oil and/or gas test, dry hole . Anderson (1948) Rasmussen and Slaughter (1955)|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP1027|38.40722222|-75.06166667|Worcester|Maryland|Standard Oil Co. of New Jersey #1 Maryland Esso|Assawoman Bay|1946|lithologic log||||||||Holocene |at surface|Miocene |200|Eocene |1650|Upper Cretaceous |2080|Lower Cretaceous |5400|||||||||||||||||||||||||7710|8
1930|BDR5-347|25.0|||RSY06|BDR5-347|0.0|Stratigraphic test. Open file|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP1028|38.44333333|-75.05555556|Worcester|Maryland|U.S. Geological Survey Maryland Beach Test Well|Assawoman Bay|1969|lithologic log||||||||Pleistocene |at surface|Chesapeake Group |100|(To bottom )||||||||||||||||||||||||||||||1212|5
1931|BDR5-348|25.0|||RSY02|BDR5-348|0.0|Oil and/or gas test, dry hole. Anderson (1948) Rasmussen and Slaughter (1955)|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP1029|38.29861111|-75.29083333|Worcester|Maryland|Socony-Vacuum Oil Co. #1 James D. Bethards|Ninepin Branch|1945|lithologic log||||||||Pleistocene |at surface|Miocene |130|Eocene |1225|Upper Cretaceous |1670|Lower Cretaceous |4876|Triassic |6570|Basement |7130|||||||||||||||||||||7178|30
1932|BDR5-349|25.0|||RSY08|BDR5-349|0.0|Water well, now abandoned but still flowing. Located under water in Pocomoke River. Clark, and others (1918) Rasmussen and Slaughter (1955)|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS04|WP1030|38.07333333|-75.57277778|Worcester|Maryland|City of Pocomoke|Pocomoke City|1907|lithologic log||||||||Holocene |at surface|Bottomed in Upper Cretaceous(?)||||||||||||||||||||||||||||||||1540|-1
1933|BDR11-350|25.0|||RSY03|BDR11-350|0.0|Gas storage well.|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS05|WP1031|39.59388889|-79.30972222|Garrett|Maryland|Texas Eastern Transmission Corp . #1 Markel Maust Walter Harman Unit|McHenry|1972|lithologic log||||||||Tully |6919|Onondaga |7634|Huntersville |7656|Needmore |7744|Oriskany |7808|Helderberg |7932|||||||||||||||||||||||7934|2749
1934|BDR11-351|25.0|||RSY03|BDR11-351|0.0|Gas storage well.|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS05|WP1032|39.62805556|-79.28888889|Garrett|Maryland|Texas Eastern Transmission Corp . #4 U.S.A. - Savage River      State Forest Charles Bowser Unit|Accident|1972|lithologic log||||||||Tully |6809|Onondaga |7672|Huntersville |1693|Needmore |7823|Oriskany |7883|Helderberg |8102|||||||||||||||||||||||8122|2760
1935|BDR11-352|25.0|||RSY03|BDR11-352|0.0|Gas storage well.|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS05|WP1033|39.63666667|-79.29416667|Garrett|Maryland|Texas Eastern Transmission Corp . #1 Freeman Bowser Charles Bowser Unit|Accident|1972|lithologic log||||||||Benson |3676|Tully |6718|Onondaga |7464|Huntersville |7482|Needmore |7594|Oriskany |7636|Helderberg |7778|||||||||||||||||||||7780|2641
1936|BDR11-353|25.0|||RSY03|BDR11-353|0.0|Gas storage well.|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS05|WP1034|39.65833333|-79.33083333|Garrett|Maryland|Texas Eastern Transmission Corp . #1 Arthur Devine Black and Frazee Unit|Accident|1972|lithologic log||||||||Tully |6023|Onondaga |6902|Huntersville |6924|||||||||||||||||||||||||||||7319|2254
1937|BDR11-354|25.0|||RSY02|BDR11-354|0.0|Gas test, dry hole. Anhydrite with dolomite in Wills Creek Fm., 6415- 6720|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS05|WP1035|39.34388889|-79.40555556|Garrett|Maryland|Columbia Gas Transmission Corp . #L- 4887 Hesse|Table Rock|1972|lithologic log||||||||Tully |4900|Onondaga |5340|Huntersville |5360|Need.more |5456|Oriskany |5481|Helderberg |5650|Keyser |5870|Tonoloway |6190|Wills Creek |6415|Williamsport |7050|McKenzie |7070|Keefer |7360|Rose Hill |7370|Clinton-Thorold |7690|Tuscarora |7808|||||7934|2533
1938|BDR11-356|25.0|||RSY04|BDR11-356|0.0|Gas test, dry hole below 7 ,454ft. Plugged back to 7,454 ft and converted to gas storage well . Salt from 8,396 to 8,959 .|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS05|WP1036|39.63305556|-79.35277778|Garrett|Maryland|Texas Eastern Transmission Corp . #2 Bowman- Seibert John Miller Unit|Accident|1973|lithologic log||||||||Tully |6250|Onondaga |7098|Chert |7112|Needmore |7216|Oriskany |7240|Helderberg |7360|Salt |8396|Wills Creek |9483|Williamsport |1245|McKenzie |10296|Clinton |10638|Rose Hill |10703|Castanea |11096|Tuscarora |11157|Juniata |11580|||||11617|2393
1939|BDR11-357|25.0|||RSY03|BDR11-357|0.0|Gas storage well .|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS05|WP1037|39.63277778|-79.29694444|Garrett|Maryland|Texas Eastern Transmission Corp . #5 U.S .A. - Savage River      State Forest Charles Bowser Unit|Accident|1973|lithologic log||||||||Tully |6877|Onondaga |7578|Huntersville |7594|Needmore |7710|Oriskany |7751|Helderberg |7909|||||||||||||||||||||||7911|2890
1940|BDR11-358|25.0|||RSY03|BDR11-358|0.0|Gas storage well . Plugged back to 7,482 ft .|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS05|WP1038|39.62638889|-79.36166667|Garrett|Maryland|Texas Eastern Transmission Corp. #4 Mitchell Rush Mitchell Rush Unit|Accident|1973|lithologic log||||||||Tully |6440|Onondaga |7144?|1st Huntersville|7242|2nd Huntersville |7395|Needmore |7570|Oriskany |7602|||||||||||||||||||||||7718|2473
1941|BDR11-359|25.0|||RSY03|BDR11-359|0.0|Gas storage well .|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS05|WP1039|39.66138889|-79.32916667|Garrett|Maryland|Texas Eastern Transmission Corp . #2 Elizabeth Everly|Accident|1975|lithologic log||||||||Tully Limestone |6066|Onondaga Limestone |6931|HuntersvilleChert |6950|Needmore Shale |7128|Oriskany Sandstone |7178|||||||||||||||||||||||||7282|2273
1942|BDR11-360|25.0|||RSY03|BDR11-360|0.0|Gas storage well.|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS05|WP1040|39.63888889|-79.28583333|Garrett|Maryland|Texas Eastern Transmission Corp #6 U.S .A. Savage River|Accident|1975|lithologic log||||||||Benson Sandstone |3868|Tully Limestone |6785|Onondaga Limestone|7538|HuntersvilleChert |7555|Needmore Shale |7650|Oriskany Sandstone|7684|Helder berg Limestone|7812|||||||||||||||||||||7812|2714
1943|BDR11-361|25.0|||RSY07|BDR11-361|0.0|Gas test, dry hole plugged and abandoned. Gas show while drilling in Benson.|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS05|WP1041|39.69944444|-79.25444444|Garrett|Maryland|Texas Eastern Transmission Corp . #1 Negro Mountain WN- 1412|Accident|1975|lithologic log||||||||1st Riley|3942|2nd Riley (fault?)|4142|Benson |4408|Onondaga |8736|Huntersville |8756|Needmore |8876|Oriskany |8898|||||||||||||||||||||8956|2908
1944|BDR11-362|25.0|||RSY03|BDR11-362|0.0|Gas storage well .|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS05|WP1042|39.65222222|-79.3375|Garrett|Maryland|Texas Eastern Transmission Corp. #4 McCullough|Accident|1976|lithologic log||||||||Tully Limestone |6142|Onondaga Limestone|6947|HuntersvilleChert |6962|Needmore Shale |7085|Oriskany Sandstone|7122|Helderberg Limestone|7242|||||||||||||||||||||||7250|2161
1945|BDR11-363|25.0|||RSY03|BDR11-363|0.0|Gas storage well.|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS05|WP1043|39.58055556|-79.32083333|Garrett|Maryland|Texas Eastern Transmission Corp . #2 Whiteface- Kelso|Accident|1976-77|lithologic log||||||||Benson |3815|Tully Lime |6799|HuntersvilleChert |7576|Needmore Shale |7677|Oriskany Sand |7714|Helderberg Lime |7814|||||||||||||||||||||||7814|2759
1946|BDR11-364|25.0|||RSY03|BDR11-364|0.0|Gas storage well.|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS05|WP1044|39.61333333|-79.295|Garrett|Maryland|Texas Eastern Transmission Corp. #3 Vernon Georg|Accident|1976|lithologic log||||||||Benson Sand |3965|Tully Limestone |6977|Onondaga Limestone|7697|HuntersvilleChert |7721|Needmore Shale |7822|Oriskany Sandstone|7862|Helderberg Limestone|7988|||||||||||||||||||||7988|2763
1947|BDR11-365|25.0|||RSY03|BDR11-365|0.0|Gas storage well.|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS05|WP1045|39.63555556|-79.28333333|Garrett|Maryland|Texas Eastern Transmission Corp . #7 U.S.A . - Savage River      State Forest|Accident|1976|lithologic log||||||||Benson Sandstone |4019|Tully Lime |6979|Onondaga Lime |7811|Huntersville Chert |7829|Needmore Shale |7920|Oriskany Sandstone|7956|Helderberg Lime |8125|||||||||||||||||||||8125|2823
1948|BDR11-366|25.0|||RSY03|BDR11-366|0.0|Gas storage well.|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS05|WP1046|39.66666667|-79.32444444|Garrett|Maryland|Texas Eastern Transmission Corp. #3 E. Everly|Accident|1977|lithologic log||||||||Tully Lime |6312|Onondaga Lime |6978|Chert |6993|Needmore Shale |7098|Oriskany Sand |7122|Helder berg Lime |7209|||||||||||||||||||||||7228|2287
1949|BDR11-367|25.0|||RSY03|BDR11-367|0.0|Gas storage well .|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS05|WP1047|39.62444444|-79.36805556|Garrett|Maryland|Texas Eastern Transmi ssion Corp. #5 M. Rush|Accident|1977|lithologic log||||||||Tully Lime |6758|Onondaga Lime |7511|HuntersvilleChert |7534|Needmore Shale |7649|Oriskany Sand |7680|Helderberg Lime |7770|||||||||||||||||||||||7788|2449
1950|BDR11-368|25.0|||RSY03|BDR11-368|0.0|Proposed gas storage well .|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS05|WP1048|39.66388889|-79.34194444|Garrett|Maryland|Texas Eastern Transmission Corp . //1 Sam Friend|Accident|?|lithologic log||||||||||||||||||||||||||||||||||||||||||--|--
1951|BDR11-369|25.0|||RSY03|BDR11-369|0.0|Gas storage well .|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS05|WP1049|39.61611111|-79.3625|Garrett|Maryland|Texas Eastern Transmission Corp . #6 M. Rush|Accident|1978|lithologic log||||||||Chert |7141|Needmore Sha l e |7276|Oriskany Sand |7322|Helder berg Lime |7455|||||||||||||||||||||||||||7460|2265
1952|BDR11-370|25.0|||RSY03|BDR11-370|0.0|Gas storage well.|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS05|WP1050|39.57722222|-79.32638889|Garrett|Maryland|Texas Eastern Transmission Corp. #1 G. H. Glotfelty|Accident|1978|lithologic log||||||||Benson Sand |3720|Huntersville Chert |7512|Ori skany Sand |7684|Helderberg Lime |7803|||||||||||||||||||||||||||7828|2714
1953|BDR11-371|25.0|||RSY03|BDR11-371|0.0|Gas storage well.|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS05|WP1051|39.64277778|-79.28888889|Garrett|Maryland|Texas Eastern Transmission Corp . #1 Henry Miller|Accident|1979|lithologic log||||||||Tully Limestone |6570|Onondaga Limestone |7296|Chert |7312|Needmore Shale |7413|Oriskany Sand |7441|Helderberg Lime |7570|||||||||||||||||||||||7576|2333
1954|BDR11-372|25.0|||RSY03|BDR11-372|0.0|Gas storage well.|Reported|WJUNKIN|2021-08-19 16:38:56|WJUNKIN|2021-08-31 16:43:21|DAS05|WP1052|39.67277778|-79.31805556|Garrett|Maryland|Texas Eastern Transmission Corp. #1 Roy C. Bender|Accident|1978|lithologic log||||||||Tully Limestone |6532|Onondaga Limestone |7305|Chert |7320|Needmore Shale |7436|Oriskany Sandstone |7466|||||||||||||||||||||||||7555|2330
